
Permit Number: 	BX8289IW				Operator: 		Princes Limited

Facility:	 Soft Drinks Site – Cardiff		Form Number: 	 Air1 / DD/MM/YY
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A2
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	100 mg/m3
	Periodic (average over one hour)
	
	BS EN 14792
	
	

	
	
	
	
	
	
	
	

	A2
	Carbon monoxide
	No limit set
	Periodic (average over one hour)
	
	BS EN 14792
	
	






[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

Permit Number: 	BX8289IW					Operator: 		Princes Limited

Facility:	 Soft Drinks Site – Cardiff			Form Number: 	Sewer1 / DD/MM/YY
Reporting of emissions to sewer for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	S1

	Effluent flow
	No limit set
	
	
	See IP6 and IP7
Reported as daily average over 1 month
	
	

	
	pH
	No limit set
	
	
	BS60682.50, ISO 10523
	
	

	
	Suspended solids
	No limit set
	
	
	BS EN 872, BS6068-2.54
	
	

	
	Chemical oxygen demand
	No limit set
	
	
	BS6068-2.34
	
	

	
	Mercury and its compounds as Hg
	0.1 µg/l
	
	
	Compliance based on mass balance calculation
	
	

	
	Cadmium and its compounds as Cd
	0.1 mg/l
	
	
	Compliance based on mass balance calculation
	
	

	
	Mercury and its compounds as Hg
	1.5 g/year
	
	
	
	
	

	
	Cadmium and its compounds as Cd
	0.5 g/year
	
	
	
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

Permit Number: 	BX8289IW				Operator: 		Princes Limited

Facility: 	Soft Drinks site – Cardiff			Form Number: 	Energy1 / DD/MM/YY

Reporting of Energy Usage for the year 20XX

	
Energy Source
	Energy Usage
	
Specific Usage
(MWh/unit output)
	

	
	
Quantity
	Primary Energy
(MWh)
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	Electricity *
	MWh
	
	
	

	Natural Gas
	MWh
	
	
	

	Gas Oil
	tonnes
	
	
	

	Recovered Fuel Oil
	tonnes
	
	
	

	
	
	
	
	

	TOTAL
	-
	
	
	

	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments :









Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)



Permit Number: 	BX8289IW			Operator: 		Princes Limited

Facility	Soft Drinks Site – Cardiff		Form Number: 	Performance1 / DD/MM/YY

Reporting of other performance indicators for the period DD/MM/YYYY to DD/MM/YYYY

	Parameter
	
	Units 
	

	
	
	
	

	Total fruit juice production 
	tonnes
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)
.


Permit Number: 	BX8289IW		Operator: 		Princes Limited

Facility: Soft Drinks Site – Cardif		Form Number: 	WaterUsage1 / DD/MM/YY

Reporting of Water Usage for the year 20XX

	Water Source
	Usage
(m3/year
	Specific Usage 
(m3/unit output)
	

	
	
	
	

	
	
	
	

	Mains water
	
	
	

	Site borehole
	
	
	

	River abstraction
	
	
	

	
	
	
	

	
	
	
	

	TOTAL WATER USAGE
	
	
	



	Operator’s comments :







Signed …………………………………………………………….  		Date………………………..   	
	(authorised to sign as representative of Operator)

