Schedule 6 - Notification 

Part A 
	Permit Number
	GP3030BE

	Name of Operator
	Tata Steel UK Limited

	Location of Installation
	Shotton Works Landfill 

	
	

	Time and date of the detection 
	13/07/2016


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and Time of the event
	N/A

	Reference or description of the location of the event 
	N/A

	Description of where any release into the environment took place
	N/A

	Substances(s) potentially released
	N/A

	Best estimate of the quantity or rate of release of substances
	N/A

	Measures taken, or intended to be taken, to stop any emission
	N/A

	Description of the failure or accident.
	N/A


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	BH10 3-Point moving average 

BH10 (Q1 2016)

	Parameter(s)
	3-Point moving average limit for Zinc

	Limit
	Zinc limit of 0.04ppm @ BH10

	Measured value and uncertainty
	Q3 BH10 3-Point moving average
0.06ppm

	Date and time of monitoring
	13/05/16

	Measures taken, or intended to be taken, to stop the emission
	As noted previously, BH10 may be showing some of the traits of the land reclamation material used in construction/reclamation. It should also be noted that the actual measured value on May was 0.04ppm (i.e. at but not breaching the limit – however as the permit states a 3 point moving average, the average value constituted a breach).


	Time periods for notification following detection of a breach of a limit 

	Parameter CO2
	Notification period 24 h

	c) Notification requirements for the detection of any significant adverse environmental effect 

To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	N/A

	Substances(s) detected
	N/A

	Concentrations of substances detected
	N/A

	Date of monitoring/sampling
	N/A


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	No further information 

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	Continue to monitor all boreholes; check monthly returns when received to determine whether this reoccurs so that local environmental factors or changes can be monitored and evaluated. 
Also, NRW are considering a proposal from the Q4 2015 Part B to adjust the sampling limits.

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	None – due to the age of the landfill and the material used for land reclamation, ascertaining the source of the breach of limits would be virtually impossible.

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	Zinc limit for BH10 (3 month average) was breached in Q1, Q2, Q3 & Q4 2015, and Q1 2016. 
CO2 limits in boreholes were breached in Q1, Q2, Q3 & Q4 2015, and Q1 2016. 


	Name*
	Peter Shephard

	Post
	Senior Energy & Environment Officer

	Signature
	

	Date
	13/07/2016


* authorised to sign on behalf of Tata Steel UK Limited

