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SAFETY & ENVIRONMENTAL PROCEDURE

	Department:     Engineering 

Area:

Operating procedure – ABP Waste Handling Procedure

	HAZARDS IDENTIFIED

1. Manoeuvring of vehicle and use of FLT to move skips or dolavs.

2. Contact with substance causing injury / Illness

3. Spillage will cause a slip hazard.

4. Hazardous to the environment.
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	Purpose

To provide general operating instructions, details of handling ABP Waste and required actions.

Scope

ABP Waste , which is clarified as the following :-
Waste Category 

Type of Waste 

CAT 2 

Chicken DOA or Line Rejects 

CAT 3 

Chicken Offal 

CAT 3

Feathers 

Overview
The Site creates the above waste during the Poultry operation and under our Permit requirements , we have an overarching requirement to prevent any odourous emissions from the site.
Feathers are sent by via a screen & conveyor to the Offal House 
Chicken Offal is sent by conveyor to the Offal House 
Chicken DOA is collected in closed tipper skips. 
Vehicle Collections 
All vehicles must be inspected prior to filling to ensure they are empty and clean certificate are available  ,which must be recorded on sheet PROC027 – Waste and Animal  By Product Movement Record . 

The drivers of the Chicken Offal & Feathers must supervise the loading , which is controlled an Effluent Operator or Maintenance Team. The vehicles must park in the Offal House and ensure that leakage from the vehicle is captured in the rear catch trays. 
The Chicken DOA is tipped into the vehicle via an Effluent Operator or a Despatch / Intake FLT driver.
All vehicles leaving site must be covered.
Document PROC027  Waste and Animal  By Product Movement Record is to be used to record details of . Completed forms are to be kept in the appropriate file in the Site Security Office.

Any spillage must be cleaned up immediately.

If any significant odours are produced when charging the vehicles the operation must STOP.  If the source cannot be identified, contact the Primary Supervisor or Engineering Manager before continuing.

The waste documents, i.e. “Duty Of Care Controlled Waste Transfer Note” must be completed by the operator and tanker driver.

Note: Strict personal hygiene standards must be adhered to at all times including hand washing and regular changes of PPE.



	Operators Instructions

In accordance with PPE clothing requirements, you must wear the following:

General work handling equipment in the area requires the use of overalls, disposable gloves, hard hat, safety boots and reflective jacket. When carrying out general cleaning or other activities that will generate spray or aerosol, an FFP3 mask is also to be used. 
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Environmental Operations
The output of this process can have a significant impact on the wider environment. All care must be taken when carrying out these procedures because of those impacts. If there is any failure of any part of the systems these are to be reported at the earliest opportunity to the HSE Manager or Engineering Manager.

If any significant Odours/Spillages are generated at the time of vehicle charging then the procedure must STOP until the Primary Supervisors or Engineering Manager have been informed and a decision has been made for the next course of action to be taken. 
Any failure of equipment involved in this process must be reported as soon as possible to the Engineering Manager.


	I have read and fully understand the requirements of the above Safety & Environmental Procedure CY-ENV2015 -11. These have also been explained to me verbally.
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