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Part A 
	Permit Number
	PP3834CB

	Name of Operator
	Morgan Technical Ceramics Limited

	Location of Installation
	Vauxhall Industrial Estate, Ruabon, Wrexham, LL14 6HY 

	Location of the emission
	Permit specified location S1.

	Time and date of the emission
	29th October 2015 time 12:36 to 14:36



	a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution.

	To be notified within 24 hrs of detection.

	Date and time of the event.
	29th October 2015 between 12:36 & 14:36

	Reference or description of the location of the event.
	Monitoring the Spray dryer to check monitoring stability and possible results.

	Substance(s) potentially released.
	Lead

	Best estimate of the quantity or rate of release of substances.
	0.56 mg/m3 or 1.8 g/hr over two hours. Or 3.6 g in total

	Measures taken, or intended to be taken, to stop any emission.
	Discussions ongoing with Natural Resources Wales

	Description of the failure or accident.
	This is how the dryer operates.



	b) Notification requirements for a breach of a limit.

	To be notified within 24 hrs of detection unless otherwise specified below.

	Emission point reference/source.
	Permit specified location B6.

	Parameter(s).
	Lead in air.

	Limit.
	0.2 mg/m3

	Measured value and uncertainty.
	0.56 +/- 0.14 mg/m3

	Date and time of monitoring.
	29th October 2015 between 12:36 & 14:36

	Measures taken, or intended to be taken, to stop the emission.
	To be determined and discussed with NRW.

	Time periods for notification following detection of a breach of a limit.

	Parameter.
	Notification period.

	Lead in air.
	Without delay.

	
	

	
	






	c) Notification requirements for the detection of any significant adverse environmental effect.

	To be modified within 24 hours of detection.

	Description of where the effect on the environment was detected.
	During monitoring to determine a stable product to monitor.

	Substance(s) detected.
	Lead

	Concentrations of substances detected.
	0.56 +/- 0.14 mg/m3

	Date of monitoring/sampling.
	29th October 2015 between 12:36 & 14:36




	Name*
	R M Newton

	Post
	EHSQ Manager

	Signature
	


	Date
	24/11/2015


* authorised to sign on behalf of Morgan Technical Ceramics Limited
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