Permit Reference Number: EPR/NP3335GR/V008



Operator: Solutia UK Ltd.
Installation: Cefn mawr ( former ‘Flexsys’ Ruabon Works) 


Form Number : W1

Reporting of Emissions to Water (other than to Sewer) for the period from ………01/07/2015…………………….to……30/09/2015………………………

	Emissions to Water

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3] [6]
	Accreditation/ Certification [4]
	Uncertainty

[5]

	W1-final discharge
	Maximun flow rate l/s
	92.5 l/s
	
61.47l/s
	On-line Electrochemical flow meter
	03/09/15
	
	Manufacturers stated accuracy is given as +/- 0.5%

	
	Maximum discharge volume M3/day
	8000m3
	897m3
	On-line Electrochemical flow meter
	03/09/15
	
	Manufacturers stated accuracy is given as +/- 0.5%

	
	Total  Tetrachloroethene ug/l
	2.5ug/l
	<3ug/l
	GCMS –TM60/PM0
	06/07/15
	
	20%

	
	Total Organic Carbon mg/l
	No Limit
	3mg/l
	TM60/PM0
	06/07/15
	
	10%

	
	Total iron mg/l
	5.0mg/l objective
	0.037mg/l
	TM30/PM14
	06/07/15
	
	5%

	
	Total Phenol mg/l
	0.2 mg/l
	<0.1mg/l
	TM26/PM0
	06/07/15
	
	15%

	
	
	
	
	
	
	
	

	
	Maximum  weekly iron result  mg/l
	5mg/l objective
	0.07mg/l
	Hach Lange DR3900
	07/09/15
	
	

	
	Iron sample comparison
	5mg/l objective
	In House 0.05mg/l
Off site 0.037mg/l
	
	06/07/2015
	
	

	
	Micro Pollutants:-
	
	
	
	
	
	

	
	Toluene ug/l
	No Limits
	<0.5 ug/l
	GCMS-TM15/PM10
	06/07/15
	
	+/- 20%

	
	TCE ug/l
	No Limits
	<3 ugL
	GCMS –TM15/PM10
	06/07/15
	
	+/- 20%

	
	p-Xylene ug/l
	No Limits
	<1 ugL
	GCMS- TM15/PM10
	06/07/15
	
	+/- 20%

	
	Ethylmorpholine ug/l
	No Limits
	<0.1 ugL
	GCMS-TM15/PM10
	06/07/15
	
	+/- 20%

	
	Aniline ug/l
	No Limits
	<0.1 ugL
	GCMS-TM26/PM10
	06/07/15
	
	+/- 20%

	
	Phenol ug/l
	No Limits
	<0.1 ugL
	GCMS-TM26/PM10
	06/07/15
	
	+/- 15%

	
	Ethoxybenzene ug/l
	No Limits
	<0.1 ugL
	GCMS-TM15/PM10
	06/07/15
	
	+/- 20%

	
	o-cresol  ug/l
	No Limits
	<0.01 ugL
	GCMS-TM26/PM0
	06/07/15
	
	+/- 15%

	
	p-cresol
	No Limits
	<0.02 ug/l
	GCMS-TM26/PM0
	06/07/15
	
	+/- 15%

	
	2,4-DCP ug/l
	No Limits
	<0.5 ugL
	GCMS-TM16/PM30
	06/07/15
	
	+/- 20%

	
	Phenyliso ug/l
	No Limits
	<0.1 ugL
	GCMS-TM16/PM30
	06/07/15
	
	+/- 20%

	
	BTH ug/l
	No Limits
	0.5 ugL
	GCMS-TM16/PM30
	06/07/15
	
	+/- 20%

	
	TCP ug/l
	No Limits
	<1 ugL
	GCMSTM16/PM30
	06/07/15
	
	+/- 20%

	
	TMQ ug/l 
	No Limits
	0.9 ug/l
	GCMS-TM16/PM30
	06/07/15
	
	+/- 20%

	
	Phthalimide ug/l
	No Limits
	<0.1 ugL
	GCMS-TM16/PM30
	06/07/15
	
	+/- 20%

	
	MMCD ug/l
	No Limits
	<0.1 ugL
	GCMS-TM16/PM30
	06/07/15
	
	+/- 20%

	
	Acetone (DMK)
	No Limits
	<50 ugL
	GCMS-TM83/PM10
	06/07/15
	
	+/- 20%


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) 

[6] This form is required to be submitted on a quarterly basis. For parameters which are required to be monitored on a twice-yearly basis, and which were monitored during the previous quarter, an entry of ‘nil’ shall be recorded against this parameter. 

Signed ……I.M.Biggs……………………………………………………….  

Date………01/10/2015………………..




(authorised to sign as representative of the Operator)

Date of form: 30/09/2015 

Date of form: 30/09/2015 

