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LICENCE TO IMPOUND WATER
The Natural Resources Body for Wales (hereafter referred to as “NRW”) grants this licence to:-
Corwen Electricity Co-Operative Limited (“the Licence Holder”)
The Owain Glyndwr Hotel
The Square
Corwen
Denbighshire
LL21 0DL

Company Registration Number: IP032341
Fiancial Conduct Authority Number: 32341R

This licence authorises the Licence Holder to obstruct or impede the flow of the inland water described in the Schedule of Conditions (to extent and manner authorised by those conditions) to this licence and subject to the provisions of that Schedule. 
The licence commences from the effective date shown below and shall remain in force until revoked, subject to Condition 4.6.
	Signed:

Ashley Lansdown

Permitting Team Leader
Permitting Service 
Natural Resources Wales

Cambria House

29 Newport Road

Cardiff 

CF24 0TP

	Date of issue…………...13 December 2018


	
	Date effective…………..13 December 2018

	
	


This licence should be kept safe and its existence disclosed on any sale of the land and the impounding works to which it relates.

SCHEDULE OF CONDITIONS 
	1.
1.1
	
	NAME OF INLAND WATER TO BE IMPOUNDED 

Inland water (stream) known as Nant Llechog at Bonwm, near Corwen, Denbighshire.


	2.
2.1
	
	Point of Impoundment
At National Grid Reference SJ 09885 42370 marked ‘Point A’ on the map.



	3.
3.1
	
	MANNER AND EXTENT OF IMPOUNDMENT

Intake works consisting of a concrete weir, Coanda screen with 2 millimetre spacing, forebay tank, compensation notch, eel passage, 315 millimetre external diameter gravity feed pipe controlled by a spear valve and plunge pool in accordance with the specifications and drawing:
‘Bonwm Hydro Intake’ dated 03/12/2018 and,
‘Bonwm Flow-Split Notch’ dated 10/12/2018

copies of which is appended to this licence, or such minor amendments to those documents that are accepted in writing by NRW prior to the date of commencement of construction.


	4.
4.1
	
	FURTHER CONDITIONS

For the purpose of this licence, references to ‘intake works’ shall mean all works consisting of a concrete weir, Coanda screen with 2 millimetre spacing, forebay tank, compensation notch, eel passage, 315 millimetre external diameter gravity feed pipe controlled by a spear valve and plunge pool. 


	4.2
	
	The Licence Holder shall ensure that during construction works, any subsequent maintenance works to the intake works, and when abstraction for the purpose of power production is not taking place, the flow in the Nant Llechog is allowed to pass downstream unchanged in quantity and quality at all times.



	4.3
	
	Prior to commencement of the works authorised by this licence, the Licence Holder shall give 28 calendar days notice in writing to NRW of their intention to commence the authorised works.


	4.4
	
	The Licence Holder shall confirm to NRW in writing that the intake works have been constructed in accordance with the submitted specifications and drawing referred to in Condition 3.1 of this licence 28 calendar days before the scheme is commissioned or becomes operational.



	4.5
	
	The Licence Holder shall construct, operate and maintain the intake works in accordance with the specifications and drawing referred to in Condition 3.1 of this licence and keep them free from leakage and obstruction at all times.



	4.6
	
	This licence shall cease to be of any effect if the intake works authorised by it have not commenced within 3 years of the licence issue date.




	4.7
	
	The intake works authorised by this licence shall not be carried out in the watercourse between 17 October and 15 May in any year.



	4.8
	
	Prior to the completion of the works authorised by this licence, the Licence Holder shall construct a plunge pool, with a minimum depth of 300 millimetres, across the width of the watercourse immediately downstream of the intake works specified in condition 3.1 to ensure the safe downstream passage of fish.


	4.9
	(i)
(ii)

(iii)
	This licence shall only take effect so as to authorise the abstraction provided that the Licence Holder has constructed an eel passage structure, approved in writing by NRW, under the Eels (England and Wales) Regulations 2009, to allow the passage of elver, yellow and silver eel at National Grid Reference SJ 09885 42370.

The Licence Holder shall maintain, repair or replace the eel passage structure to ensure that it remains effective at all times.
The Licence Holder shall keep records of maintenance, repair or replacement of the eel passage structure for 6 years and shall make them available during all reasonable hours for inspection by NRW.




ADDITIONAL INFORMATION
Note: the following information is provided for information only.  It does not form part of the licence.
REASONS FOR CONDITIONS
Conditions 4.1, 4.3, 4.4 and 4.5: to ensure the intake works are constructed, operated and maintained in accordance with the drawing and specifications agreed by NRW during the determination of this licence.
Conditions 4.2 and 4.5: to ensure a flow is maintained in the watercourse in order i) to maintain the riverine habitat for the conservation of the flora and fauna of the watercourse, and ii) to ensure that the water environment is not impacted during construction and subsequent maintenance.
Condition 4.3: to start NRW’s compliance process.

Condition 4.6: to secure the proper use of water resources and to avoid commitment of water resources to an abstraction right that cannot be exercised.

Condition 4.7: to avoid damage to fish during vulnerable life stages such as spawning, migration, emergence and early maturation.
Condition 4.8: to avoid damage to downstream migrating fish.

Condition 4.9: to ensure compliance with the Eels (England and Wales) Regulations 2009 and allow safe passage of eels and elver within the watercourse.
IMPORTANT NOTES
This impoundment licence facilitates the abstraction of water for a hydropower scheme 

authorised under licence serial number WA/067/0005/0027.
For the purposes of Conditions 3.1, 4.3 and 4.4, the Licence Holder shall contact:
Senior Environmental Planning Officer
North and Mid  Area Environmental Planning Team
Natural Resources Wales 

Maes y Ffynnon
Penrhosgarnedd
Bangor
Gwynedd
LL57 2DW
Tel: 0300 065 3000 

Email: nrp.northmid@cyfoethnaturiolcymru.gov.uk
Eel passage 

NRW may have regard to its Best Practice Guide, the Eel Manual: Elver and Eel  Passes (or equivalent guidance) in agreeing where, how and what type of eel pass should be installed and together with the results of any monitoring in determining whether the eel pass is properly effective and maintained, and in judging whether it is necessary to require repair or replacement of the eel pass.
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Would you like to find out more about us, or about your environment?





Then call us on


 0300 065 3000 (Mon-Fri 9-5)





email


� HYPERLINK "mailto:enquiries@naturalresourceswales.gov.uk" �enquiries@naturalresourceswales.gov.uk�





or visit our website


� HYPERLINK "http://www.naturalresourceswales.gov.uk" �www.naturalresourceswales.gov.uk�








incident hotline 0300 065 3000 (24hrs)


floodline 0345 988 1188

















�








Note: References to "the map" are to the map which forms part of this licence.
References to “NRW” are to the Natural Resources Body for Wales or any successor body.
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Environment Act 1995

Water Resources Act 1991 as amended by the Water Act 2003

Water Resources (Abstraction and Impounding) Regulations 2006
Article 3 of the Natural Resources Body for Wales (Establishment) Order 2012

The Natural Resources Body for Wales (Functions) Order 2013

