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 Email: permitreceiptcentre@naturalresourceswales.gov.uk

APPLICATION FOR A MARINE LICENCE FOR MARINE WORKS

Marine Works include, but are not limited to, coast defences, beneficial uses of dredged materials, subsea cables, pontoons, jetties, land reclamation, grab samples and outfall pipes under the Marine and Coastal Access Act 2009

Please read the notes carefully before completing the form.
The Marine Licensing Team (MLT) administers Part 4 of the Marine and Coastal Access Act 2009 on behalf of the Licensing Authority, the Welsh Ministers.

The completed application form must be accompanied by a location plan and, where appropriate, descriptive drawing(s) and any supporting environmental assessments. One completed hard copy of the application and supporting documents will always be required. Additional copies are required for consultation purposes. 

· For application and supporting documents less than 10MB we can accept an additional copy via email.  
· For applications larger than 10MB 16 additional copies in CD/DVD format will be required 
· When applications and supporting documents are hard copy only 16 copies will be required.

Please submit applications to the Permit Receipt Centre via the details at the top of this form
 
Please submit marine licence applications, including this form and all supporting documents, at least 4 months before the licence is required.

Some projects may raise matters that require a significantly longer time for consideration. These are most likely to be:

· Projects that fall within The Marine Works (Environmental Impact Assessment) Regulations 2007 – as amended requiring an Environmental Statement
· Large scale projects with substantial volumes of material being deposited or excavated
· Works requiring an Appropriate Assessment to be conducted under The Conservation of Habitats and Species Regulations 2017.

Information should be provided about the anticipated duration of the entire project in respect of works below/seaward of Mean High Water Spring (MHWS). Where appropriate, planned phasing of the work for which consent is sought must be detailed. For projects lasting more than one calendar year, planned phasing details must be given for each 12 month period.

A licence fee is payable in respect of an application. Details of fees can be found on our web pages.

Please note applications will not be processed without the correct relevant fee or invoicing details.  

Payments can be made via Cheque, BACS or credit/debit card. 
· Cheques should be crossed and made payable to Natural Resources Wales. 
· For BACS payments ensure you provide the reference number (not remittance number)
· For credit/debit card payments please complete the CC1 form and submit with the application. The CC1 form can be found on our web pages

Further information on payment methods can be found on our web pages

All activities need to comply with the Water Framework Directive (WFD). The framework and guidance can be found on the Natural Resources Wales website, http://naturalresources.wales. The results of your WFD assessment must be attached to your marine licence application.

Please answer all questions. If any information is not available at the time of application please indicate in the relevant section, giving reasoning in a covering letter. Outstanding details must be submitted as soon as possible. Any delay in forwarding details is likely to result in delays in determining your application.

Your application may not be considered complete and therefore not processed until key information has been submitted. Your application may be returned if you fail to submit outstanding information within given timescales.
 
Please note any licence may have conditions that must be discharged before works can commence. This will take additional time. 
If you have any queries with regards to completing this application please contact the MLT: marinelicensing@naturalresourceswales.gov.uk

How your application will be processed by the MLT: 

Submit all application to the Permit Receipt Centre via the details at the top of this form.

Checked and acknowledged by the MLT within 21 days of receipt of application and payment 

If the application is complete and no further information is needed at this time, your application will be placed in a work queue to be assigned a permitting officer

If the application is not complete, further information will be request and need to be provided before the application can be considered as complete

Our 4 months service level for determining non-EIA applications will begin from the date the completed application is received (Please note some projects may take significantly longer than 4 months to determine due to their nature)

EIA projects may take significantly longer due to their scale and complexity. Therefore we encourage early engagement with the MLT

Your application and supporting documents will be sent to for an initial consultation period of 28 days (42 days for EIA projects)

For the majority of projects, a public notice must be advertised. Public consultation will be 28 days (49 days for EIA projects).
For EIA projects a second public notice will be required. The MLT will advise on how this should be done.

Responses to consultation will be considered and additional information requested at this time, if necessary.

A decision on your Marine Licence Application will be made

All information submitted may be referred to within a licence, therefore all works must be in accordance with this information, unless otherwise agreed with NRW acting on behalf of the Licensing Authority during the determination process.

It is the responsibility of the applicant to obtain any other consents/authorisations that may be required.

Application Form Structure 
1. Project Description and Cost
2. Applicant Details
3. Details of Agent, Contractor, Vehicles and/or Vessels used to carry out works 
4. Environmental Impact Assessment (EIA)
5. Licensable Period
6. Project Description
7. Methods Statement
8. Materials of Project 
9. Beach Replenishment, Land Reclamation or Salt Marsh Feeding
10. Temporary Works
11. Dredge and Disposal of Dredge Material
12. Protected Sites
13. Other Consents
14. Statutory Powers
15. Public Register
16. Application Fee
17. Declaration

Check List
Please ensure that you have included all the necessary information before you submit you application. If any of the below are not completed in the application form, the application is likely to be considered incomplete and may be returned to you

	Item
	Yes (√)

	The applicant is a legal entity?
	√

	The declaration is signed by the applicant?
	√

	Is the application fee correct?
	√

	Are the grid references/coordinates correct?
	√

	Do the coordinates match map locations?
	√

	Have all the relevant supporting documents been submitted?
	√

	Has a clear methodology been provided in the application form?
	√

	Has Protected sites information been included?
	√

	Has a Water Framework Directive (WFD) assessment been submitted?
	√

	Are all the continuation sheets for application questions appended with correct corresponding numbers?
	√


	
Should you have any queries regarding you application please contact the MLT via marinelicensing@naturalresourceswales.gov.uk  

1. Project Description and Cost

1 (a).	Project Name

Hirael Flood Protection Detailed Design






















1(b).	Please provide a brief description of the proposed project, including locationThe scheme is located along the shore at Hirael in Bangor, Gwynedd. The total length of the scheme is approximately 600 metres.The scheme is split into 4 sections, 
1: Flood defence improvements, re-alignment and improvements to the cycle path and reconstruction of slipway at the Beach Road East section;
2: Main promenade frontage sea wall improvements; including rock armour. 
3: 50m (approx.) section of new embankment and multi user path behind Dŵr Cymru Welsh Water pumping station; 
4: Glandŵr Road flood protection improvements.
Section 2 is seaward of MHWS, the other sections are noted in the application for context.



1(c).	Please provide an estimated gross cost of the project (Inc. materials and labour) for works that fall below/seaward of Mean High Water Springs (MHWS)
£965,238.80




2. Applicant Details
To whom the licence will be issued. This must be a legal entity such as an individual, registered company/ charity or public body. 
Mr
Emyr Gareth

Title				Full Name

Company or Trading
NameCyngor Gwynedd



Company Registration
Number (if applicable)
Emyr Gareth

Name of Contact or 
individual (if different)
Principal Engineer

Position in Company

Swyddfa Penrallt, 
Ffordd Pafiliwn, 
Caernarfon, 
Gwynedd, 
LL55 1BN

Address inc. postcode
(provide registered
Company address if
applicable)


Telephone Number01286 679 419


emyrgareth@gwynedd.llyw.cymru

Email Address
3. Details of Agent, Contractor, Vehicles and/or Vessels used to carry out works 

3(a).	Agent Details 
This is who we will correspond with unless otherwise informed. If no agent we will contact the applicant.
Elen Mai Williamson
Miss

Title				Full Name

Company or Trading
NameYGC



Company Registration
Number (if applicable)


Name of Contact or 
individual (if different)

Position in CompanyTechnical Assistant


Swyddfa Penrallt,
Ffordd Pafiliwn,
Caernarfon,
Gwynedd,
LL55 1BN


Address 
(Inc. postcode)




01286 679363

Telephone Number
elenmaiwilliamson@gwynedd.llyw.cymru


Email Address

3(b).	Does the Applicant wish to be included in all correspondence? Yes ☒	No ☐

3(c).	Contractor Details
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Contractor Company or Trading Name
	Address

	


	





3(d).	Will the works require the use of vessels?				Yes ☐	No ☒

3(d) (i).Vessel Details (if applicable and available)
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Operator
	Name of Vessel
	Type of Vessel
	Vessel Registration Number
	Country of Registration

	

	
	
	
	




3(e).	Will the works require the use of vehicle?				Yes ☒	No ☐

3(e) (i). Vehicle Details (if applicable and available) to be used below MHWS
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Operator 
	Type/Description of Vehicle

	Various

	Construction Plant – to be confirmed following appointment of contractor but likely to be 5-9T excavator to prepare ground for sheet-piling. Subsequent piling work to be carried out from landward side by means of a piling-rig.

	
Various
	Rock armour will be placed by transporting onto the beach using wheeled dumpers and placing with tracked excavator fitted with rock grab.

	

	

	

	




3(f).	If the contractor or vessels or vehicles are not known at the application stage, when do you expect to provide these details?
These details will need to be confirmed prior to the licence and operations commencement


March 2023








4. Environmental Impact Assessment (EIA)
Certain projects, due to their scale, location and/or nature, may require an EIA under the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended). If a project qualifies under EIA, an Environmental Statement (ES) must be prepared and submitted with the application.

Projects that fall within Annex I of the Directive automatically require an EIA. Projects that fall within Annex II of the Directive are assessed on a case-by-case basis for the requirement for an EIA to be undertaken.

4(a).	Do you consider the works to be under the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended)?				Yes ☒	No ☐									
4(a) (i) If Yes, which Annex does the proposal fall under?	     Annex I☐	   Annex II☒

4(a) (ii) Which number(s) within the Annex does the proposal relate to?
Annex II (10)(k) - Coastal work to combat erosion and maritime works capable of 
altering the coast through the construction, for example, of dykes, moles, 
jetties and other sea defence works, excluding the maintenance and 
reconstruction of such works





4(b).	Have you applied for a screening or scoping opinion from the MLT under the Marine Works (Environmental Impact Assessment) Regulations 2007 (as amended)?  									Yes ☐	No ☒


4(b) (i). If Yes, please provide the reference number

4(c).	Has an Environmental Impact Assessment been undertaken? 	Yes ☐ No ☒											
4(c)(i).If Yes, has an Environmental Statement been submitted to support this Marine Licence application? 						Yes ☐ No ☒	

4(d).	If an Environmental Impact Assessment has been undertaken, but an ES has not been submitted, please provide an explanation
Environmental assesments have been undertaken for the project and are enclosed. These have also been used to inform the screening opinion request, submitted to the local planning authority as part of the planning application. We don’t believe that the works will require a full EIA, as demonstrated in the enclosed EIA screening report, but environmental impacts have been assessed as part of the project appraisal process.







Please continue on a separate sheet if necessary. Please tick if you have done this ☐

5. Licensable Period
Determination of applications will be based on the works taking place during these dates. Please ensure you have included an adequate contingency period. If works are not completed by the Requested Licence Expiry Date you may be required to submit a new application. Including a contingency period within your original application does not impact on Licence Fee
March 2024
March 2023

Start Date				Requested Licence Expiry Date


Please ensure you submit your application for a Marine Licence at least 4 months prior to the intended start date. Some projects, such as EIA projects, will take significantly longer to determine.
6. Project Description

6(a).	Please give a description of the proposed project.
This should include the purpose of the project, estimated timescales of construction and operation, and broken down by the phases of works, if applicable.
Details should include, but not be limited to, dimensions of project, quantity of material being deposited and removed.Only section 2 of the proposal requires work at/below MHW. The works will involve provided an increased protection level at severe flood events.
[bookmark: _Hlk87862177]Section 1 – section at Beach Road East carpark
Installation of new concrete wall between the existing field and cycle path. Cycle path to be graded and aligned at a constant gradient down from the A5 to the Beach Road East carpark. Reconstruction of slipway to provide access to the foreshore with a flood gate installed at the top of said slipway. The slipway entrance marks the starting point of Section 2. 
Section 2 – sea wall at promenade frontage
Construct a retaining wall to replace existing gabions at the promenade, from Beach Road East carpark to Welsh Water pumping station. The new defence will be constructed through a sheet pilling method on the same footprint as the existing wall. The space between the new sheet piled wall and the existing gabions will be backfilled (100-200mm). A conrete pile-cap and handrail will be installed on the new wall to provide edge protection. Rock armour (adjacent to new sheet pile wall) shown to extend approximately 4m out into the bay, with a minimum height of 2m above beach level, and laid at a 1:2 slope in front of sheet pile wall (wet side) down to beach level: 605m³ of HMA300-1000 in total. Rock armour to be sloped towards sloped apron in front of the pumping station and to tie into the base of sloped apron. Rock armour to end between sheet pile zone 4 and 3 in the southern part of this section (as shown in 60664880-ACM-CC-CC-DR-C-1203 Promenade GA sheet 3 out of 5) and the base of the rock armour extents to be rounded as shown. To ensure stability of the rock, a key-stone will be embedded on the toe. Any surplus excavated material will be deposited immediately landwards of the toe, to then be buried by the armour stone (see details of embedded toe and excavated earth in 60664880-ACM-XX-XX-DR-C-1224 Promenade Sheet Pile Wall Cross Sections Sheet  4 OF 5). 
Section 3 – embankment behind Welsh Water pumping station
A compacted 1m wide crest topsoil and clay embankment is proposed for construction between the DCWW compound and Beach Road West carpark. A raised cycle path is proposed to be installed directly behind the embankment. The construction of a reinforced concrete wall, clad both sides is also proposed to tie into the raised ground at Watkin Jones’ property (which is directly adjacent to Welsh Water pumping station). At the access to the pumping station, a 9m wide floodgate will be placed to provide both flood defence and vehicular access to the compound (flood gate will be placed between embankment and reinforced concrete wall). 
Section 4 – Glandŵr Road 
An approximate 20m section of road at Glandwr Road is scheduled to be raised slightly (highest point of increase is 0.5m). The construction of a new reinforced concrete wall is scheduled for two sections at this location. The first at the foreshore in front of Gwymon property and the second along the carpark, tying into the raised ground owned by Watkin Jones (previously known as Dickies boatyard). A 6m flood gate will also be placed on Glandŵr Road which will provide both flood protection and access to the properties.



Please continue on a separate sheet if necessary. Please tick if you have done this ☐

6(b).	Please detail the location of the proposed construction project.
This should be either Ordnance Survey National Grid Reference (i.e. AB 12345 67890) or Latitude and Longitude in decimal degrees to 4 decimal places (i.e. Lat 52.1234 Long -4.1234), defining the extent of the project. Please specify which coordinate system has been used.
See supporting document reference: 7720_Hirael_Red Line Map_V3

GRID REF: 
Section 1 - Start: 258826N, 372615E | End: 258796N, 372655E
Section 2 – Start: 258796N, 372655E | End: 258644N, 372885E
Section 3 – Start: 258643N, 372874E | End: 258588N, 372892E
Wall in section 3 tie into slate waste: Start 258599N, 372906E | End: 258626N, 372923E
Section 4: Start: 258534N, 372988E | End: 258526N, 373006E. 

Detailed outline of temporary work area and rock armour given in supporting spreadsheet: 7720_Temporary work area & rock armour coordinates (lat-long)




Please continue on a separate sheet if necessary. Please tick if you have done this ☐
6(c).	The following must be provided with the completed application form:

(i) a suitably scaled extract of an Ordnance Survey Map or Admiralty Chart with location of project, complete with North Arrow and Scale

(ii) construction plans and sectional drawings showing those proposed works below/seaward of MHWS, which should give details of the materials to be used (for beach replenishment the quantity, particle size and source of material to be deposited and deposit location is also required).

(iii) a descriptive schematic drawing and suitably scaled location plan which show the full extent of the project clearly in relation to the surrounding area and features.

Please list below all supporting documents that have been submitted with this application, including suitable documents/maps/drawing titles and reference numbersThe supporting documents relevant to the Marine License i.e below/seaward of MHWS are marked with an asterisk.
7720_Hirael_Red Line Map_V3 *
7720_Temporary work area & rock armour coordinates (lat-long) *
7720_EIA Screening Opinion Hirael_v0.2 *
1901227720_Hirael_Habitats Regulations Assessment_v0.03dh *
7720_Hirael_ECIA_v0.06 *
7720_WFD_Hirael_v0.03 *
[bookmark: _GoBack]20221121-Hirael FAS_Methodology Statement *
Hirael WNMP signposting doc.
7720_AB2004 Hirael FAS DBA-LowRes
Detailed Design Drawings: 60664880-ACM-XX-XX-DR-C-1201 up to 60664880-ACM-XX-XX-DR-C-1225 (Drawings of the Promenade are relevant to the Marine License as they show features seaward of MHWS, the others are included for context)










Please continue on a separate sheet if necessary. Please tick if you have done this ☐

The applicant should note that these drawings/plans may be copied to others as part of the MLT's consultation procedures. If they are subject to copyright, it is the responsibility of the applicant to obtain the necessary approvals to reproduce the documents and to submit up to 16 copies with the application.

7. Methods Statement

7(a).	Please provide a detailed method statement for the works
This must include methods for all works including temporary structures or deposits such as jetties, cofferdams, moorings or landing stages to be constructed seaward of MHWS

A construction methodology statement has been included in support of this application and can be found in supporting document reference: 20221111-Hirael FAS_Methodology Statement







































Please continue on a separate sheet if necessary. Please tick if you have done this ☐

7(b). Do you intend to undertake activities that could generate underwater noise?
This include piling, use of explosives, geophysical, acoustic deterrent devices and multibean echosounders. 								Yes ☒ No ☐

7(b) (i). If Yes, what type(s) of activities will be undertaken?
Discussions are taking place around which method will be used for pilling of the sheet piles. At present stage the preferred pilling option involves the use a Leader Rig. However, exact pilling technique and timescales will not be determined until a contractor is appointed to carry out the works. As the location of the piling is generally above MHW, the work won’t require piling into the water, with work to pause if the water reaches the piling location.











7(b) (ii). If Yes, approximately how many days will the activity be undertaken for?  
Not currently known as this will depend on the piling methodology selected by the appointed contractor.









If Yes, you will be required to complete an additional form that will be provided.

7(c).	Please state the measures to be taken to:
(i) Minimise risk to the marine environment 
· Implement best practice to ensure good housekeeping, for example ensuring all machinery used is kept in good repair and subject to regular checks; 
·  Ensure all fuel and other potentially hazardous chemicals is stored in a safe compound at a distance of at least 10m from the shoreline; 
· Use biodegradable lubricant and hydraulic oil in plant machinery is possible. Biodegradable oils are less toxic than most synthetic oil but should still be stored to the same standards as other oils and prevented from entering the water environment. 






· Production of a Construction Environmental Management Plan (CEMP) with pollution prevention measures noted within the plan. 
· Consider the seasonal timings of the works as disturbance is likely to have a negative impact on important high tide roosts during the winter months. 
· Activities that will generate high-level disturbance stimuli, notably purcusive sheet piling (but less so ‘silent pilling’ solutions), should be undertaken April-August when the impact on roosting waders will be minimal. 
·  Introduce disturbance buffers. Therefore, no heavy construction works to be undertaken during the autumn and winter months (from September through to the end of March) within 150m of Roost 1 or 2 and for a period extending 1.5 hours either side of high water (3 hours in total). Roost locations shown on map in HRA.
· Adopt sensitive working methods such as operating plant and machinery slowly and plant operators only entering and exiting their vehicles at designated sites away from the roost locations. 
· All plant working within the tidal area (beach) to have bio-degradable oils. 
· Fuel bowsers, oils, and lubricants to be stored at site compound in lockable and secure storage as far away from the Harbour as practicably possible.    
· Concrete wash out facilities to be located within the site compound in the form of a lined waste skip. 
· Noise / vibration monitoring will be undertaken for a minimum of 2 weeks prior to the commencement of works in order to establish a working baseline. Monitoring will then continue throughout the works. 




(ii) Prevent undue interference to others 

The contractor will have considered this within the method statement and general phasing / programming of the works.












(iii) Maintain navigational safety, including marking and lighting of works
N/A











Please continue on a separate sheet if necessary. Please tick if you have done this ☐

8. Materials of Project 

8(a).	Description of materials to be deposited seaward of MHWS (Please tick all that apply)
Timber	☐	Iron/Steel	☒	Concrete	☒	Biocides/other chemicals	☐
Silt		☐	Stone/Rock	☒	Gravel		☐	Plastic/Synthetics		☐ 
Sand	☐	Other		☐	

If other, please provide a description of materials.











8(b).	Delivery method of materials to site
If sea delivery, please include details of vessels to be used with a chart of proposed route and transhipment area. If vehicle delivery, please provide the proposed access route. 

Road Delivery – via A5.










Please continue on a separate sheet if necessary. Please tick if you have done this ☐

8(c).	Will the works involve removals seaward of MHWS?		Yes ☒ No ☐

8(c) (i). Description of materials to be removed seaward of MHWS (Please tick all that apply)
Timber	☐	Iron/Steel	☒	Concrete	☐	Biocides/other chemicals	☐
Silt		☐	Stone/Rock	☐	Gravel		☐	Plastic/Synthetics		☐ 
Sand	☐	Other		☒	
8(c) (ii). Description of objects/materials to be removed seaward of MHWS
Including quantities to be removed.
Degraded gabion baskets will be removed from the foreshore (to a licensed tip) prior to commencement of the piling work. This work will also move large rocks which would otherwise hamper the pile installation, however any such material will be retained on the foreshore. In terms of temporary work, material will also be excavated from the foreshore/seaward of MHWS to form a trench in order to construct the embedded toe of the rock armour. Any surplus excavated material will be deposited immediately landwards of the toe, to then be buried by the armour stone (as shown in 60664880-ACM-XX-XX-DR-C-1224 Promenade Sheet Pile Wall Cross Sections Sheet  4 OF 5).









9. Beach Replenishment, Land Reclamation or Salt Marsh Feeding
For works involving any of the above, please provide the following information 

9(a). Is the material to be deposited like for like to existing material? 	Yes ☐ No ☒

9(a)(i) If No for Beach Replenishment please provide justification why?N/A











9(b).	Description of material to be deposited
Please provide the grading specification of materials to be used, if using a range of grain sizes please state the percentage by weight passing. If unsure, please refer to the Wentworth Scale 
N/A












Please continue on a separate sheet if necessary. Please tick if you have done this ☐

9(c).	Source of the material to be deposited
Including dredged or land based stating the origin of material

N/A











9(d).	Has the material been chemically analysed? 			Yes ☐ No ☒
If material has been analysed, we may request this information to determine the application

9(d) (i) If Yes, is the analysis data been included with the application? Yes ☐ No ☒


10. Temporary Works

10(a).	Will there be any temporary deposits below MHWS? 		Yes ☐ No ☒
This includes construction materials, removed objects/material, jetties or cofferdams
If Yes, please continue with section 10

10(b).	Please provide the location of temporary deposits 
Please include a map/chart displaying the location of temporary deposits, if necessary.














10(c).	Description of temporary deposits
















Please continue on a separate sheet if necessary. Please tick if you have done this ☐


11. Dredge and Disposal of Dredge Material
If you are undertaking Dredge and Disposal activities please also complete the Dredge and Disposal application form and submit together.

11(a).	Do you intend to apply for a marine licence to dispose of dredged material to sea as part of the works in this application? 			Yes ☐ No ☒

12. Protected Sites

Licensing Authorities have a duty to ensure that projects will not have significant adverse environmental impact, particularly on any designated European Site of Conservation Importance - Special Areas of Conservation (SAC) and Special Protection Areas (SPA), listed under the Habitats Directive (Council Directive 92/42/EEC on the conservation of natural habitats and of wild fauna and flora). In addition, it is Government Policy that Wetlands of International Importance (Ramsar sites) are also considered as European Sites.  There is a duty to take reasonable steps to further the conservation and enhancement of nationally designated sites (Sites of Special Scientific Interest (SSSIs).

12(a).	Have you had pre-application correspondence with NRW, its legacy bodies or Natural England? 								Yes ☐ No ☒


12(a)(i). If Yes, please provide copies of correspondence with application and state which team(s) you have contacted? 

N/A








12(b).	Are any part of the works located within or likely to affect a designated conservation site? (SAC, SPA, SSSI or Ramsar)			 Yes ☒ No ☐

12(b)(i). If Yes, which designated site(s) may be affected?


Statement to inform the HRA is attached.











12(c).	Please provide a description of all mitigation measures proposed to avoid any impact on designated conservation sites.





Statement to inform the HRA is attached.












Please continue on a separate sheet if necessary. Please tick if you have done this ☐

12(d).	If the works are not located within or likely to affect a designated conservation site, please indicated the approximate distance to the nearest designated conservation site.

Statement to inform the HRA is attached.











Please note that if the proposed works are in or within 2km of a European Site of Conservation Importance you will have to provide suitable mitigation measure to avoid any impact on designated conservation sites.

















13. Other Consents

Please detail all consents that you have applied for or received for these works

	Type of Consent
	Applied for
	To be applied for
	Reference Number
	Date of Issue and Expiry

	Planning Permission under Town and County Planning Act 1990 – From Local Planning Authority (LPA)

	07/12/2021
	
	C21/1174/11/LL
	

	Name and Address of LPA for location of works

	
Cyngor Gwynedd Council



	Land Owners Consent such as The Crown Estate Consent

	Yes
	
	
	

	Port Authority or Local Harbour permissions

	
	
	
	

	Other NRW consents such as Flood Defence or SSSI assent
	
	
	
	

	Details of NRW consent

	

	Other consents such as Transport and Works Act Order, Section 36 Electricity Act, grant/loan sanction
	
	
	
	

	Details of other consents 


	



14. Statutory Powers

14(a).Does the applicant have statutory powers to consent any aspect of the project? 
E.g. coast protection authority, dredging powers, statutory undertakers	Yes ☒ No ☐

14(a)(i).If Yes, please give details and state the relevant legislation that gives these powers


Cyngor Gwynedd / Coast Protection Authority













15. Public Register

Under The Marine Licensing (Register of Licensing Information)(Wales) Regulations 2011 and the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended) , all information contained within or provided in support of this application will be placed on the Public Register unless NRW approve of the applicant’s reasons for withholding all or part.	

15.	Is there any information contained within or provided in support of this application that you consider should NOT be included on the Public Register on the grounds that its disclosure:

15(a).	Would be contrary to the interest of National Security? 		Yes ☐ No ☒

15(b).	Would prejudice to an unreasonable degree you, or some other person’s commercial interest of those of a third party? 			Yes ☐ No ☒

If Yes to either (a) or (b), please provide full justification as to why all or part of the information you have provided should be withheld
























Please continue on a separate sheet if necessary. Please tick if you have done this ☐

16. Application Fee

16(a). What are the corresponding fee band for this application? Band 2 ☒ Band 3 ☐

16(b) Band 2 Only
Projects are charged at a fixed fee of £1920. The application will not be processed until the correct fee has been provided.

Please provide the method of payment 

	Method
	Yes (√)
	Reference Number

	Cheque
	
	

	BACS (not remittance no.)
	√


	To be confirmed and sent on via email.

	World Pay (phone or CC1)
	

	


Please attach CC1 Form with application. Can be found on our web pages

16(c) Band 3 Application only
Band 3 applications are charged at on hourly rate of £120 and are invoiced in arrears. Please complete the details below which will be required for invoicing.


Customer Name




FAO



Purchase order number



Address for invoice





Telephone Number





Email Address




17. Declaration

I declare that to the best of my knowledge and belief that the information given in this application form and supporting documentation is true.

	WARNING: It is an offence under the Marine and Coastal Access Act 2009, under which this application is made, to fail to disclose information or to provide false or misleading information and can invalidate any licence granted.




[image: ]

Signature								Date	18/11/2022



Name (in capitals)	Emyr Gareth

Position in Company	Principal Engineer							
	


Applications cannot be processed unless signed by the Applicant (not agent), the applicant must have appropriate level of authority within the company.

Applications will not be processed unless signed
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