Permit Number: 	PP3238LX		Operator: 		Bakelite Synthetics UK Limited

Facility:		Barry Thermosets Plant		Form Number: 	 Air1 / 13/02/2023
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1:B1
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	180 mg/m3 when firing on natural gas
	Periodic
	
	
	
	

	
	
	220 mg/m3 when firing on oil
	Periodic
	
	
	
	

	
	Carbon monoxide
	140 mg/m3
	Periodic
	
	
	
	

	A1:B2
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	180 mg/m3 when firing on natural gas
	Periodic
	
	
	
	

	
	
	220 mg/m3 when firing on oil
	Periodic
	
	
	
	

	
	Carbon monoxide
	140 mg/m3
	Periodic
	
	
	
	

	A2
	Phenol
	10 mg/m3
	Periodic
	
	
	
	

	
	Formaldehyde
	2 mg/m3
	Periodic
	
	
	
	

	
	Styrene [5]
	No limit set
	Periodic
	
	
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
[5] Monitoring of styrene required when styrene is in use at the installation


Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


