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1.0 Purpose
The purpose of this procedure is to ensure that: -

· only permitted wastes are accepted into the household waste recycling site (HWRS) and the waste transfer station (WTS) yard, 

· adequate Duty of Care checks are carried out and records kept,
· wastes are deposited into their designated containers or containment areas, and

· explain what to do about non-permitted wastes that have been deposited at the site.
2.0 Scope
Waste deposited directly into the HWRS by householders.

Waste accepted into the waste transfer yard, including waste transferred from the HWRS.
3.0 Responsibility
Site manager

Site supervisor

Site operatives

Weighbridge clerk
Company drivers
Technically competent manager

4.0 Procedure
Household waste recycling site

4.1 HWRS layout and signs
4.1.1 It is the responsibility of the site manager or supervisor to ensure that clear signs are available on all containers to help members of the public locating the correct containers for their waste. 

4.2 Supervision of waste deposits in HWRS
4.2.1 The site operatives must be available to manage the delivery of household waste into the HWRS to ensure only wastes listed on the ‘Waste list for household waste recycling site (HWRS)’  is permitted onto the site.
4.2.2 Site operatives must be available to assist members of the public locating the correct containers or area for their waste to maximise the recycling rates and seek to ensure that any possibly non-compatible or unidentifiable wastes can be spotted early. 
4.2.3 Regular checks must be carried out to oversee that the correct containers are used and that waste is not deposited straight onto the floor. 
Asbestos advice
4.2.4 Members of the public should be encouraged to make prior arrangements before delivering asbestos to the HWRC. They should be advised that only cement bonded asbestos is permissible; friable asbestos wastes such as lagging is not permitted. Guidance should be given to householders to ensure they do not break or cut asbestos cement in order to fit it into bags. Instead they should be encouraged to wrap it in plastic sheeting and damp the sheeting to prevent the release of cement fibres.

Difficult wastes
4.2.5 For certain waste types, the site operatives should pay particular attention to ensure that members of the public are depositing waste correctly:

· Asbestos should be handled carefully to avoid breakages.

· Waste oil should be decanted carefully to avoid spillages.

· Car batteries should be placed in the container in an upright condition.

· Household chemicals should be placed in the secondary container in an upright condition. 

· Fridges and freezers should be handled with care to avoid damage of the coolant system and the motor.

4.2.6 Gas bottles and fluorescent tubes/energy saving light bulbs must be placed in the locked compound. These wastes should be identified as soon as possible and placed as appropriate in the compound. The compound should be locked when not in use or supervised. 
Non-permitted waste
4.2.7 In the event that a non-permitted waste is spotted prior to deposit by a member of public, the site operative should advise that the waste is not permitted at the site and, if possible, give advice on alternative disposal options.

4.2.8 If the operative is uncertain of the nature of a particular waste, or if a non-permitted waste is identified after deposit, it must be isolated away from other wastes, labelled as ‘quarantined’ and identification of it sought through the site supervisor or technically competent manager. A suitable place for disposal/recycling shall then be determined.
Transfer station 
4.3 Waste acceptance at weighbridge

4.3.1 All vehicles delivering waste must first report to the weighbridge / site office.
4.3.2 There must be a Duty of Care transfer note for all wastes being brought onto the site, except for waste transferred from the HWRS. 
4.3.3 For waste transferred from the HWRS, no waste transfer note is required but the material will be weighed and recorded. It should be checked that waste transferred from the HWRS to the transfer station is permitted for acceptance into the transfer yard.
Carrier registration

4.3.4 The weighbridge clerk will check that the customer is a registered waste carrier. Existing customer’s registration details will be recorded on the weighbridge database. New customers will need to supply evidence of a valid Carrier’s Certificate and be set up as new customer on system. (Local authorities and charities do not need to be registered waste carriers.)

4.3.5 If the Carrier’s Certificate has expired, the weighbridge clerk will advise that the customer should contact the Environment Agency to register.

Weighbridge waste checking and rejection

4.3.6 For one-off deliveries the Duty of Care transfer notes are checked by the weighbridge operator. Alternatively the documentation is validated against previous season ticket arrangements. 
4.3.7 In the event of there being no properly completed transfer note the name and address of the supplier is recorded against the registration number of the vehicle and the details of the materials delivered. 
4.3.8 Only wastes permitted to be accepted into the waste transfer yard part of the site should be accepted – refer to ‘Waste list for waste transfer yard’.
4.3.9 The weighbridge clerk will question the driver if unsure about the waste description to ensure it complies with the requirements of the environmental permit for the site. The clerk will make a visual check, whenever possible, to ensure an adequate description has been provided.
4.3.10 If the waste is acceptable, the customer will be directed to the appropriate unloading area.
4.3.11 If it is not clear if the waste is acceptable or it is described incorrectly on the waste transfer note, the customer should be directed to a segregated area and the site supervisor or technically competent manager should be contacted for further advice. 
4.3.12 If the waste is not acceptable under the terms of the permit, the weighbridge clerk should: -
· Refuse entry to the site;

· If possible, advise on alternative disposal options;
· Make record of the waste rejection in site diary with date, time, waste description, reasons for rejection, customer name and vehicle’s registration number;
· If deemed necessary, the advice of the Environment Agency may be sought.

4.4 Waste deposit and inspection in the waste transfer yard   

4.4.1 The site operatives should assist in directing the customers to the correct storage areas for their waste. Refer to SOP-03 for designated storage areas. 

4.4.2 When the waste is unloaded, the site operatives must inspect the waste to check that it meets the waste description and is acceptable at the site. 
Difficult wastes

4.4.3 Site operatives should supervise all deposits of wastes such as waste refrigeration equipment, car batteries or any liquid containerised waste, which may leak on deposit if it becomes damaged or is otherwise not handled carefully.
4.4.4 Site operatives should also supervise all deposits of asbestos in order to ensure the asbestos is handled carefully to minimise the risk of breakages during deposit. In the event that any asbestos is accidentally broken, then the actions described in the Spillage Response Procedure should be followed.
Waste ‘contraries’ – rejection or quarantine 

4.4.5 If the waste does not match its description or includes contraries (materials within the load that does not match the waste description), the appropriate action must be taken dependent on the amount and risk associated with the non-conforming waste. Where there is doubt over the appropriate action to take, the site supervisor or technically competent manager should be contacted for further advice. The following actions should be taken: 
· If only a small amount of contraries are detected of materials which are otherwise permitted on the site, these contraries can be segregated and placed in the appropriate storage area within the site.

· If only a small amount of contraries are detected of a waste type that is not permitted on the site, then the contraries need to be segregated. If possible, the customer should be asked to remove the contraries and dispose of them elsewhere. If the waste has already been accepted, however, the contraries should be segregated and quarantined. Quarantined waste should be placed in a suitable container and labeled as to its content.

· If the load in general is found not to be as described but would otherwise be acceptable at the site, then it may be appropriate to amend the waste transfer note and accept the load.

· If it is deemed that the load is unacceptable, it should be reloaded and rejected following the procedure outlined above.

4.4.6 In all circumstances where loads are found to contain contraries, this should be recorded in the Site Diary. Customers who repeatedly bring in loads with unacceptable wastes or incorrectly described wastes, should be contacted to discuss how to prevent it reoccurring.

4.5 Legal compliance for waste transfer notes and consignment notes

4.5.1 The site manager must ensure that the company’s own waste transfer note template complies with the requirements of the Duty of Care for Waste (Section 34 of the Environmental Protection Act 1990) and that the hazardous waste consignment note templates contain all the information required by the Hazardous Waste Regulations. 

4.5.2 It should also be ensured that the company is registered as a registered waste carrier.

5.0 References
· Consolidated waste list (attached)

· Waste transfer notes 

· Hazardous waste consignment notes 

· Company Registered Waste Carrier certificate 

· Weighbridge tickets 

· Site Diary
Appendix A – Consolidated waste list

	Consolidated list of acceptable wastes at site

	Waste code:
	Description:
	Transfer station yard
	Household waste site

	01
	WASTES RESULTING FROM EXPLORATION, MINING, QUARRYING, AND PHYSICAL AND CHEMICAL TREATMENT OF MINERALS
	
	

	01 01
	wastes from mineral excavation
	
	

	01 01 01
	wastes from mineral metalliferous excavation
	X
	

	01 01 02
	wastes from mineral non-metalliferous excavation
	X
	

	01 03
	wastes from physical and chemical processing of metalliferous minerals
	
	

	01 03 06
	 tailings other than those mentioned in 01 03 04 and 01 03 05
	X
	

	01 03 09
	red mud from alumina production other than the wastes mentioned in 01 03 07
	X
	

	01 04
	wastes from physical and chemical processing of non-metalliferous minerals
	
	

	01 04 08
	waste gravel and crushed rocks other than those mentioned in 01 04 07
	X
	

	01 04 09
	waste sand and clays
	X
	

	01 04 11
	wastes from potash and rock salt processing other than those mentioned in 01 04 07
	X
	

	01 04 12
	tailings and other wastes from washing and cleaning of minerals other than those mentioned in 01 04 07 and 01 04 11
	X
	

	01 04 13
	wastes from stone cutting and sawing other than those mentioned in 01 04 07
	X
	

	02
	WASTES FROM AGRICULTURE, HORTICULTURE, AQUACULTURE, FORESTRY, HUNTING AND FISHING,  FOOD PREPARATION AND PROCESSING
	
	

	02 01
	wastes from agriculture, horticulture, aquaculture, forestry, hunting and fishing
	
	

	02 01 03
	plant-tissue waste
	X
	

	02 01 04
	waste plastics (except packaging)
	X
	

	02 01 07
	wastes from forestry
	X
	

	02 01 09
	agrochemical waste other than those mentioned in 02 01 08
	X
	

	02 01 10
	waste metal
	X
	

	02 02
	wastes from the preparation and processing of meat, fish and other foods of animal origin
	
	

	02 02 03
	materials unsuitable for consumption or processing
	X
	

	02 03
	wastes from fruit, vegetables, cereals, edible oils, cocoa, coffee, tea and tobacco preparation and processing; conserve production; yeast and yeast extract production, molasses preparation and fermentation
	
	

	02 03 02
	wastes from preserving agents
	X
	

	02 03 03
	wastes from solvent extraction
	X
	

	02 03 04
	materials unsuitable for consumption or processing
	X
	

	02 04
	wastes from sugar processing
	
	

	02 04 01
	soil from cleaning and washing beet
	X
	

	02 04 02
	off-specification calcium carbonate
	X
	

	02 05
	wastes from the dairy products industry
	
	

	02 05 01
	materials unsuitable for consumption or processing
	X
	

	02 06
	wastes from the baking and confectionery industry
	
	

	02 06 01
	materials unsuitable for consumption or processing
	X
	

	02 06 02
	wastes from preserving agents
	X
	

	02 07
	wastes from the production of alcoholic and non-alcoholic beverages (except coffee, tea and cocoa)
	
	

	02 07 01
	wastes from washing, cleaning and mechanical reduction of raw materials
	X
	

	02 07 02
	wastes from spirits distillation
	X
	

	02 07 04
	materials unsuitable for consumption or processing
	X
	

	03
	WASTES FROM WOOD PROCESSING AND THE PRODUCTION OF PANELS AND FURNITURE, PULP, PAPER AND CARDBOARD
	
	

	03 01
	wastes from wood processing and the production of panels and furniture
	
	

	03 01 01
	waste bark and cork
	X
	

	03 01 05
	sawdust, shavings, cuttings, wood, particle board and veneer other than those mentioned in 03 01 04
	X
	

	03 03
	wastes from pulp, paper and cardboard production and processing
	
	

	03 03 01
	waste bark and wood
	X
	

	03 03 07
	mechanically separated rejects from pulping of waste paper and cardboard
	X
	

	03 03 08
	wastes from sorting of paper and cardboard destined for recycling
	X
	

	03 03 10
	fibre rejects, fibre-, filler- and coating-sludges from mechanical separation
	X
	

	04
	WASTES FROM THE LEATHER, FUR AND TEXTILE INDUSTRIES
	
	

	04 01
	wastes from the leather and fur industry
	
	

	04 01 01
	fleshings and lime split wastes
	X
	

	04 01 02
	liming waste
	X
	

	04 01 08
	waste tanned leather (blue sheetings, shavings, cuttings, buffing dust) containing chromium
	X
	

	04 01 09
	wastes from dressing and finishing
	X
	

	04 02
	wastes from the textile industry
	
	

	04 02 09
	wastes from composite materials (impregnated textile, elastomer, plastomer)
	X
	

	04 02 10
	organic matter from natural products (for example grease, wax)
	X
	

	04 02 15
	wastes from finishing other those mentioned in 04 02 14
	X
	

	04 02 17
	dyestuff and pigments other than those mentioned 04 02 16
	X
	

	04 02 21
	wastes from unprocessed textile fibres
	X
	

	04 02 22
	wastes from processed textile fibres
	X
	

	05
	WASTES FROM petroleum refining, natural gas purification and pyrolytic treatment of coal
	
	

	05 01
	oily sludges and solid wastes
	
	

	05 01 14
	wastes from cooling columns
	X
	

	05 01 17
	bitumen
	X
	

	05 06
	wastes from the pyrolytic treatment of coal
	
	

	05 06 04
	wastes from cooling columns
	X
	

	06
	WASTES FROM INORGANIC CHEMICAL PROCESSES
	
	

	06 03
	waste salts and their solutions
	
	

	06 03 14
	solid salts and solutions other than those mentioned in 06 03 11 and 06 03 13
	X
	

	06 03 16
	metallic oxides other than those mentioned in 06 03 15
	X
	

	06 09
	wastes from the MSFU of phosphorous chemicals and phosphorous chemical processes
	
	

	06 09 02
	phosphorous slag
	X
	

	06 09 04
	calcium-based reaction wastes other than those mentioned in 06 09 03
	X
	

	06 11
	wastes from the manufacture of inorganic pigments and opacificiers
	
	

	06 11 01
	calcium-based reaction wastes from titanium dioxide production
	X
	

	07
	WASTES FROM ORGANIC CHEMICAL PROCESSES
	
	

	07 02
	wastes from the MFSU of plastics, synthetic rubber and man-made fibres
	
	

	07 02 13
	waste plastic
	X
	

	07 02 15
	wastes from additives other than those mentioned in 07 02 14
	X
	

	07 02 17
	wastes not containing silicones other than those mentioned in 07 02 16
	X
	

	08
	WASTES FROM the manufacture, formulation, supply and use (MFSU) of coatings (paints, varnishes and vitreous enamels), adhesives, sealants and printing inks
	
	

	08 01
	wastes from MFSU and removal of paint and varnish
	
	

	08 01 12
	waste paint and varnish other than those mentioned in 08 01 11
	X
	

	08 01 18
	wastes from paint or varnish removal other than those mentioned in 08 01 17
	X
	

	08 03
	wastes from MFSU of printing inks
	
	

	08 03 13
	waste ink other than those mentioned in 08 03 12
	X
	

	08 03 18
	waste printing toner other than those mentioned in 08 03 17
	X
	

	08 04
	wastes from MFSU of adhesives and sealants (including waterproofing products)
	
	

	08 04 10
	waste adhesives and sealants other than those mentioned in 08 04 09
	X
	

	08 04 12
	adhesive and sealant sludges other than those mentioned 08 04 11
	X
	

	09
	WASTES FROM THE PHOTOGRAPHIC INDUSTRY
	
	

	09 01
	wastes from the photographic industry
	
	

	09 01 07
	photographic film and paper containing silver or silver compounds
	X
	

	09 01 08
	photographic film and paper free of silver or silver compounds
	X
	

	09 01 10
	single-use cameras without batteries
	X
	

	09 01 12
	single-use cameras containing batteries other than those mentioned in 09 01 11
	X
	

	10
	WASTES FROM THERMAL PROCESSES
	
	

	10 01
	wastes from power stations and other combustion plants (except 19)
	
	

	10 01 01
	bottom ash, slag and boiler dust (excluding boiler dust mentioned in 10 01 04)
	X
	

	10 01 05
	calcium-based reaction wastes from flue-gas desulphurisation in solid form
	X
	

	10 01 07
	calcium-based reaction wastes from flue-gas desulphurisation in sludge form
	X
	

	10 01 15
	bottom ash, slag and boiler dust from co-incineration other than those mentioned in 10 01 14
	X
	

	10 01 19
	wastes from gas cleaning other than those mentioned in 10 01 05, 10 01 07 and 10 01 18
	X
	

	10 01 21
	sludges from on-site effluent treatment other than those mentioned in 10 01 20
	X
	

	10 01 24
	sands from fluidised beds
	X
	

	10 01 25
	wastes from fuel storage and preparation of coal-fired power plants
	X
	

	10 01 26
	wastes from cooling-water treatment
	X
	

	10 02
	wastes from the iron and steel industry
	
	

	10 02 01
	wastes from the processing of slag
	X
	

	10 02 02
	unprocessed slag
	X
	

	10 02 08
	solid wastes from gas treatment other than those mentioned in 10 02 07
	X
	

	10 02 10
	mill scales
	X
	

	10 02 12
	wastes from cooling-water treatment other than those mentioned in 10 02 11
	X
	

	10 02 14
	filter cakes from gas treatment other than those mentioned in 10 02 13
	X
	

	10 02 15
	other filter cakes
	X
	

	10 03
	wastes from aluminium thermal metallurgy
	
	

	10 03 02
	anode scraps
	X
	

	10 03 05
	waste alumina
	X
	

	10 03 16
	skimmings other than those mentioned in 10 03 15
	X
	

	10 03 18
	carbon-containing wastes from anode manufacture other than those mentioned in 10 03 17
	X
	

	10 03 24
	solid wastes from gas treatment other than those mentioned in 10 03 23
	X
	

	10 03 26
	filter cakes from gas treatment other than those mentioned in 10 03 25
	X
	

	10 03 28
	wastes from cooling-water treatment other than those mentioned in 10 03 27
	X
	

	10 03 30
	wastes from treatment of salt slags and black drosses other than those mentioned in 10 03 29
	X
	

	10 04
	wastes from lead thermal metallurgy
	
	

	10 04 10
	wastes from cooling-water treatment other than those mentioned in 10 04 09
	X
	

	10 05
	wastes from zinc thermal metallurgy
	
	

	10 05 01
	slags from primary and secondary production
	X
	

	10 05 09
	wastes from cooling-water treatment other than those mentioned in 10 05 08
	X
	

	10 05 11
	dross and skimmings other than those mentioned in 10 05 10
	X
	

	10 06
	wastes from copper thermal metallurgy
	
	

	10 06 01
	slags from primary and secondary production
	X
	

	10 06 02
	dross and skimmings from primary and secondary production
	X
	

	10 06 10
	wastes from cooling-water treatment other than those mentioned in 10 06 09
	X
	

	10 07
	wastes from silver, gold and platinum thermal metallurgy
	
	

	10 07 01
	slags from primary and secondary production
	X
	

	10 07 02
	dross and skimmings from primary and secondary production
	X
	

	10 07 03
	solid wastes from gas treatment
	X
	

	10 07 05
	filter cakes from gas treatment
	X
	

	10 07 08
	wastes from cooling-water treatment other than those mentioned in 10 07 07
	X
	

	10 08
	wastes from other non-ferrous thermal metallurgy
	
	

	10 08 09
	other slags
	X
	

	10 08 11
	dross and skimmings other than those mentioned in 10 08 10
	X
	

	10 08 13
	carbon-containing wastes from anode manufacture other than those mentioned in 10 08 12
	X
	

	10 08 14
	anode scrap
	X
	

	10 08 18
	filter cakes from flue-gas treatment other than those mentioned in 10 08 17
	X
	

	10 08 20
	wastes from cooling-water treatment other than those mentioned in 10 08 19
	X
	

	10 09
	wastes from casting of ferrous pieces
	
	

	10 09 03
	furnace slag
	X
	

	10 09 06
	casting cores and moulds which have not undergone pouring other than those mentioned in 10 09 05
	X
	

	10 09 08
	casting cores and moulds which have undergone pouring other than those mentioned in 10 09 07
	X
	

	10 09 14
	waste binders other than those mentioned in 10 09 13
	X
	

	10 09 16
	waste crack-indicating agent other than those mentioned in 10 09 15
	X
	

	10 10
	wastes from casting of non-ferrous pieces
	
	

	10 10 03
	furnace slag
	X
	

	10 10 06
	casting cores and moulds which have not undergone pouring, other than those mentioned in 10 10 05
	X
	

	10 10 08
	casting cores and moulds which have undergone pouring, other than those mentioned in 10 10 07
	X
	

	10 10 14
	waste binders other than those mentioned in 10 10 13
	X
	

	10 10 16
	waste crack-indicating agent other than those mentioned in 10 10 15
	X
	

	10 11
	wastes from manufacture of glass and glass products
	
	

	10 11 03
	waste glass-based fibrous materials
	X
	

	10 11 10
	waste preparation mixture before thermal processing, other than those mentioned in 10 11 09
	X
	

	10 11 12
	waste glass other than those mentioned in 10 11 11
	X
	

	10 11 16
	solid wastes from flue-gas treatment other than those mentioned in 10 11 15
	X
	

	10 11 18
	filter cakes from flue-gas treatment other than those mentioned in 10 11 17
	X
	

	10 12
	wastes from manufacture of ceramic goods, bricks, tiles and construction products
	
	

	10 12 01
	waste preparation mixture before thermal processing
	X
	

	10 12 05
	filter cakes from gas treatment
	X
	

	10 12 06
	discarded moulds
	X
	

	10 12 08
	waste ceramics, bricks, tiles and construction products (after thermal processing)
	X
	

	10 12 10
	solid wastes from gas treatment other than those mentioned in 10 12 09
	X
	

	10 12 12
	wastes from glazing other than those mentioned in 10 12 11
	X
	

	10 13
	wastes from manufacture of cement, lime and plaster and articles and products made from them
	
	

	10 13 01
	waste preparation mixture before thermal processing
	X
	

	10 13 04
	wastes from calcination and hydration of lime
	X
	

	10 13 07
	filter cakes from gas treatment
	X
	

	10 13 10
	wastes from asbestos-cement manufacture other than those mentioned in 10 13 09
	X
	

	10 13 11
	wastes from cement-based composite materials other than those mentioned in 10 13 09 and 10 13 10
	X
	

	10 13 13
	solid wastes from gas treatment other than those mentioned in 10 13 12
	X
	

	10 13 14
	waste concrete and concrete sludge
	X
	

	11
	WASTES FROM CHEMICAL SURFACE TREATMENT AND COATING OF METALS AND OTHER MATERIALS; NON-FERROUS HYDRO METALLURGY
	
	

	11 01
	wastes from chemical surface treatment and coating of metals and other materials (for example galvanic processes, zinc coating processes, pickling processes, etching, phosphating, alkaline degreasing, anodising)
	
	

	11 01 10
	filter cakes other than those mentioned in 11 01 09
	X
	

	11 01 14
	degreasing wastes other than those mentioned in 11 01 13
	X
	

	11 02
	wastes from non-ferrous hydrometallurgical processes
	
	

	11 02 03
	wastes from the production of anodes for aqueous electrolytical processes
	X
	

	11 02 06
	wastes from copper hydrometallurgical processes other than those mentioned in 11 02 05
	X
	

	11 05
	wastes from hot galvanising processes
	
	

	11 05 01
	hard zinc
	X
	

	11 05 02
	zinc ash
	X
	

	12
	WASTES FROM SHAPING AND PHYSICAL AND MECHANICAL SURFACE TREATMENT OF METALS AND PLASTICS
	
	

	12 01
	wastes from shaping and physical and mechanical surface treatment of metals and plastics
	
	

	12 01 01
	ferrous metal filings and turnings
	X
	

	12 01 03
	non-ferrous metal filings and turnings
	X
	

	12 01 05
	plastics shavings and turnings
	X
	

	12 01 13
	welding wastes
	X
	

	12 01 17
	waste blasting material other than those mentioned in 12 01 16
	X
	

	12 01 21
	spent grinding bodies and grinding materials other than those mentioned in 12 01 20
	X
	

	13
	OIL WASTES AND WASTES OF LIQUID FUELS
	
	

	13 02
	waste engine, gear and lubricating oils
	
	

	13 02 05*
	mineral-based non chlorinated engine, gear and lubricating oils
	
	X

	13 02 06*
	synthetic engine, gear and lubricating oils
	
	X

	13 02 07*
	readily biodegradable engine, gear and lubricating oils
	
	X

	15
	WASTE PACKAGING; ABSORBENTS, WIPING CLOTHS, FILTER MATERIALS AND PROTECTIVE CLOTHING NOT OTHERWISE SPECIFIED
	
	

	15 01
	packaging (including separately collected municipal packaging waste)
	
	

	15 01 01
	paper and cardboard packaging
	X
	

	15 01 02
	plastic packaging
	X
	

	15 01 03
	wooden packaging
	X
	

	15 01 04
	metallic packaging
	X
	

	15 01 05
	composite packaging
	X
	

	15 01 06
	mixed packaging
	X
	

	15 01 07
	glass packaging
	X
	

	15 01 09
	textile packaging
	X
	

	15 02
	absorbents, filter materials, wiping cloths and protective clothing
	
	

	15 02 03
	absorbents, filter materials, wiping cloths and protective clothing other than those mentioned in 15 02 02
	X
	

	16
	WASTES NOT OTHERWISE SPECIFIED IN THE LIST
	
	

	16 01
	end-of-life vehicles from different means of transport [including off-road machinery] and wastes from dismantling of end-of-life vehicles and vehicle maintenance (except 13, 14, 16 06 and 16 08)
	
	

	16 01 03
	end-of-life tyres
	X
	X

	16 01 04*
	end-of-life vehicles
	X
	

	16 01 06
	end-of-life vehicles, containing neither liquids nor other hazardous components
	X
	

	16 01 07*
	oil filters
	X
	

	16 01 11*
	brake pads containing asbestos
	X
	

	16 01 12
	brake pads other than those mentioned in 16 01 11
	X
	

	16 01 16
	tanks for liquefied gas
	X
	

	16 01 17
	ferrous metal
	X
	

	16 01 18
	non-ferrous metal
	X
	

	16 01 19
	plastic
	X
	

	16 01 20
	glass
	X
	

	16 01 22
	components not otherwise specified
	X
	

	16 02
	wastes from electrical and electronic equipment
	
	

	16 02 11*
	discarded equipment containing chlorofluorocarbons, HCFC, HFC
	X
	

	16 02 13*
	discarded equipment containing hazardous components(2) other than those mentioned in 16 02 09 to 16 02 12
	X
	

	16 02 14
	discarded equipment other than those mentioned in 16 02 09 to 16 02 13
	X
	

	16 02 16
	components removed from discarded equipment other than those mentioned in 16 02 15
	X
	

	16 03
	off-specification batches and unused products
	
	

	16 03 04
	inorganic wastes other than those mentioned in 16 03 03
	X
	

	16 03 06
	organic wastes other than those mentioned in 16 03 05
	X
	

	16 05
	gases in pressure containers and discarded chemicals
	
	

	16 05 05
	gases in pressure containers other than those mentioned in 16 05 04
	
	X

	16 06
	batteries and accumulators
	
	

	16 06 01*
	lead batteries
	X
	

	16 06 04
	alkaline batteries (except 16 06 03)
	X
	

	16 06 05
	other batteries and accumulators
	X
	

	16 08
	spent catalysts
	
	

	16 08 01
	spent catalysts containing gold, silver, rhenium, rhodium, palladium, iridium or platinum (except 16 08 07)
	X
	

	16 08 03
	spent catalysts containing transition metals or transition metal compounds not otherwise specified
	X
	

	16 11
	waste linings and refractories
	
	

	16 11 02
	carbon-based linings and refractories from metallurgical processes others than those mentioned in 16 11 01
	X
	

	16 11 04
	other linings and refractories from metallurgical processes other than those mentioned in 16 11 03
	X
	

	16 11 06
	linings and refractories from non-metallurgical processes others than those mentioned in 16 11 05
	X
	

	17
	CONSTRUCTION AND DEMOLITION WASTES (INCLUDING EXCAVATED SOIL FROM CONTAMINATED SITES)
	
	

	17 01
	concrete, bricks, tiles and ceramics
	
	

	17 01 01
	concrete
	X
	X

	17 01 02
	bricks
	X
	X

	17 01 03
	tiles and ceramics
	X
	X

	17 01 07
	mixtures of concrete, bricks, tiles and ceramics other than those mentioned in 17 01 06
	X
	X

	17 02
	wood, glass and plastic
	
	

	17 02 01
	wood
	X
	

	17 02 02
	glass
	X
	

	17 02 03
	plastic
	X
	

	17 03
	bituminous mixtures, coal tar and tarred products
	
	

	17 03 02
	bituminous mixtures other than those mentioned in 17 03 01
	X
	

	17 04
	metals (including their alloys)
	
	

	17 04 01
	copper, bronze, brass
	X
	

	17 04 02
	aluminium
	X
	

	17 04 03
	lead
	X
	

	17 04 04
	zinc
	X
	

	17 04 05
	iron and steel
	X
	

	17 04 06
	tin
	X
	

	17 04 07
	mixed metals
	X
	

	17 04 11
	cables other than those mentioned in 17 04 10
	X
	

	17 05
	soil (including excavated soil from contaminated sites), stones and dredging spoil
	
	

	17 05 04
	soil and stones other than those mentioned in 17 05 03
	X
	

	17 05 06
	dredging spoil other than those mentioned in 17 05 05
	X
	

	17 05 08
	track ballast other than those mentioned in 17 05 07
	X
	

	17 06
	insulation materials and asbestos-containing construction materials
	
	

	17 06 01*
	insulation materials containing asbestos
	X
	X

	17 06 04
	insulation materials other than those mentioned in 17 06 01 and 17 06 03
	X
	X

	17 06 05*
	construction materials containing asbestos
	X
	X

	17 08
	gypsum-based construction material
	
	

	17 08 02
	gypsum-based construction materials other than those mentioned in 17 08 01
	X
	X

	17 09
	other construction and demolition wastes
	
	

	17 09 04
	mixed construction and demolition wastes other than those mentioned in 17 09 01, 17 09 02 and 17 09 03
	X
	

	18
	WASTES FROM human or animal health care and/or related research (except kitchen and restaurant wastes arising from immediate health care)
	
	

	18 01
	wastes from natal care, diagnosis, treatment or prevention of disease in humans
	
	

	18 01 07
	chemicals other than those mentioned in 18 01 06
	X
	

	18 02
	wastes from research, diagnosis, treatment or prevention of disease involving animals
	
	

	18 02 06
	chemicals other than those mentioned in 18 02 05
	X
	

	19
	WASTES FROM WASTE MANAGEMENT FACILITIES, OFF-SITE WASTE WATER TREATMENT PLANTS AND PREPARATION OF WATER INTENDED FOR HUMAN CONSUMPTION/INDUSTRIAL USE
	
	

	19 01
	wastes from incineration or pyrolysis of waste
	
	

	19 01 02
	ferrous materials removed from bottom ash
	X
	

	19 01 12
	bottom ash and slag other than those mentioned in 19 01 11
	X
	

	19 01 18
	pyrolysis wastes other than those mentioned in 19 01 17
	X
	

	19 01 19
	sands from fluidised beds
	X
	

	19 02
	wastes from physico/chemical treatments of waste (including dechromatation, decyanidation, neutralisation)
	
	

	19 02 03
	premixed wastes composed only of non-hazardous wastes
	X
	

	19 02 10
	combustible wastes other than those mentioned in 19 02 08 and 19 02 09
	X
	

	19 03
	stabilised/solidified wastes 
	
	

	19 03 05
	stabilised wastes other than those mentioned in 19 03 04
	X
	

	19 03 07
	solidified wastes other than those mentioned in 19 03 06
	X
	

	19 04
	vitrified waste and wastes from vitrification
	
	

	19 04 01
	vitrified waste
	X
	

	19 05
	wastes from aerobic treatment of solid wastes
	
	

	19 05 01
	non-composted fraction of municipal and similar wastes
	X
	

	19 05 02
	non-composted fraction of animal and vegetable waste
	X
	

	19 05 03
	off-specification compost
	X
	

	19 08
	wastes from waste water treatment plants not otherwise specified
	
	

	19 08 01
	screenings
	X
	

	19 08 02
	waste from desanding
	X
	

	19 09
	wastes from the preparation of drinking water or water for industrial use
	
	

	19 09 01
	solid waste from primary filtration and screenings
	X
	

	19 09 04
	spent activated carbon
	X
	

	19 09 05
	saturated or spent ion exchange resins
	X
	

	19 10
	wastes from shredding of metal-containing wastes
	
	

	19 10 01
	iron and steel waste
	X
	

	19 10 02
	non-ferrous waste
	X
	

	19 10 04
	fluff-light fraction and dust other than those mentioned in 19 10 03 
	X
	

	19 10 06
	other fractions other than those mentioned in 19 10 05
	X
	

	19 12
	wastes from the mechanical treatment of waste (for example sorting, crushing, compacting, pelletising) not otherwise specified
	
	

	19 12 01
	paper and cardboard
	X
	

	19 12 02
	ferrous metal
	X
	

	19 12 03
	non-ferrous metal
	X
	

	19 12 04
	plastic and rubber
	X
	

	19 12 05
	glass
	X
	

	19 12 07
	wood other than that mentioned in 19 12 06
	X
	

	19 12 08
	textiles
	X
	

	19 12 09
	minerals (for example sand, stones)
	X
	

	19 12 10
	combustible waste (refuse derived fuel)
	X
	

	19 12 12
	other wastes (including mixtures of materials) from mechanical treatment of wastes other than those mentioned in 19 12 11
	X
	

	19 13
	wastes from soil and groundwater remediation
	
	

	19 13 02
	solid wastes from soil remediation other than those mentioned in 19 13 01
	X
	

	20
	MUNICIPAL WASTES (HOUSEHOLD WASTE AND SIMILAR COMMERCIAL, INDUSTRIAL AND INSTITUTIONAL WASTES) INCLUDING SEPARATELY COLLECTED FRACTIONS
	
	

	20 01
	separately collected fractions (except 15 01)
	
	

	20 01 01
	paper and cardboard
	X
	X

	20 01 02
	glass
	X
	X

	20 01 08
	biodegradable kitchen and canteen waste
	X
	X

	20 01 10
	clothes
	X
	X

	20 01 11
	textiles
	X
	X

	20 01 13*
	solvents
	
	X

	20 01 14*
	acids
	
	X

	20 01 15*
	alkalines
	
	X

	20 01 17*
	photochemicals
	
	X

	20 01 19*
	pesticides
	
	X

	20 01 21*
	fluorescent tubes and other mercury-containing waste
	
	X

	20 01 23*
	discarded equipment containing chlorofluorocarbons
	X
	X

	20 01 25
	edible oil and fat
	
	X

	20 01 26*
	oil and fat other than those mentioned in 20 01 25
	
	X

	20 01 27*
	paint, inks, adhesives and resins containing dangerous substances
	
	X

	20 01 28
	paint, inks, adhesives and resins other than those mentioned in 20 01 27
	
	X

	20 01 29*
	detergents containing dangerous substances
	
	X

	20 01 30
	detergents other than those mentioned in 20 01 29
	
	X

	20 01 33*
	batteries and accumulators included in 16 06 01, 16 06 02 or 16 06 03 and unsorted batteries and accumulators containing these batteries
	X
	X

	20 01 34
	batteries and accumulators other than those mentioned in 20 01 33
	X
	X

	20 01 35*
	discarded electrical and electronic equipment other than those mentioned in 20 01 21 and 20 01 23 containing hazardous components(6)
	X
	X

	20 01 36
	discarded electrical and electronic equipment other than those mentioned in 20 01 21, 20 01 23 and 20 01 35
	X
	X

	20 01 37*
	wood containing dangerous substances
	
	X

	20 01 38
	wood other than that mentioned in 20 01 37
	X
	X

	20 01 39
	plastics
	X
	X

	20 01 40
	metals
	X
	X

	20 01 41
	wastes from chimney sweeping
	X
	X

	20 02
	garden and park wastes (including cemetery waste)
	
	

	20 02 01
	biodegradable waste
	X
	X

	20 02 02
	soil and stones
	X
	X

	20 02 03
	other non-biodegradable wastes
	X
	X

	20 03
	other municipal wastes
	
	

	20 03 01
	mixed municipal waste
	X
	X

	20 03 02
	waste from markets
	X
	

	20 03 03
	street-cleaning residues
	X
	

	20 03 07
	bulky waste
	X
	X
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