Schedule 5 - Notification 

This page outlines the information that the Operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part A 
	Permit Number
	EPR/PR3733PC V010

	Name of Operator
	Biffa Waste Services Limited

	Location of Facility
	Trecatti Landfill Site

Fochriw Road

Merthyr Tydfil

Mid Glamorgan

CF48 4AB

	
	

	Time and date of the detection 
	17/12/2018 @ 12:58



	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and Time of the event
	N/A

	Reference or description of the location of the event 
	N/A

	Description of where any release into the environment took place
	N/A

	Substances(s) potentially released
	N/A

	Best estimate of the quantity or rate of release of substances
	N/A

	Measures taken, or intended to be taken, to stop any emission
	N/A

	Description of the failure or accident.
	N/A


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	81705002

81705004



	Parameter(s)
	Dust Monitoring. 
Deposited Dust

	Limit
	Deposited Dust 200 mg/m3 

	Measured value and uncertainty
	81705002 Deposited Dust 230 mg/m2
81705004 Deposited Dust 270 mg/m2

	Date and time of monitoring
	 30/11/2018 @ 09:49

	Measures taken, or intended to be taken, to stop the emission
	The emission is unlikely to be arising from this installation due to the location of the sampling points, wind direction and weather conditions at the time of sampling. 


	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	Dust Monitoring  
	24 Hours


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	N/A

	Substances(s) detected
	N/A

	Concentrations of substances detected
	N/A

	Date of monitoring/sampling
	N/A


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	Site experienced heavy rainfall during the 24 hour period of monitoring. The wind direction was South Westerly during this time.

As a consequence the labs were asked if they could verify the results as 81705004 was upwind of operations with 81705002 being downwind. 

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	The contractors have been booked in to return to the site to carry out Dust Monitoring at the same locations for Deposited Dust.  

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	No pollution to the environment occurred due to this reading.  

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	No schedules for Dust Monitoring within the last 24 Months.


	Name*
	Simon Milford

	Post
	Site Manager

	Signature
	Simon Milford

	Date
	07.01.19


* authorised to sign on behalf of the Operator.

