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	Consent no
	NRWWIA363

	
	


WATER INDUSTRY ACT 1991

SECTION 165 / 166
CONSENT TO DISCHARGE

TO:
Dŵr Cymru Cyfyngedig 


Linea House


Fortran Road 


St Mellons 


Cardiff 


CF3 0LT  
	The NATURAL RESOURCES BODY FOR WALES ("Natural Resources Wales") in pursuance of its powers under the Water Industry Act 1991 HEREBY CONSENTS to the making of a discharge as follows:
Raw Water 


	FROM: Canaston Bridge Water Pumping Station, Canaston Bridge,

              Narberth, Pembrokeshire, SA67 8DF

	

	AT: NATIONAL GRID REFERENCE SN 06487 14697

	

	TO: Eastern Cleddau

	

	SUBJECT TO: the conditions set out in the following schedule:

Raw Water                     Schedule No. NRWWIA363

	

	This consent is issued on the 21st day of March 2023
This consent takes effect on the 1st day of April 2023
This consent shall cease to have effect on the 31st day of March 2028
Signed: Stephanie Evans


	


CONDITIONS OF CONSENT TO DISCHARGE

RAW WATER (“the Discharge”)

NATURE OF THE DISCHARGE

1.
The Discharge shall consist solely of raw water. 

SOURCE OF THE DISCHARGE

2. The Discharge shall be derived from Canaston Bridge Water Pumping Station.
LOCATION OF DISCHARGE

3.
The location of the Discharge shall be at NGR SN 06487 14697, marked ‘Discharge point at SN 06487 14697” on the site plan in Annex 1.
SAMPLE POINT

4.
A sample point shall be provided and maintained so that a representative sample of the Discharge may be obtained. 

VOLUME

5. The total daily volume of the Discharge shall not exceed 5000 cubic metres.

6. The rate of the Discharge shall not exceed 50 litres per second.
COMPOSITION

7.
The consent holder shall take all necessary steps to secure that any water discharged by it under this consent is as free as may be reasonably practicable from — 

(a) 
mud and silt;

(b) 
solid, polluting, offensive or injurious substances; 
and

(c)
any substances prejudicial to fish or spawn, or to spawning beds or food of fish.
SCOURING
8.
The rate of discharge shall be controlled to prevent any significant scouring of the bed or bankside of the receiving water. 
FLOODING

09.
The discharge shall not cause or significantly contribute to flooding in the downstream catchment.
PERIOD OF DISCHARGE

10.
The Discharge shall only be made between 1st day of April 2023 and the 31st day of March 2028.
ANNEX 1- PLAN No. NRWWIA363
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