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Mr Guy Baskerville
Natural Resources Wales (NRW)
Cambria House
29 Newport Road
Cardiff
CF24 0TP
BY EMAIL

Dear Guy,

Resources Management (UK) Limited - WITHYHEDGE LANDFILL SITE
4th Quarterly Monitoring Report 2022

[bookmark: _Hlk115338862]Please find enclosed a summary of the monitoring data for leachate, groundwater, surface water and landfill gas collected at Withyhedge Landfill Site for the 1st Quarter of 2023, review period January to March 2023. This letter summarises the main findings with reference to the compliance limits set in the Site Permit (reference EPR/MP3330WP, previously GP3630HT/V005).

LEACHATE
Leachate Volume
[bookmark: _Hlk112162935][bookmark: _Hlk123906926]A total of 6242 tonnes of leachate were removed off-site during the period January to March 2023. 

Leachate levels
Leachate level monitoring data for this quarter, consistent with the requirements in Table S4.1 of the Permit, are provided in the Site Monitoring Worksheets.

There were no exceedances of the compliance limits during the review period January to March 2023. 

However, the total leachate volume extracted from boreholes LE1-LE6 was lower than the total monthly limits of 106 m3/month at 26 m3, 25 m3 and 25 m3 for the months of January, February, and March respectively.  The low extraction is the result of the low levels of leachate in the wells. The leachate pumps only work when the leachate levels in the wells are greater than 0.8m. 

Leachate quality
Leachate quality monitoring data is provided in the Site Monitoring Worksheets and will be reviewed as part of the Annual Report as required by Condition 4.9 of the Permit. 

GROUNDWATER
Groundwater level
Groundwater levels are recorded monthly and are provided in the Site Monitoring Worksheets.
Groundwater quality sampling
Groundwater quality sampling is undertaken on a monthly and quarterly basis in accordance with Table S4.5 and Table S4.11 of the Permit. The groundwater quality monitoring data has been assessed against the compliance limits set in the Permit and are provided in the Site Monitoring Worksheets. 

There were no exceedances of the compliance limits during the review period January to March 2023.

SURFACE WATER
Surface water is monitored monthly in accordance with Table S4.3 and Table S4.10 of the Permit and the surface water quality data is the Site Monitoring Worksheets. 
There were no exceedances of the compliance limits during the review period January to March 2023.


LANDFILL GAS
CO2, CH4 and O2 are monitored on a fortnightly basis in all gas collection wells and any other (in-waste) gas monitoring points as specified in Table S4.8 of the Permit. The remaining locations are monitored monthly as specified in Table S4.6 and S4.8 of the Permit. The results of landfill gas monitoring are provided in the Site Monitoring Worksheets.


Engines Emissions
The engines are monitored for oxides of nitrogen, carbon monoxide on a quarterly basis in accordance with table S4.2 of the permit. The results of the quarterly engines monitoring are provided in the Site Monitoring Worksheets


I trust that the above meets your requirements; please do not hesitate to contact me if you have any queries.

Yours sincerely,

Phil Ridley
Business development Director
The Dauson Environmental group.
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