Schedule 5 - Notification                            TIR0237 05/05/2023

Part A 
	Permit Number
	VP3935AT

	Name of Operator
	Enovert South Ltd

	Location of Installation
	Tir John Landfill, Wern Terrace, Off Fabian Way, Swansea, SA1 8PA

	Time and date of the detection 
	April 2023

	(b) Notification requirements for the breach of a limit (within 24 hours unless otherwise agreed)

	Emission point reference/ source
	Phase 2 LEW Leachate Wells
Leachate Head above Cell Base
>1m
See Table 1 Below

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	Leachate remains contained within the engineered containment system, so no emission from the site is occurring.


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	Leachate removal to sewer is ongoing.

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	Landfill capping works progressed well in 2021 and 2022, which will reduce rainfall infiltration.

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	The elevated levels in LEW14 are due to the pump failing due to the well conditions and a solution has been discussion within Enovert and with NRW. Dosing with bleach failed to break up the blockage, we are now looking into maceration. We managed to get a pump working in August, but this got fouled subsequently by the precipitate causing the blockages and destroyed the pump. 
Similar precipitate issues are evidencing in other areas of the site, all are under ongoing investigation and the precipitate has been sampled for laboratory analysis.

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	See previous notifications.


	Name*
	Elizabeth Forrest

	Post
	Environmental Data Analyst

	Date
	05/05/2023


[bookmark: _Int_iiKeGdxg]* authorised to sign on behalf of Enovert South Ltd









	Sample Point
	Date
	Leachate Head (m)
	Comment

	LEW07
	18/04/2023
	4.47
	

	LEW07
	29/04/2023
	4.42
	

	LEW09a
	18/04/2023
	4.06
	

	LEW09a
	29/04/2023
	4.06
	

	LEW09b
	18/04/2023
	16.63
	Blockage in well

	LEW09b
	29/04/2023
	16.65
	Blockage in well

	LEW13a
	18/04/2023
	1.25
	

	LEW13a
	29/04/2023
	1.09
	

	LEW14
	18/04/2023
	16.61
	Blockage in well

	LEW14
	29/04/2023
	16.66
	Blockage in well

	LEW15
	18/04/2023
	1.38
	

	LEW15
	29/04/2023
	1.38
	

	LEW16
	18/04/2023
	1.06
	

	LEW16
	29/04/2023
	1.01
	

	LEW20
	18/04/2023
	1.77
	

	LEW20
	29/04/2023
	1.66
	

	LEW21
	18/04/2023
	2.44
	

	LEW21
	29/04/2023
	2.47
	

	LEW22
	18/04/2023
	1.66
	

	LEW22
	18/04/2023
	1.70
	

	LEW23
	18/04/2023
	3.97
	

	LEW23
	29/04/2023
	3.94
	

	LEW24
	18/04/2023
	3.17
	

	LEW24
	29/04/2023
	3.11
	

	LEW25
	18/04/2023
	4.42
	

	LEW25
	29/04/2023
	4.45
	

	LEW26
	18/04/2023
	2.73
	

	LEW26
	29/04/2023
	2.68
	

	LEW27
	18/04/2023
	3.18
	

	LEW27
	29/04/2023
	3.23
	

	LEW28
	18/04/2023
	1.40
	

	LEW28
	29/04/2023
	1.29
	

	LEW29
	18/04/2023
	7.59
	Pump is being repaired

	LEW29
	29/04/2023
	7.53
	Pump is being repaired

	LEW32
	18/04/2023
	2.95
	

	LEW32
	29/04/2023
	3.09
	


Table 1: Breach of Compliance Limit for Leachate Boreholes Phase 2 area April 2023
