Schedule 5 - Notification
These pages outline the information that the operator must provide.

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part A
	Permit Number
	EP3034GS

	Name of operator
	Wynnstay

	Location of Facility
	Llysonnen Mill, Carmarthen

	Time and date of the detection
	12/10/22 16:31



	(a) Notification requirements for any activity that gives rise to an incident or accident which significantly affects or may significantly affect the environment

	To be notified Immediately

	Date and time of the event
	

	Reference or description of the location of the event
	

	Description of where any release into the environment took place
	

	Substances(s) potentially
released
	

	Best estimate of the quantity or rate of release of substances
	

	Measures taken, or intended to
be taken, to stop any emission
	

	Description of the failure or
accident.
	



	(b) Notification requirements for the breach of a permit condition

	To be notified immediately

	Emission point reference/ source
	W1

	Parameter(s)
	Total suspended solids

	Limit
	15 mg/l

	Measured value and uncertainty
	76.7 mg/l +/- 10 %

	Date and time of monitoring
	29/09/22 14:00

	Measures taken, or intended to be taken, to stop the emission
	The site drainage system has been assessed by an external drainage consultant.  It has been identified that the design of the attenuation tank is likely to be contributing to the exceedances in TSS.  A proposal for a revised site drainage system including appropriately designed attenuation tank with silt traps is awaiting board approval.

The site hygiene will continue to be monitored and maintained to a high standard to reduce the amount of TSS entering the surface water drainage system.



	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	



	(c) In the event of a breach of permit condition which poses an immediate danger to human health
or threatens to cause an immediate significant adverse effect on the environment:

	To be notified immediately

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances
detected
	

	Date of monitoring/sampling
	




Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify,
limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	



	Name*
	 Sally Davies

	Post
	QC & Compliance Manager

	Signature
	[image: ]

	Date
	15/02/23


* authorised to sign on behalf of the Operator
.
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