Schedule - Notification

This page outlines the information that the operator must provide.
Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.
Part A

	Permit Number
	BU0800IZ
	Name of Operator
	3C Waste Limited
	Location of Facility
	Llanddulas Landfill
	
	

	Time and date of the detection
	See Part A (b)



	(a) Notification requirements for any incident or accident which significantly affects or may significantly affect the environment

	To be notified within 24 hours of detection

	Date and Time of the event
	
	Reference or description of the location of the event
	
	Description of where any release into the environment took place
	

	Substance(s) potentially released
	
	Best estimate of the quantity or rate of release of substances 
	
	Measures taken, or intended to be taken, to stop any emission
	
	Description of the failure or accident.
	


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference / source
	As listed

	Parameter(s) 
	As listed
	Limit
	As listed
	Measure value and uncertainty
	See table below 
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	Date and time of monitoring
	As listed
	Measures taken, or intended to be taken, to stop the emission
	Action plan in place to rectify leachate level exceedances, please see further information in part B.  


	
Time periods for notification following detection of a breach of a limit

	Parameter 
	Notification period

	As listed	Click or tap here to enter text.


	(c) Notification requirements in the event of a breach of permit condition which poses an immediate danger to human health or threatens to cause an immediate significant adverse effect on the environment

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances detected
	
	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B To be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	Please note that the delay in submission of this information has been due to the sudden departure of the site’s Compliance Advisor (back in March 2023), and time taken to recruit and hand over to the new compliance advisor.  There have also been issues with the information in the in-house monitoring database, which are being resolved as a matter of urgency
	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	There is an issue with the base of LCP2Cr.  When the chamber was drilled, Dragon Drilling had an issue with cobble blocks at the base, they carried out ‘pressure grouting’ to extract all materials from the base, but this was unsuccessful.  This is detailed on the attached CQA plan.  Due to this, some of the chamber depth has been lost and it also silts up on a regular basis.  The air pump in the chamber is repositioned at regular intervals as required, however this continues to become blocked with silt.  The combination of these factors has made it difficult to obtain a complaint dip to liquid reading (Vs CQA base), despite the chamber appearing compliant Vs field DTB (dip to base)
	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	An access platform must be built so a de-silt rig can access the chamber, after that we will book a contractor in to carry out desilting works on the chamber in question.  The air pump will then be reinstalled at the correct position and the chamber dipped to monitor levels decide next course of action
	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	N/A


	Name*
	Chris Bennion
	Post
	Site Business Manager
	Signature
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	Date
	23/08/2023

* authorised to sign on behalf of the operator
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