Schedule 6 – Notification
These pages outline the information that the operator must provide.
Units of measurement used in information supplied under Part A and B requirements shall be appropriate
to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions 

and authorized emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential 

information, supplied on a separate sheet and accompanied by an application for commercial confidentiality 

under the provisions of the PPC Regulations.

Part A
	Permit Number / Variation Notice Number
	BR8212IK / (EPR/BR8212IK/V004)

	Name of operator
	Knauf Insulation

	Location of Installation
	Cwmbran

	Time and date of the detection
	17/05/2019 approx 09:00-12:00


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	17th May 2019 approx 09:00-12:00

	Reference or description of the location of the event
	A0 – White Wool Stack

	Description of where any release into the environment took place
	To air in the Pontypool /Cwmbran area 

	Substance(s) potentially

released
	Total Particulate Matter

	Best estimate of the quantity or rate of release of substance
	Average three sample result of 38.4 mg/m3

	Measures taken, or intended to be taken, to stop any emission
	Investigating root cause by reviewing process data and undertaking site investigation. Re-sampling to take place 24/07/19 to verify results.

	Description of the failure or accident
	Investigation ongoing


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	A0

	Parameter(s)
	Total Particulate Matter

	Limit
	35 mg/m3

	Measured value and uncertainty
	38.4 mg/m3    +/- 2.3

	Date and time of monitoring
	17th May 2019 approximately 09:00-12:00

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection 

	
	

	Substance(s) detected
	Total Particulate Matter

	Concentrations of substances detected
	38.4 mg/m3

	Date of monitoring/sampling
	17th May 2019 between 09:00-12:00


Part B – to be submitted as soon as practicable

	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused be the emission
	

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	


	Name*
	Warren Christy

	Post 
	HS&E Manager

	Signature
	                             [image: image1.emf]

	Date
	18/07/2019


* authorised to sign on behalf of Knauf Insulation Limited

Permit Number BR8212IK

Variation Notice Number EA/EPR/BR8212IK/V003


