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	Consent no
	NRWWIA378

	
	


WATER INDUSTRY ACT 1991

SECTION 165 / 166
CONSENT TO DISCHARGE

TO:
Dŵr Cymru/Welsh Water

Linea


Fortran Road


St. Mellons


Cardiff


CF3 0LT
	The NATURAL RESOURCES BODY FOR WALES ("Natural Resources Wales") in pursuance of its powers under the Water Industry Act 1991 HEREBY CONSENTS to the making of a discharge as follows:
Raw Water


	FROM: LLANISHEN RESERVOIR, LLANISHEN, CARDIFF, CF23 6PZ

	

	AT: NATIONAL GRID REFERENCE ST 18750 81437

	

	TO: NANT FAWR

	

	SUBJECT TO: the conditions set out in the following schedule:

Raw Water                                        Schedule No. NRWWIA378-01

	

	This consent is issued on the 3rd day of January 2024
This consent takes effect on the 8th day of January 2024
This consent shall cease to have effect on the 29th day of January 2024
Signed: Emma Jones


	


CONDITIONS OF CONSENT TO DISCHARGE

RAW WATER (“the Discharge”)

NATURE OF THE DISCHARGE

1.
The Discharge shall consist solely of raw water. 

SOURCE OF THE DISCHARGE

2. The Discharge shall be derived from Llanishen Reservoir.
LOCATION OF DISCHARGE

3.
The location of the Discharge shall be at NGR ST 18750 81437, marked ‘Discharge Point’ on the site plan in Annex 1.
SAMPLE POINT

4.
A sample point shall be provided and maintained so that a representative sample of the Discharge may be obtained. 

VOLUME

5. The total volume of the Discharge shall not exceed 228,039 cubic metres.

6. The total daily volume of the Discharge shall not exceed 17,280 cubic metres.

7. The rate of the Discharge shall not exceed 200 litres per second.
COMPOSITION

8.
The consent holder shall take all necessary steps to secure that any water discharged by it under this consent is as free as may be reasonably practicable from — 

(a) 
mud and silt;

(b) 
solid, polluting, offensive or injurious substances; 
and

(c)
any substances prejudicial to fish or spawn, or to spawning beds or food of fish.
SCOURING
9.
The rate of discharge shall be controlled to prevent any significant scouring of the bed or bankside of the receiving water. (as in line with Environmental Risk Assessment and Management System dated 18/12/2023 and submitted as part of the application of consent and approved by NRW.)
FLOODING

10.
The discharge shall not cause or significantly contribute to flooding in the downstream catchment.
PERIOD OF DISCHARGE

11.
The Discharge shall only be made between 8th day of January 2024 and the 29th day of January 2024.
ANNEX 1- PLAN No. NRWWIA378
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