


Permit Number: 	EPR/BV4177IS			Operator: 		Volac International Ltd

Facility:		Volac Felinfach		Form Number: 	 Air1 / 16/03/2022
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission Point
	0BSubstance / Parameter
	Emission Limit Value
	Reference Period
	Monitoring frequency
	Result0F[footnoteRef:1] [1:  The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.] 

	Test Method1F[footnoteRef:2] [2:  Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases, the principal technique is stated, for example gas chromatography.] 

	Sample Date and Times2F[footnoteRef:3] [3:  For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   ] 

	Uncertainty3F[footnoteRef:4] [4:  The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.] 


	A15
	Sulphur Dioxide (SO2)
	30 mg/Nm3
	Periodic
	Annual
	
	BS EN 14791
	
	

	
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	250 mg/Nm3
	Periodic
	Annual
	
	BS EN 14792
	
	

	
	Total Particulate Matter (PM)
	10 mg/Nm3
	Periodic
	Annual
	
	BS EN 13284-1
	
	

	
	Carbon Monoxide (CO)
	150 mg/Nm3
	Periodic
	Annual
	
	BS EN 15058
	
	

	
	Carbon Monoxide (CO)
	150 mg/Nm3
	Hourly average
	Continuous Measurement
	
	BS EN 14181[footnoteRef:5] [5:  CEMs which meet the MCERTS requirements should also follow the principles of EN 14181 (i.e. QAL2/AST and QAL3) but a reduced number of parallel measurements may be acceptable (subject to NRW approval).] 

	
	





Signed …………………………………………………………….  		Date………………………...   	
	(Authorised to sign as representative of Operator)
Permit Number: 	EPR/BV4177IS			Operator: 		Volac International Limited

Facility:		Volac Felinfach                           	Form Number: 	Sewer1 / 16/03/2022
Reporting of emissions to sewer, effluent treatment plant or other transfers off-site for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	S1
	Biological Oxygen Demand
	10,000 mg/l
	Spot sample
	
	BS EN 1899-1
	
	

	
	Chemical Oxygen demand
	22,162 mg/l
	Spot sample
	
	BS 6068-2.34 or ISO 6060
	
	

	
	Copper
	1.0 mg/l
	Spot sample
	
	BS EN ISO 11885
	
	

	
	Lead
	1.0 mg/l
	Spot sample
	
	BS EN ISO 11885
	
	

	
	Nitrogen, total oxidised as N
	50 mg/l
	Spot sample
	
	BS EN ISO 11905-1, BS EN 12260 or BS ISO 29441
	
	

	
	Phosphate as P
	No limit set
	Spot sample
	
	BS EN ISO 6878
	
	

	
	Suspended Solids
	3,324 mg/l
	Spot sample
	
	BS EN 872
	
	

	
	Flow
	No limit set
	Hourly average (continuous)
	
	Volumetric method
	
	


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)
Permit Number: 	EPR/BV4177IS			Operator: 		Volac International Ltd

Facility:		Volac Felinfach		Form Number: 	Water1 / 16/03/2022
Reporting of emissions to water (other than to sewer) and land for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission Point
	0BSubstance / Parameter[footnoteRef:6] [6:  Table S3.2 of the permit states that the discharge at W1 and W2 is to be free of any visible solids, oil or grease.] 

	Emission Limit Value
	Test Method1F
	Month
	Result[footnoteRef:7] [7:  For each monitoring period, the operator should confirm the presence (or otherwise) of any of the stated substances.] 

	Sample Date and Times

	W1
	Visible solids, oil or grease
	Discharge to be free of any visible solids, oil or grease
	Visual check
	January
	
	

	
	
	
	
	February
	
	

	
	
	
	
	March
	
	

	
	
	
	
	April
	
	

	
	
	
	
	May
	
	

	
	
	
	
	June
	
	

	
	
	
	
	July
	
	

	
	
	
	
	August
	
	

	
	
	
	
	September
	
	

	
	
	
	
	October
	
	

	
	
	
	
	November
	
	

	
	
	
	
	December
	
	

	

	W2
	Visible solids, oil or grease
	Discharge to be free of any visible solids, oil or grease
	Visual check
	January
	
	

	
	
	
	
	February
	
	

	
	
	
	
	March
	
	

	
	
	
	
	April
	
	

	
	
	
	
	May
	
	

	
	
	
	
	June
	
	

	
	
	
	
	July
	
	

	
	
	
	
	August
	
	

	
	
	
	
	September
	
	

	
	
	
	
	October
	
	

	
	
	
	
	November
	
	

	
	
	
	
	December
	
	



Signed …………………………………………………………….  		Date………………………...
	(Authorised to sign as representative of Operator)

 
Permit Number: 	EPR/BV4177IS			Operator: 		Volac International Ltd

Facility:		Volac Felinfach		Form Number: 	Performance1 / 16/03/2022

Reporting of other performance indicators for the period DD/MM/YYYY to DD/MM/YYYY

	Parameter
	Quantity
	Units 
	

	
	
	
	

	Total feed production 
	
	tonnes
	

	Total food production
	
	tonnes
	

	Waste disposal and/or recovery
	
	t/tonne
	



	Operator’s comments:








Signed …………………………………………………………….  		Date………………………...   	
	(Authorised to sign as representative of Operator)







