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APPLICATION FOR A MARINE LICENCE FOR MARINE WORKS

Marine Works include, but are not limited to, coast defences, beneficial uses of dredged materials, subsea cables, pontoons, jetties, land reclamation, grab samples and outfall pipes under the Marine and Coastal Access Act 2009

Please read the notes carefully before completing the form.
The Marine Licensing Team (MLT) administers Part 4 of the Marine and Coastal Access Act 2009 on behalf of the Licensing Authority, the Welsh Ministers.

The completed application form must be accompanied by a location plan and, where appropriate, descriptive drawing(s) and any supporting environmental assessments. One completed hard copy of the application and supporting documents will always be required. Additional copies are required for consultation purposes. 

· For application and supporting documents less than 10MB we can accept an additional copy via email.  
· For applications larger than 10MB 16 additional copies in CD/DVD format will be required 
· When applications and supporting documents are hard copy only 16 copies will be required.

Please submit applications to the Permit Receipt Centre via the details at the top of this form
 
Please submit marine licence applications, including this form and all supporting documents, at least 4 months before the licence is required.

Some projects may raise matters that require a significantly longer time for consideration. These are most likely to be:

· Projects that fall within The Marine Works (Environmental Impact Assessment) Regulations 2007 – as amended requiring an Environmental Statement
· Large scale projects with substantial volumes of material being deposited or excavated
· Works requiring an Appropriate Assessment to be conducted under The Conservation of Habitats and Species Regulations 2017.

Information should be provided about the anticipated duration of the entire project in respect of works below/seaward of Mean High Water Spring (MHWS). Where appropriate, planned phasing of the work for which consent is sought must be detailed. For projects lasting more than one calendar year, planned phasing details must be given for each 12 month period.

A licence fee is payable in respect of an application. Details of fees can be found on our web pages.

Please note applications will not be processed without the correct relevant fee or invoicing details.  

Payments can be made via Cheque, BACS or credit/debit card. 
· Cheques should be crossed and made payable to Natural Resources Wales. 
· For BACS payments ensure you provide the reference number (not remittance number)
· For credit/debit card payments please complete the CC1 form and submit with the application. The CC1 form can be found on our web pages

Further information on payment methods can be found on our web pages

All activities need to comply with the Water Framework Directive (WFD). The framework and guidance can be found on the Natural Resources Wales website, http://naturalresources.wales. The results of your WFD assessment must be attached to your marine licence application.

Please answer all questions. If any information is not available at the time of application please indicate in the relevant section, giving reasoning in a covering letter. Outstanding details must be submitted as soon as possible. Any delay in forwarding details is likely to result in delays in determining your application.

Your application may not be considered complete and therefore not processed until key information has been submitted. Your application may be returned if you fail to submit outstanding information within given timescales.
 
Please note any licence may have conditions that must be discharged before works can commence. This will take additional time. 
If you have any queries with regards to completing this application please contact the MLT: marinelicensing@naturalresourceswales.gov.uk

How your application will be processed by the MLT: 

Submit all application to the Permit Receipt Centre via the details at the top of this form.

Checked and acknowledged by the MLT within 21 days of receipt of application and payment 

If the application is complete and no further information is needed at this time, your application will be placed in a work queue to be assigned a permitting officer

If the application is not complete, further information will be request and need to be provided before the application can be considered as complete

Our 4 months service level for determining non-EIA applications will begin from the date the completed application is received (Please note some projects may take significantly longer than 4 months to determine due to their nature)

EIA projects may take significantly longer due to their scale and complexity. Therefore we encourage early engagement with the MLT

Your application and supporting documents will be sent to for an initial consultation period of 28 days (42 days for EIA projects)

For the majority of projects, a public notice must be advertised. Public consultation will be 28 days (49 days for EIA projects).
For EIA projects a second public notice will be required. The MLT will advise on how this should be done.

Responses to consultation will be considered and additional information requested at this time, if necessary.

A decision on your Marine Licence Application will be made

All information submitted may be referred to within a licence, therefore all works must be in accordance with this information, unless otherwise agreed with NRW acting on behalf of the Licensing Authority during the determination process.

It is the responsibility of the applicant to obtain any other consents/authorisations that may be required.

Application Form Structure 
1. Project Description and Cost
2. Applicant Details
3. Details of Agent, Contractor, Vehicles and/or Vessels used to carry out works 
4. Environmental Impact Assessment (EIA)
5. Licensable Period
6. Project Description
7. Methods Statement
8. Materials of Project 
9. Beach Replenishment, Land Reclamation or Salt Marsh Feeding
10. Temporary Works
11. Dredge and Disposal of Dredge Material
12. Protected Sites
13. Other Consents
14. Statutory Powers
15. Public Register
16. Application Fee
17. Declaration

Check List
Please ensure that you have included all the necessary information before you submit you application. If any of the below are not completed in the application form, the application is likely to be considered incomplete and may be returned to you

	Item
	Yes (√)

	The applicant is a legal entity?
	Y

	The declaration is signed by the applicant?
	Y

	Is the application fee correct?
	Y

	Are the grid references/coordinates correct?
	Y

	Do the coordinates match map locations?
	Y

	Have all the relevant supporting documents been submitted?
	Y

	Has a clear methodology been provided in the application form?
	Y

	Has Protected sites information been included?
	Y

	Has a Water Framework Directive (WFD) assessment been submitted?
	

	Are all the continuation sheets for application questions appended with correct corresponding numbers?
	


	
Should you have any queries regarding you application please contact the MLT via marinelicensing@naturalresourceswales.gov.uk  

1. Project Description and Cost

1 (a).	Project Name

Living Sea Walls – Menai Strait




1(b).	Please provide a brief description of the proposed project, including location

The North Wales Rivers Trust, are aiming to install Living Sea Wall panels onto modern walls throughout the Menai Strait are various locations on both the Gwynedd and Ynys Mon side. 







1(c).	Please provide an estimated gross cost of the project (Inc. materials and labour) for works that fall below/seaward of Mean High Water Springs (MHWS)
£40,000





2. Applicant Details
To whom the licence will be issued. This must be a legal entity such as an individual, registered company/ charity or public body. 
Mr			
Liam Whitmore

Title				Full Name

Company or Trading
NameNorth Wales Rivers Trust

06100324

Company Registration
Number (if applicable)
Liam Whitmore

Name of Contact or 
individual (if different)
River Restoration Officer

Position in Company

Gwel Yr Afon, Llanddoged, Llanrwst, Conwy, Wales, LL26 0TY

Address inc. postcode
(provide registered
Company address if
applicable)


Telephone Number07972564796


liam@northwalesriverstrust.org


Email Address
3. Details of Agent, Contractor, Vehicles and/or Vessels used to carry out works 

3(a).	Agent Details 
This is who we will correspond with unless otherwise informed. If no agent we will contact the applicant.



Title				Full Name

Company or Trading
Name



Company Registration
Number (if applicable)


Name of Contact or 
individual (if different)

Position in Company




Address 
(Inc. postcode)






Telephone Number



Email Address

3(b).	Does the Applicant wish to be included in all correspondence? Yes ☒	No ☐

3(c).	Contractor Details
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Contractor Company or Trading Name
	Address

	
Not yet awarded.

	
Details will be provided before work commences. Please provide any further precautions/information that is required of the contractor.


	


	



	


	



3(d).	Will the works require the use of vessels?				Yes ☒	No ☐

3(d) (i).Vessel Details (if applicable and available)
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Operator
	Name of Vessel
	Type of Vessel
	Vessel Registration Number
	Country of Registration

	

	
	
	
	

	

	
	
	
	

	

	
	
	
	

	

	
	
	
	




3(e).	Will the works require the use of vehicle?				Yes ☒	No ☐

3(e) (i). Vehicle Details (if applicable and available) to be used below MHWS
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Operator 
	Type/Description of Vehicle

	

	Only for transportation purposes of LSW panels to some sites which are not accessible by foot.

	

	

	

	

	

	




3(f).	If the contractor or vessels or vehicles are not known at the application stage, when do you expect to provide these details?
These details will need to be confirmed prior to the licence and operations commencement


Within the 4 month application process.







4. Environmental Impact Assessment (EIA)
Certain projects, due to their scale, location and/or nature, may require an EIA under the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended). If a project qualifies under EIA, an Environmental Statement (ES) must be prepared and submitted with the application.

Projects that fall within Annex I of the Directive automatically require an EIA. Projects that fall within Annex II of the Directive are assessed on a case-by-case basis for the requirement for an EIA to be undertaken.

4(a).	Do you consider the works to be under the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended)?				Yes ☒	No ☐									
4(a) (i) If Yes, which Annex does the proposal fall under?	     Annex I☐	   Annex II☒

4(a) (ii) Which number(s) within the Annex does the proposal relate to?






4(b).	Have you applied for a screening or scoping opinion from the MLT under the Marine Works (Environmental Impact Assessment) Regulations 2007 (as amended)?  									Yes ☐	No ☒


4(b) (i). If Yes, please provide the reference number

4(c).	Has an Environmental Impact Assessment been undertaken? 	Yes ☐ No ☒											
4(c)(i).If Yes, has an Environmental Statement been submitted to support this Marine Licence application? 						Yes ☐ No ☐	

4(d).	If an Environmental Impact Assessment has been undertaken, but an ES has not been submitted, please provide an explanation







Please continue on a separate sheet if necessary. Please tick if you have done this ☐

5. Licensable Period

Determination of applications will be based on the works taking place during these dates. Please ensure you have included an adequate contingency period. If works are not completed by the Requested Licence Expiry Date you may be required to submit a new application. Including a contingency period within your original application does not impact on Licence Fee
01/05/2025
01/05/2024

Start Date				Requested Licence Expiry Date


Please ensure you submit your application for a Marine Licence at least 4 months prior to the intended start date. Some projects, such as EIA projects, will take significantly longer to determine.
6. Project Description

6(a).	Please give a description of the proposed project.
This should include the purpose of the project, estimated timescales of construction and operation, and broken down by the phases of works, if applicable.
Details should include, but not be limited to, dimensions of project, quantity of material being deposited and removed.

The Menai Strait has a wide variety of habitat types and is home to over 1,400 recorded species of plants and animals. The area forms part of the Menai Strait and Conwy Special Area of Conservation (SAC) and Site of Special Scientific Interest (SSSI). This is a designation which enables the protection of special habitat types and species (excluding birds) which are considered to be most in need of conservation at a European level. The combination of strong currents in the Strait along with other environmental factors has led to the development of a number of rare features and unusual animal associations. However, there are a number of urbanised coastal regions along the Menai Strait, which have degraged the local environment and ecology of these particular areas as they provide minimal habitat. 

We aim to improve the available habitat at modern, urban sea walls with Living Sea Wall (LSW) panels to improve biodiversity within the Menai Strait. Living Sea Walls (LSWs) are an innovative way to utilise cutting-edge technology and apply it to degraded man-made marine habitats. LSWs are 3-D printed panels which help diversify the structural habitat of degraded man-made coastal structures. These urbanised shorelines are detrimental to marine life, providing a non-porous mono-textured environment and by diversifying the structural environment, it will boost marine biodiversity and benefit the Strait.

We are aiming to install LSWs in the Summer period (July-September), but have included a sufficient contingency period. Installation of LSW panels we foresee to take no longer than 2 weeks to complete all sites along Gwynedd and Ynys Mon.

Living Sea Walls are hexagonal panels made from super tough concrete, weigh approx. 25kg per panel, and have a variety of naturally mimicking textures. They are fitted to urbanised walls with a maximum or 4 fixings, using rebar screws. LSW panels are not flush with the urbanised wall, leaving an approx. 10cm gap between the wall and the back of the panel (also provided more habitat). These panels can be removed if necessary. We are estimating to install 100-200 panels across the listed sites onto modern urbanised walls.












































Please continue on a separate sheet if necessary. Please tick if you have done this ☐

6(b).	Please detail the location of the proposed construction project.
This should be either Ordnance Survey National Grid Reference (i.e. AB 12345 67890) or Latitude and Longitude in decimal degrees to 4 decimal places (i.e. Lat 52.1234 Long -4.1234), defining the extent of the project. Please specify which coordinate system has been used.
There are multiple discrete sites where we are aiming to install Living Sea Walls (NGR used).

Gwynedd: 

Site 1 – Aber foreshore, midpoint: SH 47087 62579

Site 2 – Shell site car park modern wall, midpoint: SH 48034 63317

Site 3 – Modern wall below Britannia Bridge, midpoint: SH 54150 70891

Site 4 – Garth Pier car park modern wall, midpoint: SH 58419 73209

Site 4a – Garth Pier house newly installed concrete sea wall, midpoint: SH 58456 73218

Ynys Mon

Site 1 – Beaumaris pier, western wall (lower), midpoint: SH 60627 75933

Site 2 – Concrete road wall, front face, midpoint: SH 62649 79510

Site 3 – Modern road wall, near Anglesey Sea Zoo, midpoint: SH 47897 65262

Site 4 – Coastal wall, near Menai Bridge slipway. Midpoint: SH 55846 71827 (this would be a small trial site, using smaller than standard sized panels (max of 6 panels) at this site, as an educational tool.

The NWRT are not seeking to cover more than 20% of the total sea wall ay any site.




































Please continue on a separate sheet if necessary. Please tick if you have done this ☐
6(c).	The following must be provided with the completed application form:

(i) a suitably scaled extract of an Ordnance Survey Map or Admiralty Chart with location of project, complete with North Arrow and Scale

(ii) construction plans and sectional drawings showing those proposed works below/seaward of MHWS, which should give details of the materials to be used (for beach replenishment the quantity, particle size and source of material to be deposited and deposit location is also required).

(iii) a descriptive schematic drawing and suitably scaled location plan which show the full extent of the project clearly in relation to the surrounding area and features.
Please list below all supporting documents that have been submitted with this application, including suitable documents/maps/drawing titles and reference numbers

LSW01 - Proposed LSW sites (modern walls) v1

LIVING SEAWALLS INSTALATION MANUAL JULY 2023

LIVING SEAWALLS PRODUCT INFORMATION JULY 2023 (1)

















Please continue on a separate sheet if necessary. Please tick if you have done this ☐

The applicant should note that these drawings/plans may be copied to others as part of the MLT's consultation procedures. If they are subject to copyright, it is the responsibility of the applicant to obtain the necessary approvals to reproduce the documents and to submit up to 16 copies with the application.

7. Methods Statement

7(a).	Please provide a detailed method statement for the works
This must include methods for all works including temporary structures or deposits such as jetties, cofferdams, moorings or landing stages to be constructed seaward of MHWS
Installation of LSWs
Living Seawall panels are attached to sandstone or concrete walls using M16 SS 316 threaded rod. There are 4 connection points per panel; the recommended number will depend on the wave energy at the installation site. For high energy sites, all 4 connection points can be used with the panel positioned flush to the seawall. For low energy sites 3 connection points can be used with a maximum of 100mm gap between the back of panel and seawall. Panels can also be glued to a flat seawall with a marine grouting system and a single centre connection point. We recommend consultation with the Living Seawalls team before installation. *Bolt holes for securing the threaded rod must be cleaned prior to inserting adhesive.

















Fastening options:
Option A is suitable for sites that have high wave energy because they are close to harbour/estuarine mouths or have high exposure to boat traffic. Panels should be installed using all four bolting holes and offset from the seawall to mitigate disturbing established local marine habitat.
Option B is suitable for sites where seawalls experience moderate to low to high wave energy. Panels should be installed using at least three bolting holes and offset from the seawall to enhance habitat potential. Option C is suitable for sites where high wave energy is experienced and the seawall surface is flat. Panels should be secured with at least one bolt and thread and a generous coating of epoxy on the backside of each panel
Option C is suitable for sites where high wave energy is experienced and the seawall surface is flat. Panels should be secured with at least one bolt and thread and a generous coating of epoxy on the backside of each panel.
Mark out height and length of installation area as per panel configuration diagram. Use a panel template to mark drill points along length of seawall. Panels can be positioned to interlock snugly or be separated. Avoid disturbing existing growth except where holes must be drilled. Cut the stainless steel threaded rods to required length. Core-drill or hammer drill out the designated bolt hole locations using a M18 masonry drill bit. The number of drill holes depends on the wave energy of the site. Drill holes should be 80-100 mm deep, dependent on seawall condition. If using 3 connection points per panel, any of the panel's 4 available connection points can be used. 1. MEASURE AND DRILL I













Mark out height and length of installation area as per panel configuration diagram. Use a panel template to mark drill points along length of seawall. Panels can be positioned to interlock snugly or be separated. Avoid disturbing existing growth except where holes must be drilled. Cut the stainless steel threaded rods to required length. Core-drill or hammer drill out the designated bolt hole locations using a M18 masonry drill bit. The number of drill holes depends on the wave energy of the site. Drill holes should be 80-100 mm deep, dependent on seawall condition. If using 3 connection points per panel, any of the panel's 4 available connection points can be used. Any refueling of equipment will be carried out at least 10m from the high mean water mark.

ALL LIVING SEA WALL PANELS WILL BE FITTED BY HAND, BUT MAY REQUIRE A VESSEL, TEMPORARY JETTY TO TRANSPORT LSW FOR INSTALLATION.












Please continue on a separate sheet if necessary. Please tick if you have done this ☐

7(b). Do you intend to undertake activities that could generate underwater noise?
This include piling, use of explosives, geophysical, acoustic deterrent devices and multibean echosounders. 								Yes ☐ No ☐






7(b) (i). If Yes, what type(s) of activities will be undertaken?














7(b) (ii). If Yes, approximately how many days will the activity be undertaken for?  

We estimate no longer than 2-3 weeks, although each discrete site should be completed in 1 day. 












If Yes, you will be required to complete an additional form that will be provided.

7(c).	Please state the measures to be taken to:
(i) Minimise risk to the marine environment 
If a temporary Jetty is to be used (may only be required at one site; shell site car park Caernarfon), this project will be finished within a day and the jetty will be removed after that day. 

All LSW panels will be fitted by hand and no use any machinery to install them.












(ii) Prevent undue interference to others 
All installation areas will be cordoned off from others. No installation would affect any highways traffic. 














(iii) Maintain navigational safety, including marking and lighting of works
All work will take place during the day.














Please continue on a separate sheet if necessary. Please tick if you have done this ☐

8. Materials of Project 

8(a).	Description of materials to be deposited seaward of MHWS (Please tick all that apply)
Timber	☐	Iron/Steel	☐	Concrete	☒	Biocides/other chemicals	☐
Silt		☐	Stone/Rock	☐	Gravel		☐	Plastic/Synthetics		☐ 
Sand	☐	Other		☐	

If other, please provide a description of materials.













8(b).	Delivery method of materials to site
If sea delivery, please include details of vessels to be used with a chart of proposed route and transhipment area. If vehicle delivery, please provide the proposed access route. 
For the majority of sites, materials will be delivered via vehicle. However, two sites may require delivery via vessel (Gwynedd site 2, 3). Details of this can be confirmed at a later date.












Please continue on a separate sheet if necessary. Please tick if you have done this ☐

8(c).	Will the works involve removals seaward of MHWS?3		Yes ☐ No ☒

8(c) (i). Description of materials to be removed seaward of MHWS (Please tick all that apply)
Timber	☐	Iron/Steel	☐	Concrete	☐	Biocides/other chemicals	☐
Silt		☐	Stone/Rock	☐	Gravel		☐	Plastic/Synthetics		☐ 
Sand	☐	Other		☐	
8(c) (ii). Description of objects/materials to be removed seaward of MHWS
Including quantities to be removed.















9. Beach Replenishment, Land Reclamation or Salt Marsh Feeding
For works involving any of the above, please provide the following information 

9(a). Is the material to be deposited like for like to existing material? 	Yes ☐ No ☐

9(a)(i) If No for Beach Replenishment please provide justification why?













9(b).	Description of material to be deposited
Please provide the grading specification of materials to be used, if using a range of grain sizes please state the percentage by weight passing. If unsure, please refer to the Wentworth Scale 
















Please continue on a separate sheet if necessary. Please tick if you have done this ☐

9(c).	Source of the material to be deposited
Including dredged or land based stating the origin of material
















9(d).	Has the material been chemically analysed? 			Yes ☐ No ☐
If material has been analysed, we may request this information to determine the application

9(d) (i) If Yes, is the analysis data been included with the application? Yes ☐ No ☐


10. Temporary Works

10(a).	Will there be any temporary deposits below MHWS? 		Yes ☒ No ☐
This includes construction materials, removed objects/material, jetties or cofferdams
If Yes, please continue with section 10

10(b).	Please provide the location of temporary deposits 
Please include a map/chart displaying the location of temporary deposits, if necessary.
A Jetty may be used at one site (Gwynedd site 2) as the sediment exposed at low tide isn’t consolidated to support weight. This jetty would be installed for 1 day only during installation. 













10(c).	Description of temporary deposits
Temporary buoyant modular jetty. 
















Please continue on a separate sheet if necessary. Please tick if you have done this ☐


11. Dredge and Disposal of Dredge Material
If you are undertaking Dredge and Disposal activities please also complete the Dredge and Disposal application form and submit together.

11(a).	Do you intend to apply for a marine licence to dispose of dredged material to sea as part of the works in this application? 			Yes ☐ No ☒

12. Protected Sites

Licensing Authorities have a duty to ensure that projects will not have significant adverse environmental impact, particularly on any designated European Site of Conservation Importance - Special Areas of Conservation (SAC) and Special Protection Areas (SPA), listed under the Habitats Directive (Council Directive 92/42/EEC on the conservation of natural habitats and of wild fauna and flora). In addition, it is Government Policy that Wetlands of International Importance (Ramsar sites) are also considered as European Sites.  There is a duty to take reasonable steps to further the conservation and enhancement of nationally designated sites (Sites of Special Scientific Interest (SSSIs).

12(a).	Have you had pre-application correspondence with NRW, its legacy bodies or Natural England? 								Yes ☐ No ☒


12(a)(i). If Yes, please provide copies of correspondence with application and state which team(s) you have contacted? 















12(b).	Are any part of the works located within or likely to affect a designated conservation site? (SAC, SPA, SSSI or Ramsar)			 Yes ☒ No ☐

12(b)(i). If Yes, which designated site(s) may be affected?
Ynys Mon site 2 (NGR: SH 62649 79510)
sssi_name:
GLANNAU PENMON - BIWMARES
sssi_id:
545
sssi_code:
31WYW
type:
Mixed/Mstatus:
Confirmedlayer:SSSI Non River Designationshape_length: 14061.046462371167 shape_area:
115318.74545767524





















12(c).	Please provide a description of all mitigation measures proposed to avoid any impact on designated conservation sites.
Biosecurity measures will be adhered to, and any equipment will be properly cleaned, sanitised before accessing this site. 

All materials (LSWs) will be fitted by hand, so no large machinery will be used on site and therefore any disturbance will be kept to a minimum. 

A power drill will be required but this will only be used when necessary for installation.



















Please continue on a separate sheet if necessary. Please tick if you have done this ☐

12(d).	If the works are not located within or likely to affect a designated conservation site, please indicated the approximate distance to the nearest designated conservation site.













Please note that if the proposed works are in or within 2km of a European Site of Conservation Importance you will have to provide suitable mitigation measure to avoid any impact on designated conservation sites.

13. Other Consents

Please detail all consents that you have applied for or received for these works

	Type of Consent
	Applied for
	To be applied for
	Reference Number
	Date of Issue and Expiry

	Planning Permission under Town and County Planning Act 1990 – From Local Planning Authority (LPA)

	N/A
	
	
	

	Name and Address of LPA for location of works

	




	Land Owners Consent such as The Crown Estate Consent

	
	
	
	

	Port Authority or Local Harbour permissions

	
	
	
	

	Other NRW consents such as Flood Defence or SSSI assent
	
	
	
	

	Details of NRW consent

	

	Other consents such as Transport and Works Act Order, Section 36 Electricity Act, grant/loan sanction
	
	
	
	

	Details of other consents 


	



14. Statutory Powers

14(a).Does the applicant have statutory powers to consent any aspect of the project? 
E.g. coast protection authority, dredging powers, statutory undertakers	Yes ☐ No ☒

14(a)(i).If Yes, please give details and state the relevant legislation that gives these powers
















15. Public Register

Under The Marine Licensing (Register of Licensing Information)(Wales) Regulations 2011 and the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended) , all information contained within or provided in support of this application will be placed on the Public Register unless NRW approve of the applicant’s reasons for withholding all or part.	

15.	Is there any information contained within or provided in support of this application that you consider should NOT be included on the Public Register on the grounds that its disclosure:

15(a).	Would be contrary to the interest of National Security? 		Yes ☐ No ☒

15(b).	Would prejudice to an unreasonable degree you, or some other person’s commercial interest of those of a third party? 			Yes ☐ No ☒

If Yes to either (a) or (b), please provide full justification as to why all or part of the information you have provided should be withheld
























Please continue on a separate sheet if necessary. Please tick if you have done this ☐

16. Application Fee

16(a). What are the corresponding fee band for this application? Band 2 ☒ Band 3 ☐

16(b) Band 2 Only
Projects are charged at a fixed fee of £1920. The application will not be processed until the correct fee has been provided.

Please provide the method of payment 

	Method
	Yes (√)
	Reference Number

	Cheque
	
	

	BACS (not remittance no.)
	YES


	PRCAPPNORTHLSW

	World Pay (phone or CC1)
	

	


Please attach CC1 Form with application. Can be found on our web pages

16(c) Band 3 Application only
Band 3 applications are charged at on hourly rate of £120 and are invoiced in arrears. Please complete the details below which will be required for invoicing.


Customer Name




FAO



Purchase order number



Address for invoice





Telephone Number





Email Address




17. Declaration

I declare that to the best of my knowledge and belief that the information given in this application form and supporting documentation is true.

	WARNING: It is an offence under the Marine and Coastal Access Act 2009, under which this application is made, to fail to disclose information or to provide false or misleading information and can invalidate any licence granted.




Signature		[image: ]			15.03.24			Date	



Name (in capitals)	Liam Whitmore

Position in Company	River restoration team							
	

Applications cannot be processed unless signed by the Applicant (not agent), the applicant must have appropriate level of authority within the company.

Applications will not be processed unless signed
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