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Natural Resources Wales
29 Newport Road
Cambria House
Cardiff 
CF24 0TP
  Tel: 0300 065 3000
 Email: permitreceiptcentre@naturalresourceswales.gov.uk

[bookmark: _Hlk160550611]APPLICATION FOR A MARINE LICENCE FOR MARINE WORKS

Marine Works include, but are not limited to, coast defences, beneficial uses of dredged materials, subsea cables, pontoons, jetties, land reclamation, grab samples and outfall pipes under the Marine and Coastal Access Act 2009

Please read the notes carefully before completing the form.
The Marine Licensing Team (MLT) administers Part 4 of the Marine and Coastal Access Act 2009 on behalf of the Licensing Authority, the Welsh Ministers.

The completed application form must be accompanied by a location plan and, where appropriate, descriptive drawing(s) and any supporting environmental assessments. One completed hard copy of the application and supporting documents will always be required. Additional copies are required for consultation purposes. 

· For application and supporting documents less than 10MB we can accept an additional copy via email.
· For applications larger than 10MB 16 additional copies in CD/DVD format will be required. 
· When applications and supporting documents are hard copy only 16 copies will be required.

Please submit applications to the Permit Receipt Centre via the details at the top of this form.
 
Please submit marine licence applications, including this form and all supporting documents, at least 4 months before the licence is required.

Some projects may raise matters that require a significantly longer time for consideration. These are most likely to be:

· Projects that fall within The Marine Works (Environmental Impact Assessment) Regulations 2007 – as amended requiring an Environmental Statement
· Large scale projects with substantial volumes of material being deposited or excavated
· Works requiring an Appropriate Assessment to be conducted under The Conservation of Habitats and Species Regulations 2017

Information should be provided about the anticipated duration of the entire project in respect of works below/seaward of Mean High Water Spring (MHWS). Where appropriate, planned phasing of the work for which consent is sought must be detailed. For projects lasting more than one calendar year, planned phasing details must be given for each 12 month period.

A licence fee is payable in respect of an application. Details of fees can be found on our web pages.

Please note applications will not be processed without the correct relevant fee or invoicing details.

Payments can be made via Cheque, BACS or credit/debit card. 
· Cheques should be crossed and made payable to Natural Resources Wales. 
· For BACS payments ensure you provide the reference number (not remittance number)
· For credit/debit card payments please complete the CC1 form and submit with the application. The CC1 form can be found on our web pages

Further information on payment methods can be found on our web pages

All activities need to comply with the Water Framework Directive (WFD). The framework and guidance can be found on the Natural Resources Wales website, http://naturalresources.wales. The results of your WFD assessment must be attached to your marine licence application.

Please answer all questions. If any information is not available at the time of application please indicate in the relevant section, giving reasoning in a covering letter. Outstanding details must be submitted as soon as possible. Any delay in forwarding details is likely to result in delays in determining your application.

Your application may not be considered complete and therefore not processed until key information has been submitted. Your application may be returned if you fail to submit outstanding information within given timescales.
 
Please note any licence may have conditions that must be discharged before works can commence. This will take additional time. 
If you have any queries with regards to completing this application please contact the MLT: marinelicensing@naturalresourceswales.gov.uk

How your application will be processed by the MLT: 

Submit all application to the Permit Receipt Centre via the details at the top of this form.

Checked and acknowledged by the MLT within 21 days of receipt of application and payment 

If the application is complete and no further information is needed at this time, your application will be placed in a work queue to be assigned a permitting officer

If the application is not complete, further information will be requested and need to be provided before the application can be considered as complete

Our 4 months service level for determining non-EIA applications will begin from the date the completed application is received (Please note some projects may take significantly longer than 4 months to determine due to their nature)

EIA projects may take significantly longer due to their scale and complexity. Therefore we encourage early engagement with the MLT

Your application and supporting documents will be sent to for an initial consultation period of 28 days (42 days for EIA projects)

For the majority of projects, a public notice must be advertised. Public consultation will be 28 days (49 days for EIA projects).
For EIA projects a second public notice will be required. The MLT will advise on how this should be done.

Responses to consultation will be considered and additional information requested at this time, if necessary.

A decision on your Marine Licence Application will be made

All information submitted may be referred to within a licence, therefore all works must be in accordance with this information, unless otherwise agreed with NRW acting on behalf of the Licensing Authority during the determination process.

It is the responsibility of the applicant to obtain any other consents/authorisations that may be required.

Application Form Structure 
1. Project Description and Cost
2. Applicant Details
3. Details of Agent, Contractor, Vehicles and/or Vessels used to carry out works 
4. Environmental Impact Assessment (EIA)
5. Licensable Period
6. Project Description
7. Methods Statement
8. Materials of Project 
9. Beach Replenishment, Land Reclamation or Salt Marsh Feeding
10. Temporary Works
11. Dredge and Disposal of Dredge Material
12. Protected Sites
13. Other Consents
14. Statutory Powers
15. Public Register
16. Application Fee
17. Declaration

Check List
Please ensure that you have included all the necessary information before you submit you application. If any of the below are not completed in the application form, the application is likely to be considered incomplete and may be returned to you

	Item
	Yes (√)

	The applicant is a legal entity?
	√

	The declaration is signed by the applicant?
	√

	Is the application fee correct?
	√

	Are the grid references/coordinates correct?
	√

	Do the coordinates match map locations?
	√

	Have all the relevant supporting documents been submitted?
	√

	Has a clear methodology been provided in the application form?
	√

	Has Protected sites information been included?
	√

	Has a Water Framework Directive (WFD) assessment been submitted?
	√

	Are all the continuation sheets for application questions appended with correct corresponding numbers?
	N/A


	
Should you have any queries regarding you application please contact the MLT via marinelicensing@naturalresourceswales.gov.uk  

1. Project Description and Cost

1 (a).	Project Name
Chapel Reen (Outfall Repairs)



1(b).	Please provide a brief description of the proposed project, including location
The purpose of the project is to repair the Chapel Reen outfall (the scheme), which is centred at National Grid Reference ST 367830, in the village of Goldcliff to the south-east of Newport in South Wales. The repairs will comprise the replacement of a collapsed masonry wall with a new sheet piled retaining wall and replacement of the existing masonry channel bed with a reinforced concrete bed. Upgrades to the tidal flap and reinstatement of an effluent pipe from the Farmers Arms pub to its original position (following a temporary relocation during previous emergency works) will also be undertaken. The works required to complete the scheme are referred to as the proposed works. 












1(c).	Please provide an estimated gross cost of the project (Inc. materials and labour) for works that fall below/seaward of Mean High Water Springs (MHWS)
£250k




2. Applicant Details
To whom the licence will be issued. This must be a legal entity such as an individual, registered company/ charity or public body. 
Mr
David Jenkins

Title				Full Name

Company or Trading
NameNatural Resources Wales

 N/A

Company Registration
Number (if applicable)


Name of Contact or 
individual (if different)
Project Manager, Projects and Programme Delivery

Position in Company

Plas Gwendraeth, Heol Parc Mawr,
Crosshands Business Park, Cross Hands,
Llanelli, Carmarthenshire, 
SA14 6RE


Address inc. postcode
(provide registered
Company address if
applicable)


Telephone Number07815 977515


Email Addressdavid.jenkins@cyfoethnaturiolcymru.gov.uk

3. Details of Agent, Contractor, Vehicles and/or Vessels used to carry out works 

3(a).	Agent Details 
This is who we will correspond with unless otherwise informed. If no agent we will contact the applicant.
Ella Niehorster
Ms

Title				Full Name

Company or Trading
NameBinnies UK Ltd.

03163649

Company Registration
Number (if applicable)


Name of Contact or 
individual (if different)

Position in CompanyPrincipal Environmental Scientist


1 Redwood Court, Tawe Business Village, Phoenix Way, Swansea, SA7 9LAs

Address 
(Inc. postcode)




01737 856281  

Telephone Number
niehorstere@binnies.com 


Email Address

3(b).	Does the Applicant wish to be included in all correspondence? Yes ☒	No ☐

3(c).	Contractor Details
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Contractor Company or Trading Name
	Address

	
To be confirmed prior to commencement of operations. This will be confirmed following a competitive tender process. 





3(d).	Will the works require the use of vessels?				Yes ☐	No ☒

3(d) (i).Vessel Details (if applicable and available)
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Operator
	Name of Vessel
	Type of Vessel
	Vessel Registration Number
	Country of Registration

	

	
	
	
	

	

	
	
	
	

	

	
	
	
	

	

	
	
	
	




3(e).	Will the works require the use of vehicle?			Yes ☒	No ☐

3(e) (i). Vehicle Details (if applicable and available) to be used below MHWS
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Operator 
	Type/Description of Vehicle

	To be confirmed

	Suitably sized 360˚ excavator 

	To be confirmed


	Suitably sized wheeled or tracked dumper

	To be confirmed
	All-terrain mobile crane (1005)

	To be confirmed
	Remotely controlled trench roller

	To be confirmed

	Piling plant and equipment

	

	

	*Please note that details of any additional plant and the operator will be confirmed following contract award and prior to commencement of the works.




3(f).	If the contractor or vessels or vehicles are not known at the application stage, when do you expect to provide these details?
These details will need to be confirmed prior to the licence and operations commencement

Contractor to be appointed in April/May 2024, details to be confirmed following appointment.







4. Environmental Impact Assessment (EIA)
Certain projects, due to their scale, location and/or nature, may require an EIA under the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended). If a project qualifies under EIA, an Environmental Statement (ES) must be prepared and submitted with the application.

Projects that fall within Annex I of the Directive automatically require an EIA. Projects that fall within Annex II of the Directive are assessed on a case-by-case basis for the requirement for an EIA to be undertaken.

4(a).	Do you consider the works to be under the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended)?			Yes ☐	No ☒									
4(a) (i) If Yes, which Annex does the proposal fall under?	     Annex I☐	   Annex II☐

4(a) (ii) Which number(s) within the Annex does the proposal relate to?














4(b).	Have you applied for a screening or scoping opinion from the MLT under the Marine Works (Environmental Impact Assessment) Regulations 2007 (as amended)?  									Yes ☐	No ☒
N/A

4(b) (i). If Yes, please provide the reference number

4(c).	Has an Environmental Impact Assessment been undertaken? 	Yes ☐ No ☒											
4(c)(i).If Yes, has an Environmental Statement been submitted to support this Marine Licence application? 						Yes ☐ No ☐	

4(d).	If an Environmental Impact Assessment has been undertaken, but an ES has not been submitted, please provide an explanation
N/A




Please continue on a separate sheet if necessary. Please tick if you have done this ☐


5. Licensable Period

Determination of applications will be based on the works taking place during these dates. Please ensure you have included an adequate contingency period. If works are not completed by the Requested Licence Expiry Date you may be required to submit a new application. Including a contingency period within your original application does not impact on Licence Fee
31 October 2025
17 June 2024

Start Date				Requested Licence Expiry Date


Please ensure you submit your application for a Marine Licence at least 4 months prior to the intended start date. Some projects, such as EIA projects, will take significantly longer to determine.

6. Project Description

6(a).	Please give a description of the proposed project.
This should include the purpose of the project, estimated timescales of construction and operation, and broken down by the phases of works, if applicable.
Details should include, but not be limited to, dimensions of project, quantity of material being deposited and removed.
Please also refer to answer in section 1(b) above and Contractor’s Method Statement submitted alongside this application. The quantities of materials being deposited and removed are set out in section 8 below. The area of the works is approximately 0.26ha, of which approximately 0.01ha is below Mean High Water Springs.

The Chapel Reen outfall requires repair to continue to function as intended. A collapsed section of the south-west wing wall noted during a June 2018 inspection was subsequently reconstructed with the introduction of a new drainage pipe and flap valve in September 2018. The repaired masonry wing wall failed again in November/ December 2020; the estuarine channel side of the right hand bank had slumped leading to a collapse of the wing wall. An inspection of the failure also highlighted bulging of the masonry wing wall on the channel side on the left hand bank of the estuarine channel, indicating that the same failure mechanism was likely on this bank. Emergency repair works were undertaken in December 2021, comprising of trench boxes, which necessitated relocation of the Farmers Arm pub effluent pipe. The works applied for in this marine licence are the permanent repair works to the Chapel Reen outfall.

Due to the small scale of works the works will not be separated into phases. The estimated timescales of construction are approximately 12 weeks. The scheme is expected to be managed, operated and maintained for a service life of 50 years. 

(continued on next page)

























 The scheme comprises:
· Upgrading the existing tidal flap valves and installation of new mechanical lifting equipment.
· Repairs to the upstream face of the outfall structure consisting of de-vegetation of the wall and masonry works.
· Reinstatement of the effluent pipe from the Farmers Arms pub to its original position, which was relocated as part of the emergency works.
· Replacement of a 12.6m plan length of existing and failed retaining walls on both sides of the outfall with steel sheet piled retaining walls, driven to a footing level of approximately -6.0m Ordnance Datum (Newlyn). This is an approximate pile length of 12m. The sheet piles will be installed behind the existing retaining walls, within the area of profiled ground between the head wall and the channel (therefore no underwater noise anticipated). 
· The temporary works currently located within the channel will be removed, along with the remnants of the failed existing walls and slumped soils. Ground level will be reinstated around the downstream end of the new structure to tie-in with existing levels.
· Installation of steel/reinforced concrete capping beam to the piles.
· Installation of 7.5m long structural steel universal columns to prop the sheet piles. 
· Replacement of a 12.6m plan length of existing masonry channel (invert) bed with a reinforced concrete bed. 

Due to the nature of piling works, there is some uncertainty on the embedment depth that can be reached. The drawings submitted as part of the marine licence application show the assumed worst case scenario on site (Drawing References 4021359-BUK-ZZ-00-DR-C-00002, 4021359-BUK-ZZ-00-DR-C-00001, 4021359-BUK-ZZ-00-DR-C-00010 and 4021359-BUK-ZZ-00-DR-C-00009). This comprises a retained height of approximately 3.5m - 4m and the installation of four 7.5m long structural steel universal columns between 6.5 and 7.5mAOD to prop the sheet piles.  If possible, during the works, the number of steel universal columns and the retained height will be reduced and the surrounding ground reprofiled and reinstated accordingly. The ground profile behind the piles will not exceed a 1 in 2 slope.


Please continue on a separate sheet if necessary. Please tick if you have done this ☐

6(b).	Please detail the location of the proposed construction project.
This should be either Ordnance Survey National Grid Reference (i.e. AB 12345 67890) or Latitude and Longitude in decimal degrees to 4 decimal places (i.e. Lat 52.1234 Long -4.1234), defining the extent of the project. Please specify which coordinate system has been used.
Latitude and longitude for the corners of the site:


Latitude 
Longitude
Point 1

51.542374
-2.9141218
Point 2

51.542496
-2.9136997
Point 3

51.542583
-2.9139758
Point 4

51.542471
-2.9142318




















Please continue on a separate sheet if necessary. Please tick if you have done this ☐
6(c).	The following must be provided with the completed application form:

(i) a suitably scaled extract of an Ordnance Survey Map or Admiralty Chart with location of project, complete with North Arrow and Scale

(ii) construction plans and sectional drawings showing those proposed works below/seaward of MHWS, which should give details of the materials to be used (for beach replenishment the quantity, particle size and source of material to be deposited and deposit location is also required).

(iii) a descriptive schematic drawing and suitably scaled location plan which show the full extent of the project clearly in relation to the surrounding area and features.

Please list below all supporting documents that have been submitted with this application, including suitable documents/maps/drawing titles and reference numbers
[bookmark: _Hlk155873583]Site plan: 4021359-BUK-ZZ-00-DR-C-00002
General arrangement: 4021359-BUK-ZZ-00-DR-C-00001
Typical cross sections: 4021359-BUK-ZZ-00-DR-C-00010
Elevations: 4021359-BUK-ZZ-00-DR-C-00009
Pipe easement plan (Farmer’s Arm effluent pipe): 4021359-BUK-ZZ-00-DR-C-00006
Contractor’s Method Statements: A9179-RAMS-01
WFD Compliance Assessment (Screening): 4021359-BUK-ZZ-00-RP-EN-00006
WFD Compliance Assessment (Scoping): Chapel Reen – WFD Assessment – Scoping – V2
Ecology Report: 4021359-BUK-ZZ-00-RP-EN-00001 
Welsh National Marine Plan Signposting Document: 4021359-BUK-ZZ-00-RP-EN-00003
Habitats Regulation Assessment: 4021359-BUK-ZZ-00-RP-EN-00004
Environmental Action Plan (EAP): Chapel Reen EAP – V2




















Please continue on a separate sheet if necessary. Please tick if you have done this ☐

The applicant should note that these drawings/plans may be copied to others as part of the MLT's consultation procedures. If they are subject to copyright, it is the responsibility of the applicant to obtain the necessary approvals to reproduce the documents and to submit up to 16 copies with the application.

7. Methods Statement

7(a).	Please provide a detailed method statement for the works
This must include methods for all works including temporary structures or deposits such as jetties, cofferdams, moorings or landing stages to be constructed seaward of MHWS
Refer to attached document, A9179 Chapel Reen Method Statement V2 (A9179-RAMS-01).












Please continue on a separate sheet if necessary. Please tick if you have done this ☐

7(b). Do you intend to undertake activities that could generate underwater noise?
This include piling, use of explosives, geophysical, acoustic deterrent devices and multibeam echosounders. 								Yes ☐ No ☒

7(b) (i). If Yes, what type(s) of activities will be undertaken?
N/A









7(b) (ii). If Yes, approximately how many days will the activity be undertaken for?  
N/A












If Yes, you will be required to complete an additional form that will be provided.

7(c).	Please state the measures to be taken to:
(i) Minimise risk to the marine environment 
Measures to minimise risks to the marine environment are set out within the Environmental Action Plan submitted as part of this application.













(ii) Prevent undue interference to others 
A Public Right of way, Part of the Wales Coast Path, runs parallel to the west of the watercourse. No other parts of the site are publicly accessible or in the ownership of other bodies. Measures to avoid and reduce interference to the Wales Coast Path are provided within the Contractors Method Statement (A9179-RAMS-01). A Public Right of way diversion will be agreed with the Local Authority prior to commencement of the works.














(iii) Maintain navigational safety, including marking and lighting of works
The watercourse that will be impacted by the works is not navigable by watercraft, therefore there will be no impact to navigational safety.














Please continue on a separate sheet if necessary. Please tick if you have done this ☐

8. Materials of Project 

8(a).	Description of materials to be deposited seaward of MHWS (Please tick all that apply)
Timber	☐	Iron/Steel	☒	Concrete	☒	Biocides/other chemicals	☐
Silt		☐	Stone/Rock	☐	Gravel		☒	Plastic/Synthetics		☐ 
Sand	☐	Other		☐	

If other, please provide a description of materials.
N/A











8(b).	Delivery method of materials to site
If sea delivery, please include details of vessels to be used with a chart of proposed route and transhipment area. If vehicle delivery, please provide the proposed access route. 
Materials will be delivered on land by vehicle. The access route proposed is set out within the Contractors Method Statement (A9179-RAMS-01).










Please continue on a separate sheet if necessary. Please tick if you have done this ☐

8(c).	Will the works involve removals seaward of MHWS?		Yes ☒ No ☐

8(c) (i). Description of materials to be removed seaward of MHWS (Please tick all that apply)
Timber	☐	Iron/Steel	☒	Concrete	☐	Biocides/other chemicals	☐
Silt		☒	Stone/Rock	☐	Gravel		☒	Plastic/Synthetics		☒ 
Sand	☐	Other		☐	
8(c) (ii). Description of objects/materials to be removed seaward of MHWS
Including quantities to be removed.
· Iron/Steel to be removed is the trench boxes from the temporary works, the quantity of metal is approximately 1.6m3.
· Silt to be removed includes material present on the existing masonry bed. Quantity to be removed is approximately 110m3.
· Stone/Rock to be removed includes the masonry from the failed retaining wall. Quantity to be removed is approximately 42m3.
· Gravel backfill from the emergency works, behind the trench boxes, to be removed is approximately 50m3.
· Plastic bulk bags used in the emergency works behind the trench boxes will also be removed.

[bookmark: _Hlk160024056]It is noted that the measurements set out above were calculated using a MHWS level of 6.3mAOD. The stated volumes are estimates based on limited reprofiling and reinstatement to tie-in around the new structure. There may be an opportunity to reduce the visual impact of engineered structures by reducing the surrounding ground levels, lowering a section of the retaining wall and reprofiling accordingly. This may result in some change in the precise volume of excavated materials below MHWS during construction.


















9. Beach Replenishment, Land Reclamation or Salt Marsh Feeding

For works involving any of the above, please provide the following information 

9(a). Is the material to be deposited like for like to existing material? 	Yes ☐ No ☐

9(a)(i) If No for Beach Replenishment please provide justification why?N/A












9(b).	Description of material to be deposited
Please provide the grading specification of materials to be used, if using a range of grain sizes please state the percentage by weight passing. If unsure, please refer to the Wentworth Scale 
N/A








Please continue on a separate sheet if necessary. Please tick if you have done this ☐

9(c).	Source of the material to be deposited
Including dredged or land based stating the origin of material

N/A












9(d).	Has the material been chemically analysed? 			Yes ☐ No ☐
If material has been analysed, we may request this information to determine the application

9(d) (i) If Yes, is the analysis data been included with the application? Yes ☐ No ☐

10. Temporary Works

10(a).	Will there be any temporary deposits below MHWS? 		Yes ☒ No ☐
This includes construction materials, removed objects/material, jetties or cofferdams
If Yes, please continue with section 10

10(b).	Please provide the location of temporary deposits 
Please include a map/chart displaying the location of temporary deposits, if necessary.
All temporary deposits will be within the site boundary as set out on the site plan, drawing 4021359-BUK-ZZ-00-DR-C-00002. Sections 15 of the Contractor’s Method Statement (A9179-RAMS-01) provides further detail on the location of temporary deposits. 
















10(c).	Description of temporary deposits
Temporary deposits below Mean High Water Springs are anticipated to comprise:
· Overpumping set up
· Extender pipes to temporarily extend the existing culverts
· A piling pad formed from rockbags and imported clean stone or stockpiled material
· A temporary dam, likely to take the form of a frame dam (see the Contractor’s Method Statement)














Please continue on a separate sheet if necessary. Please tick if you have done this ☐

11. Dredge and Disposal of Dredge Material
If you are undertaking Dredge and Disposal activities please also complete the Dredge and Disposal application form and submit together.

11(a).	Do you intend to apply for a marine licence to dispose of dredged material to sea as part of the works in this application? 			Yes ☐ No ☒

12. Protected Sites

Licensing Authorities have a duty to ensure that projects will not have significant adverse environmental impact, particularly on any designated European Site of Conservation Importance - Special Areas of Conservation (SAC) and Special Protection Areas (SPA), listed under the Habitats Directive (Council Directive 92/42/EEC on the conservation of natural habitats and of wild fauna and flora). In addition, it is Government Policy that Wetlands of International Importance (Ramsar sites) are also considered as European Sites. There is a duty to take reasonable steps to further the conservation and enhancement of nationally designated sites (Sites of Special Scientific Interest (SSSIs)).

12(a).	Have you had pre-application correspondence with NRW, its legacy bodies or Natural England? 								Yes ☒ No ☐


12(a)(i). If Yes, please provide copies of correspondence with application and state which team(s) you have contacted? 
Consultation was undertaken with:
Richard Sheppard - Angling Developments and Technical Support Officer. 
Stuart Craxford – Operations Environmental Assessment Officer
Geomorphology South - Josh Macmillan - Advisor, Geomorphology
All correspondence is submitted within appendix A of the WFD Assessment – Scoping – V2. 









12(b).	Are any part of the works located within or likely to affect a designated conservation site? (SAC, SPA, SSSI or Ramsar)			 Yes ☒ No ☐

12(b)(i). If Yes, which designated site(s) may be affected?
Severn Estuary Ramsar, Special Area of Conservation, Special Protection Area and Site of Special Scientific Interest (SSSI)
Newport Wetlands National Nature Reserve and SSSI
Gwent Levels – Nash and Goldcliff SSSI













12(c).	Please provide a description of all mitigation measures proposed to avoid any impact on designated conservation sites.
Refer to the Environmental Action Plan.















Please continue on a separate sheet if necessary. Please tick if you have done this ☐

12(d).	If the works are not located within or likely to affect a designated conservation site, please indicated the approximate distance to the nearest designated conservation site.
N/A











Please note that if the proposed works are in or within 2km of a European Site of Conservation Importance you will have to provide suitable mitigation measure to avoid any impact on designated conservation sites.

13. Other Consents

Please detail all consents that you have applied for or received for these works

	Type of Consent
	Applied for
	To be applied for
	Reference Number
	Date of Issue and Expiry

	Planning Permission under Town and County Planning Act 1990 – From Local Planning Authority (LPA)

	N/A
	
	
	

	Name and Address of LPA for location of works

	Note the applicant has permitted development rights for the terrestrial elements of the works, this has been confirmed by the local planning authority (Newport County Council) on 20/02/2024.

	Land Owners Consent such as The Crown Estate Consent

	N/A
	
	
	

	Port Authority or Local Harbour permissions

	N/A
	
	
	

	Other NRW consents such as Flood Defence or SSSI assent
	
	Yes (temporary works FRAP and SSSI Assent)
	
	

	Details of NRW consent

	SSSI Assent to be applied for regarding the three SSSIs interfacing with the scheme.

A FRAP for the temporary works will be applied for by the contractor once available.

	Other consents such as Transport and Works Act Order, Section 36 Electricity Act, grant/loan sanction
	N/A
	
	
	

	Details of other consents 


	



14. Statutory Powers

14(a).Does the applicant have statutory powers to consent any aspect of the project? 
E.g. coast protection authority, dredging powers, statutory undertakers	Yes ☒ No ☐

14(a)(i).If Yes, please give details and state the relevant legislation that gives these powers
NRW benefits from various permitted development rights. Schedule 2, Part 15, Class A of the Town and Country Planning (General Permitted Development) Order 1995 (as amended) grants planning permission for development by NRW for the purpose of their functions, consisting of:
b) development in, on or under any watercourse or land drainage works and required in connection with the improvement, maintenance or repair of that watercourse or those works.






There are no exclusions or conditions associated with the permitted development Class A(b) described above.

Given that the proposed works described will be undertaken within the Chapel Reen watercourse, the works fall within permitted development Part 15, Class A(b). These rights apply to the elements of the works above mean high water springs.

NRW will follow the requirements under the Environmental Impact Assessment (Land Drainage Improvement Works) Regulations 1999 (as amended) for the proposed works.







15. Public Register

Under The Marine Licensing (Register of Licensing Information) (Wales) Regulations 2011 and the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended), all information contained within or provided in support of this application will be placed on the Public Register unless NRW approve of the applicant’s reasons for withholding all or part.	

15.	Is there any information contained within or provided in support of this application that you consider should NOT be included on the Public Register on the grounds that its disclosure:

15(a).	Would be contrary to the interest of National Security? 		Yes ☐ No ☒

15(b).	Would prejudice to an unreasonable degree you, or some other person’s commercial interest of those of a third party? 			Yes ☐ No ☒

If Yes to either (a) or (b), please provide full justification as to why all or part of the information you have provided should be withheld

N/A












Please continue on a separate sheet if necessary. Please tick if you have done this ☐

16. Application Fee

16(a). What are the corresponding fee band for this application? Band 2 ☒ Band 3 ☐

16(b) Band 2 Only
Projects are charged at a fixed fee of £1920. The application will not be processed until the correct fee has been provided.

Please provide the method of payment 

Applicant is Natural Resources Wales therefore no fee to be charged. 

	Method
	Yes (√)
	Reference Number

	Cheque
	
	

	BACS (not remittance no.)
	


	

	World Pay (phone or CC1)
	

	


Please attach CC1 Form with application. Can be found on our web pages

16(c) Band 3 Application only
Band 3 applications are charged at on hourly rate of £120 and are invoiced in arrears. Please complete the details below which will be required for invoicing.


Customer Name




FAO



Purchase order number



Address for invoice





Telephone Number





Email Address




17. Declaration

I declare that to the best of my knowledge and belief that the information given in this application form and supporting documentation is true.

	WARNING: It is an offence under the Marine and Coastal Access Act 2009, under which this application is made, to fail to disclose information or to provide false or misleading information and can invalidate any licence granted.



[image: ]
Signature	                                          				            05/03/2024



Name (in capitals)	DAVID JENKINS

Position in Company	 Project Manager 							
	


Applications cannot be processed unless signed by the Applicant (not agent), the applicant must have appropriate level of authority within the company.

Applications will not be processed unless signed
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