



Permit Number: 	AB3591ZQ						Operator: 		Maelor Foods Limited 

Facility:		Maelor Poultry Processing	Plant			Form Number: 	Water1 / 16/07/24
Reporting of emissions to water (other than to sewer) for the period from                         to      
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value [1]
	Reference Period
	Result [2]
	Test
Method [3] 
	Sample
Date and Times [4]
	Uncertainty
[5]

	W1
	Flow/volume
	1,500 m3 per day
	Daily
	
	MCERTS
	
	

	W1
	Flow/volume
	1,200 m3 per day
	Per annum (mean daily volume)
	
	MCERTS
	
	

	W1
	Temperature
	30OC
	Continuous
	 
	Standard Temperature sensor
	
	

	W1
	Total suspended solids
	30 mg/l
	24-hour flow proportional sample
	
	BS EN 872
	
	

	W1
	Ammonia 
	5 mg/l
	24-hour flow proportional sample
	
	BS EN 11732:2005
	
	

	W1
	Phosphate
	2.5 mg/l
	24-hour flow proportional sample
	
	BS EN ISO 15681-1:2004
	
	

	W1
	pH
	6-9
	Continuous
	
	MCERTS
	
	

	W1
	BOD
	20 mg/l
	24-hour flow proportional sample
	
	BS EN 1899-1 (1998)
	
	



[1] Emission Limit Values as set out in Table S3.2a within the Permit (Phase 1 Operations).
[2] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[3] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[4] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given. 
[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.  

Signed …………………………………………………………….  		Date………………………..
	(Authorised to sign as representative of Operator)
Permit Number: 	AB3591ZQ						Operator: 		Maelor Foods Limited 

Facility:		Maelor Poultry Processing	Plant			Form Number: 	Water1 / 16/07/24
Reporting of emissions to water (other than to sewer) for the period from                         to      
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value [1]
	Reference Period
	Result [2]
	Test
Method [3] 
	Sample
Date and Times [4]
	Uncertainty
[5]

	W1
	Flow/volume
	3,120m3 per day
	Daily
	
	MCERTS
	
	

	W1
	Flow/volume
	2,400m3 per day 
	Per annum (mean daily volume)
	
	MCERTS
	
	

	W1
	Temperature
	30OC
	Continuous
	
	Standard Temperature sensor
	
	

	W1
	Total suspended solids
	15 mg/l
	24-hour flow proportional sample
	
	BS EN 872
	
	

	W1
	Ammonia 
	2 mg/l
	24-hour flow proportional sample
	
	BS EN 11732:2005
	
	

	W1
	Phosphate
	1 mg/l
	24-hour flow proportional sample
	
	BS EN ISO 15681-1:2004
	
	

	W1
	pH
	6-9
	Continuous
	
	MCERTS
	
	

	W1
	BOD
	10 mg/l
	24-hour flow proportional sample
	
	BS EN 1899-1 (1998)
	
	



[1] Emission Limit Values as set out in Table S3.2b within the Permit (Phase 2 Operations).
[2] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[3] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[4] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given. 
[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.  

Signed …………………………………………………………….  		Date………………………..
	(Authorised to sign as representative of Operator)

 
Permit Number: 	AB3591ZQ					Operator: 		Maelor Foods Limited 

Facility:		Maelor Poultry Processing	Plant		Form Number: 	WaterUsage1 / 29/08/17

Reporting of Water Usage for the year:

	Water Source
	Specific Usage 
(litres/bird)
	

	
	
	

	
	
	

	Mains water
	
	

	Site borehole
	
	

	Other
	
	

	
	
	

	
	
	

	TOTAL WATER USAGE
	
	



	Operator’s comments :







Signed …………………………………………………………….  		Date………………………..   	
	(authorised to sign as representative of Operator)

Permit Number: 	AB3591ZQ					Operator: 		Maelor Foods Limited 

Facility:		Maelor Poultry Processing	Plant		Form Number: 	Energy1 / 29/08/17

Reporting of Energy Usage for the year:

	
Energy Source
	Energy Usage	
	

	
	
Quantity
	Specific Usage
(KWh/bird)
	

	
	
	
	

	
	
	
	

	
	
	
	

	Electricity *
	
	
	

	Natural Gas
	
	
	

	Gas Oil
	
	
	

	Recovered Fuel Oil
	
	
	

	
	
	
	

	TOTAL
	
	
	

	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments :









Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number: 	AB3591ZQ					Operator: 		Maelor Foods Limited 

Facility:		Maelor Poultry Processing	Plant		Form Number: 	Performance1 / 29/08/17

Reporting of other performance indicators for the period                                      to 

	Parameter
	
	Units 
	Result

	
	
	
	

	Number of chickens slaughtered per week
	Number per week (maximum week in reporting year)
	

	Chicken Products produced per week
	Tonnes per week (maximum week in reporting year)
	

	
	
	

	
	
	

	
	
	

	
	
	



	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)
