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Permit with introductory note

The Environmental Permitting (England & Wales) Regulations 2016
Morgan Sindall Construction & Infrastructure Ltd
Dewatering Activities from Points DC1 to DC14 serving Dinorwig Heritage Railway (400kV buried electricity cable replacement scheme)
Gilfach Ddu,

Llanberis, 

Caernarfon, 

Gwynedd, 

LL55 4TY
Permit number

EPR/DB3491FM
Dewatering Activities at Dinorwig Heritage Railway (400kV buried electricity cable replacement scheme)
Permit Number EPR/DB3491FM
Introductory note

This introductory note does not form a part of the permit

The main features of the permit are as follows. 
The permit is to regulate the discharge of site drainage resulting from rainfall and groundwater intrusion into working trenches. Limits are set to control the discharge rate, suspended solid concentration and pH.
Morgan Sindall, on behalf of National Grid, are installing a replacement underground electricity cable to connect the hydroelectric power station at Llanberis to the national grid. In total 14 discharge locations will be required along the Dinorwig Heritage Railway cable replacement route.
Prior to final discharge the dewatered discharge will be passed through a filtration sock to trap sand and silt particles to prevent it entering the surface water drainage system. The works are estimated to take 12 months, there should only be discharges from two locations at any one time.
The status log of the permit sets out the permitting history, including any changes to the permit reference number.
	Status log of the permit

	Description
	Date
	Comments

	Application PAN-027133
	Duly made 05/11/2024
	Application for discharge of trade effluent consisting of site drainage.

	Permit determined
	10/02/2024
	Permit issued to Morgan Sindall Construction & Infrastructure Ltd


End of introductory note

	Permit


The Environmental Permitting (England and Wales) Regulations 2016
Permit number 

EPR/DB3491FM
The Natural Resources Body for Wales (“Natural Resources Wales”) authorises, under regulation 13 of the Environmental Permitting (England and Wales) Regulations 2016 
Morgan Sindall Construction & Infrastructure Ltd  (“the operator”),

whose registered office is

Kent House

14 – 17 Market Place

London

W1W 8AJ

company registration number 04273754
to operate a water discharge activity at

Points DC1 to DC14 
Dinorwig Heritage Railway 

(400kV buried electricity cable replacement scheme)
Gilfach Ddu,

Llanberis, 

Caernarfon, 

Gwynedd, 

LL55 4TY 

to the extent authorised by and subject to the conditions of this permit.

	Name
	Date

	Joanne Fitton
	10/02/2025


Authorised on behalf of Natural Resources Wales
Conditions 

1 Management
1.1 General management

1.1.1 The operator shall manage and operate the activities:

(a) in accordance with a written management system that identifies and minimises risks of pollution, including those arising from operations, maintenance, accidents, incidents, non-conformances and those drawn to the attention of the operator as a result of complaints; and

(b) using sufficient competent persons and resources.
1.1.2 Records demonstrating compliance with condition 1.1.1 shall be maintained. 

1.1.3 Any person having duties that are or may be affected by the matters set out in this permit shall have convenient access to a copy of it kept at or near the place where those duties are carried out.

2
Operations
2.1
Permitted activities

2.1.1
The operator is only authorised to carry out the activities specified in schedule 1 table S1.1 (the “activities”). 

2.2
The site 

2.2.1
The activities shall not extend beyond the site, being the land shown edged in green and the discharges shall be made at the points marked on the site plan at schedule 7 to this permit and as listed in table S3.2 (discharge points). 

2.3
Operating techniques

2.3.1
(a)
The activities shall, subject to the conditions of this permit, be operated using the techniques and in the manner described in the documentation specified in schedule 1, table S1.2, unless otherwise agreed in writing by Natural Resources Wales.


(b)
If notified by Natural Resources Wales that the activities are giving rise to pollution, the operator shall submit to Natural Resources Wales for approval within the period specified, a revision of any plan or other documentation (“plan”) specified in schedule 1, table S1.2 or otherwise required under this permit which identifies and minimises the risks of pollution relevant to that plan, and shall implement the approved revised plan in place of the original from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.

2.5
Pre-operational conditions

2.5.1
The activities shall not be brought into operation until 01/12/2025
3
Emissions and monitoring
3.1
Emissions to water

3.1.1
There shall be no point source emissions to water except from the sources and emission points listed in schedule 3.

3.1.2
The limits given in schedule 3 shall not be exceeded.

3.2 Emissions of substances not controlled by emission limits

3.2.1 Emissions of substances not controlled by emission limits (excluding odour) shall not cause pollution. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved emissions management plan, have been taken to prevent or where that is not practicable, to minimise, those emissions.

3.2.3
All liquids in containers, whose emission to water or land could cause pollution, shall be provided with secondary containment, unless the operator has used other appropriate measures to prevent or where that is not practicable, to minimise, leakage and spillage from the primary container.

3.3
Monitoring 

3.3.1
Permanent means of access shall be provided to enable sampling/monitoring to be carried out in relation to the emission points specified in schedule 3 tables S3.1, S3.2 and S3.3 unless otherwise agreed in writing by Natural Resources Wales.

4
Information

4.1
Records
4.1.1 All records required to be made by this permit shall:

(a) be legible;

(b) be made as soon as reasonably practicable;

(c) if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and

(d) be retained, unless otherwise agreed in writing by Natural Resources Wales, for at least 6 years from the date when the records were made.
4.1.2
The operator shall keep on site all records, plans and the management system required to be maintained by this permit, unless otherwise agreed in writing by Natural Resources Wales. 

4.2
Reporting
4.2.1
The operator shall send all reports and notifications required by the permit to Natural Resources Wales using the contact details supplied in writing by Natural Resources Wales.

4.3
Notifications
4.3.1
Natural Resources Wales shall be notified without delay following the detection of:

(a) any malfunction, breakdown or failure of equipment or techniques, accident, or  emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution;

(b) the breach of a limit specified in the permit; or 

(c) any significant adverse environmental effects.  

4.3.2
Any information provided under condition 4.3.1 shall be confirmed by sending the information listed in schedule 5 to this permit within the time period specified in that schedule.
4.3.3
Where Natural Resources Wales has requested in writing that it shall be notified when the operator is to undertake monitoring and/or spot sampling, the operator shall inform Natural Resources Wales when the relevant monitoring and/or spot sampling is to take place. The operator shall provide this information to Natural Resources Wales at least 14 days before the date the monitoring is to be undertaken.

4.3.4
Natural Resources Wales shall be notified within 14 days of the occurrence of the following matters, except where such disclosure is prohibited by Stock Exchange rules: 

Where the operator is a registered company:
(a) any change in the operator’s trading name, registered name or registered office address; and

(b)
any steps taken with a view to the operator going into administration, entering into a company voluntary arrangement or being wound up.

Where the operator is a corporate body other than a registered company:
(a) any change in the operator’s name or address; and

(b) any steps taken with a view to the dissolution of the operator.

4.3.5
Where the operator proposes to make a change in the nature or functioning, or an extension of the activities, which may have consequences for the environment and the change is not otherwise the subject of an application for approval under the Regulations or this permit:

(a)
Natural Resources Wales shall be notified at least 14 days before making the change; and


(b)
the notification shall contain a description of the proposed change in operation. 

4.4
Interpretation
4.4.1
In this permit the expressions listed in schedule 6 shall have the meaning given in that schedule.

4.4.2
In this permit references to reports and notifications mean written reports and notifications, except where reference is made to notification being made “without delay”, in which case it may be provided by telephone. 

Schedule 1 - Operations 

	Table S1.1 Activities

	Activity reference
	Description of activity
	Limits of specified activity

	A1
	Discharge of trade effluent consisting of  site drainage via DC1
	There should only be discharges from two locations at anyone time.

	A2
	Discharge of trade effluent consisting of  site drainage via DC2
	

	A3
	Discharge of trade effluent consisting of  site drainage via DC3
	

	A4
	Discharge of trade effluent consisting of  site drainage via DC4
	

	A5
	Discharge of trade effluent consisting of  site drainage via DC5
	

	A6
	Discharge of trade effluent consisting of  site drainage via DC6
	

	A7
	Discharge of trade effluent consisting of  site drainage via DC7
	

	A8
	Discharge of trade effluent consisting of  site drainage via DC8
	

	A9
	Discharge of trade effluent consisting of  site drainage via DC9
	

	A10
	Discharge of trade effluent consisting of  site drainage via DC10
	

	A11
	Discharge of trade effluent consisting of  site drainage via DC11
	

	A12
	Discharge of trade effluent consisting of  site drainage via DC12
	

	A13
	Discharge of trade effluent consisting of  site drainage via DC13
	

	A14
	Discharge of trade effluent consisting of  site drainage via DC14
	


	Table S1.2 Operating techniques

	Activity reference
	Description of documentation
	Parts
	Date Received

	A1
	PAN-027133 ERA & Management Plan 

PAN-027133 – Non Technical Summary 


	All Parts

All Parts
	07/10/2024

	A2
	
	
	

	A3
	
	
	

	A4
	
	
	

	A5
	
	
	

	A6
	
	
	

	A7
	
	
	

	A8
	
	
	

	A9
	
	
	

	A10
	
	
	

	A11
	
	
	

	A12
	
	
	

	A13
	
	
	

	A14
	
	
	


Schedule 2 - Waste types, raw materials and fuels

Wastes are not accepted as part of the permitted activities and there are no restrictions on raw materials or fuels under this schedule.

Schedule 3 – Emissions and monitoring

	Table S3.1 Point Source emissions to water (other than sewer) – emission limits and monitoring requirements

	Discharge source and discharge point ref. & location
	Parameter  
	Limit (including unit)
	Reference Period
	Limit of effective range
	Monitoring frequency
	Compliance Statistic

	A1 to A14 - Trade effluent consisting of site drainage via DC1 to DC14
	Maximum rate of discharge
	5.8  litres per second
	Instantaneous (spot sample)
	N/A
	N/A
	Maximum

	
	Suspended solids (measured after drying at 105o C)
	50 mg/l
	Instantaneous (spot sample)
	N/A
	N/A
	Maximum 

	
	pH
	6 to 9
	Instantaneous (spot sample)
	N/A
	N/A
	Minimum and maximum

	
	Visible oil or grease
	No significant trace present
	Instantaneous (spot sample)
	N/A
	N/A
	No significant trace


	Table S3.2 Discharge points

	Effluent Name
	Discharge Point
	Discharge point NGR
	Receiving water/Environment



	A1 - Trade effluent consisting of site drainage  
	DC1
	SH 58605 60387
	Existing surface drainage system which discharges to Llyn Padarn

	A2 - Trade effluent consisting of site drainage  
	DC2
	SH 58438 60575
	Existing surface drainage system which discharges to Llyn Padarn

	A3 - Trade effluent consisting of site drainage  
	DC3
	SH 58152 60757
	Existing surface drainage system which discharges to Llyn Padarn

	A4 - Trade effluent consisting of site drainage  
	DC4
	SH 57929 60893
	Existing surface drainage system which discharges to Llyn Padarn

	A5 - Trade effluent consisting of site drainage  
	DC5
	SH 57790 61141
	Existing surface drainage system which discharges to Llyn Padarn

	A6 - Trade effluent consisting of site drainage  
	DC6
	SH 57707 61277
	Existing surface drainage system which discharges to Llyn Padarn

	A7 - Trade effluent consisting of site drainage  
	DC7
	SH 57473 61401
	Existing surface drainage system which discharges to Llyn Padarn

	A8 - Trade effluent consisting of site drainage  
	DC8
	SH 57256 61512
	Existing surface drainage system which discharges to Llyn Padarn

	A9 - Trade effluent consisting of site drainage  
	DC9
	SH 57055 61601
	Existing surface drainage system which discharges to Llyn Padarn

	A10 - Trade effluent consisting of site drainage  
	DC10
	SH 56802 61773
	Existing surface drainage system which discharges to Llyn Padarn

	A11 - Trade effluent consisting of site drainage  
	DC11
	SH 56589 61972
	Existing surface drainage system which discharges to Llyn Padarn

	A12 - Trade effluent consisting of site drainage  
	DC12
	SH 56341 62132
	Existing surface drainage system which discharges to Llyn Padarn

	A13 - Trade effluent consisting of site drainage  
	DC13
	SH 56110 62319
	Existing surface drainage system which discharges to Llyn Padarn

	A14 - Trade effluent consisting of site drainage  
	DC14
	SH 55883 62572
	Existing surface drainage system which discharges to Llyn Padarn


	Table S3.3 Monitoring points

	Effluent(s) and discharge point(s)
	Monitoring type
	Monitoring point NGR
	Monitoring point reference

	A1 - Trade effluent consisting of site drainage Via DC1
	Effluent sampling
	SH 58605 60387
	DC1

	A2 - Trade effluent consisting of site drainage Via DC2
	Effluent sampling
	SH 58438 60575
	DC2

	A3 - Trade effluent consisting of site drainage Via DC3
	Effluent sampling
	SH 58152 60757
	DC3

	A4 - Trade effluent consisting of site drainage Via DC4
	Effluent sampling
	SH 57929 60893
	DC4

	A5 - Trade effluent consisting of site drainage Via DC5
	Effluent sampling
	SH 57790 61141
	DC5

	A6 - Trade effluent consisting of site drainage Via DC6
	Effluent sampling
	SH 57707 61277
	DC6

	A7 - Trade effluent consisting of site drainage Via DC7
	Effluent sampling
	SH 57473 61401
	DC7

	A8 - Trade effluent consisting of site drainage Via DC8
	Effluent sampling
	SH 57256 61512
	DC8

	A9 - Trade effluent consisting of site drainage Via DC9
	Effluent sampling
	SH 57055 61601
	DC9

	A10 - Trade effluent consisting of site drainage Via DC10
	Effluent sampling
	SH 56802 61773
	DC10

	A11 - Trade effluent consisting of site drainage Via DC11
	Effluent sampling
	SH 56589 61972
	DC11

	A12 - Trade effluent consisting of site drainage Via DC12
	Effluent sampling
	SH 56341 62132
	DC12

	A13 - Trade effluent consisting of site drainage Via DC13
	Effluent sampling
	SH 56110 62319
	DC13

	A14 - Trade effluent consisting of site drainage Via DC14
	Effluent sampling
	SH 55883 62572
	DC14


Schedule 4 – Reporting

There is no reporting under this schedule.

Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part A 
	Permit Number
	EPR/DB3491FM

	Name of operator
	

	Location of Facility
	Dinorwig Heritage Railway (400kV buried electricity cable replacement scheme) Gilfach Ddu Llanberis, Caernarfon, Gwynedd, LL55 4TY

	Time and date of the detection 
	


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of  release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	


	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	


	Name*
	

	Post
	

	Signature
	

	Date
	


* authorised to sign on behalf of the operator
Schedule 6 - Interpretation 

“accident” means an accident that may result in pollution.

“annually” means once every year.
“application” means the application for this permit, together with any additional information supplied by the operator as part of the application and any response to a notice served under Schedule 5 to the EP Regulations.

“emissions of substances not controlled by emission limits” means emissions of substances to air, water or land from the activities, which are not controlled by an emission or background concentration limit.
“EP Regulations” means The Environmental Permitting (England and Wales) Regulations SI 2016 No.1154 and words and expressions used in this permit which are also used in the Regulations have the same meanings as in those Regulations.

“groundwater” means all water, which is below the surface of the ground in the saturation zone and in direct contact with the ground or subsoil.
“Natural Resources Wales” means the Natural Resources Body for Wales established by article 3 of the Natural Resources Body for Wales (Establishment) Order 2012. The Natural Resources Body for Wales (Functions) Order 2013 transferred the relevant functions of the Countryside Council for Wales, and functions of the Environment Agency and the Forestry Commission in Wales to the Natural Resources Body for Wales.  
“quarter” means a calendar year quarter commencing on 1 January, 1 April, 1 July or 1 October.

“year” means calendar year ending 31 December.

Schedule 7 - Site plan
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