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APPLICATION FOR A MARINE LICENCE FOR MARINE WORKS

Marine Works include, but are not limited to, coast defences, beneficial uses of dredged materials, subsea cables, pontoons, jetties, land reclamation, grab samples and outfall pipes under the Marine and Coastal Access Act 2009

Please read the notes carefully before completing the form.
The Marine Licensing Team (MLT) administers Part 4 of the Marine and Coastal Access Act 2009 on behalf of the Licensing Authority, the Welsh Ministers.

The completed application form must be accompanied by a location plan and, where appropriate, descriptive drawing(s) and any supporting environmental assessments. 

Please submit applications to the Permit Receipt Centre via the details at the top of this form. For applications larger than 20MB, we would advise that you contact us to determine the most appropriate method for submitting your application.
 
Please submit marine licence applications, including this form and all supporting documents, at least 4 months before the licence is required.

Some projects may raise matters that require a significantly longer time for consideration. These are most likely to be:

· Projects that fall within The Marine Works (Environmental Impact Assessment) Regulations 2007 – as amended requiring an Environmental Statement
· Large scale projects with substantial volumes of material being deposited or excavated
· Works requiring an Appropriate Assessment to be conducted under The Conservation of Habitats and Species Regulations 2017.

Information should be provided about the anticipated duration of the entire project in respect of works below/seaward of Mean High Water Spring (MHWS). Where appropriate, planned phasing of the work for which consent is sought must be detailed. For projects lasting more than one calendar year, planned phasing details must be given for each 12 month period.

A licence fee is payable in respect of an application. Details of fees can be found on our web pages.

Please note applications will not be processed without the correct relevant fee or invoicing details.  

Payments can be made via Cheque, BACS or credit/debit card. 
· Cheques should be crossed and made payable to Natural Resources Wales. 
· For BACS payments ensure you provide the reference number (not remittance number)
· For credit/debit card payments please complete the CC1 form and submit with the application. The CC1 form can be found on our web pages

Further information on payment methods can be found on our web pages

All activities need to comply with the Water Framework Directive (WFD). The framework and guidance can be found on the Natural Resources Wales website, http://naturalresources.wales. The results of your WFD assessment must be attached to your marine licence application.

Please answer all questions. If any information is not available at the time of application please indicate in the relevant section, giving reasoning in a covering letter. Outstanding details must be submitted as soon as possible. Any delay in forwarding details is likely to result in delays in determining your application.

Your application may not be considered complete and therefore not processed until key information has been submitted. Your application may be returned if you fail to submit outstanding information within given timescales.
 
Please note any licence may have conditions that must be discharged before works can commence. This will take additional time. 
If you have any queries with regards to completing this application please contact the MLT: marinelicensing@naturalresourceswales.gov.uk

How your application will be processed by the MLT: 

Submit all application to the Permit Receipt Centre via the details at the top of this form.

Checked and acknowledged by the MLT within 21 days of receipt of application and payment 

If the application is complete and no further information is needed at this time, your application will be placed in a work queue to be assigned a permitting officer

If the application is not complete, further information will be request and need to be provided before the application can be considered as complete

Our 4 months service level for determining non-EIA applications will begin from the date the completed application is received (Please note some projects may take significantly longer than 4 months to determine due to their nature)

EIA projects may take significantly longer due to their scale and complexity. Therefore we encourage early engagement with the MLT

Your application and supporting documents will be sent to for an initial consultation period of 28 days (42 days for EIA projects)

For the majority of projects, a public notice must be advertised. Public consultation will be 28 days (49 days for EIA projects). For EIA projects a second public notice will be required. The MLT will advise on how this should be done.

Responses to consultation will be considered and additional information requested at this time, if necessary.

A decision on your Marine Licence Application will be made

All information submitted may be referred to within a licence, therefore all works must be in accordance with this information, unless otherwise agreed with NRW acting on behalf of the Licensing Authority during the determination process.
It is the responsibility of the applicant to obtain any other consents/authorisations that may be required.

Application Form Structure 
1. Project Description and Cost
2. Applicant Details
3. Details of Agent, Contractor, Vehicles and/or Vessels used to carry out works 
4. Environmental Impact Assessment (EIA)
5. Licensable Period
6. Project Description
7. Methods Statement
8. Materials of Project 
9. Beach Replenishment, Land Reclamation or Salt Marsh Feeding
10. Temporary Works
11. Dredge and Disposal of Dredge Material
12. Protected Sites
13. Other Consents
14. Statutory Powers
15. Public Register
16. Application Fee
17. Declaration

Check List
Please ensure that you have included all the necessary information before you submit your application. If any of the below are not completed in the application form, the application is likely to be considered incomplete and may be returned to you

	Item
	Yes (√)

	The applicant is a legal entity?
	Y

	The declaration is signed by the applicant?
	Y

	Is the application fee correct?
	Y

	Are the grid references/coordinates correct?
	Y

	Do the coordinates match map locations?
	Y

	Have all the relevant supporting documents been submitted?
	Y

	Has a clear methodology been provided in the application form?
	Y

	Has Protected sites information been included?
	Y

	Has a Water Framework Directive (WFD) assessment been submitted?
	Y

	Are all the continuation sheets for application questions appended with correct corresponding numbers?
	N/A


	
Should you have any queries regarding you application please contact the MLT via marinelicensing@naturalresourceswales.gov.uk  

1. Project Description and Cost

1 (a).	Project Name
WWT Llanelli Saline Lagoons Restoration Project





1(b).	Please provide a brief description of the proposed project, including location
[bookmark: _Hlk203304168]This project will repair damaged banks, and diversify the depth profile of the saline lagoons at WWT Llanelli Wetland Centre, to protect and increase the the resilience of the lagoons to dry spells in future. The work will restore and enhance the habitat for specialised saline lagoon invertebrates and fish including the critically endangered European Eel, and benefit thousands of migratory waterbirds which visit the lagoons for safe roosting and feeding opportunities. 







1(c).	Please provide an estimated gross cost of the project (Inc. materials and labour) for works that fall below/seaward of Mean High Water Springs (MHWS)
£50,138.00





2. Applicant Details
To whom the licence will be issued. This must be a legal entity such as an individual, registered company/ charity or public body. 



Title				Full Name

Company or Trading
NameThe Wildfowl and Wetlands Trust

Registered Charity No. 1030884


Company Registration
Number (if applicable)
Brian Briggs	

Name of Contact or 
individual (if different)
WWT Llanelli Reserve Manager

Position in Company

WWT Llanelli Wetland Centre
Penclacwydd
Llwynhendy
Llanelli
SA14 9SH


Address inc. postcode
(provide registered
Company address if
applicable)


Telephone Number01554 741087


Brian.briggs@wwt.org.uk


Email Address
3. Details of Agent, Contractor, Vehicles and/or Vessels used to carry out works 

3(a).	Agent Details 
This is who we will correspond with unless otherwise informed. If no agent we will contact the applicant.



Title				Full Name

Company or Trading
Name



Company Registration
Number (if applicable)


Name of Contact or 
individual (if different)

Position in Company




Address 
(Inc. postcode)






Telephone Number



Email Address

3(b).	Does the Applicant wish to be included in all correspondence? Yes ☒	No ☐

3(c).	Contractor Details
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Contractor Company or Trading Name
	Address

	
TJK Harries 

	TJK GM HARRIES & SON
LLETTYRDRYW FARM 
FELINFOEL
LLANELLI, CARMS SA14 8NX 

	


	



	


	



3(d).	Will the works require the use of vessels?				Yes ☐	No ☒

3(d) (i).Vessel Details (if applicable and available)
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Operator
	Name of Vessel
	Type of Vessel
	Vessel Registration Number
	Country of Registration

	

	
	
	
	

	

	
	
	
	

	

	
	
	
	

	

	
	
	
	




3(e).	Will the works require the use of vehicle?				Yes ☒	No ☐

3(e) (i). Vehicle Details (if applicable and available) to be used below MHWS
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Operator 
	Type/Description of Vehicle

	Iwan Harries (TJK HARRIES & SON)
	13 tonne tracked excavator 

	Iwan Harries (TJK HARRIES & SON)
	Tracked dumper truck

	

	

	

	




3(f).	If the contractor or vessels or vehicles are not known at the application stage, when do you expect to provide these details?
These details will need to be confirmed prior to the licence and operations commencement










4. Environmental Impact Assessment (EIA)
Certain projects, due to their scale, location and/or nature, may require an EIA under the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended). If a project qualifies under EIA, an Environmental Statement (ES) must be prepared and submitted with the application.

Projects that fall within Annex I of the Directive automatically require an EIA. Projects that fall within Annex II of the Directive are assessed on a case-by-case basis for the requirement for an EIA to be undertaken.

4(a).	Do you consider the works to be under the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended)?				Yes ☐	No ☒									
4(a) (i) If Yes, which Annex does the proposal fall under?	     Annex I☐	   Annex II☐

4(a) (ii) Which number(s) within the Annex does the proposal relate to?






4(b).	Have you applied for a screening or scoping opinion from the MLT under the Marine Works (Environmental Impact Assessment) Regulations 2007 (as amended)?  									Yes ☐	No ☒


4(b) (i). If Yes, please provide the reference number

4(c).	Has an Environmental Impact Assessment been undertaken? 	Yes ☐ No ☒											
4(c)(i).If Yes, has an Environmental Statement been submitted to support this Marine Licence application? 						Yes ☐ No ☐	

4(d).	If an Environmental Impact Assessment has been undertaken, but an ES has not been submitted, please provide an explanation







Please continue on a separate sheet if necessary. Please tick if you have done this ☐

5. Licensable Period

Determination of applications will be based on the works taking place during these dates. Please ensure you have included an adequate contingency period. If works are not completed by the Requested Licence Expiry Date you may be required to submit a new application. Including a contingency period within your original application does not impact on Licence Fee
18/11/2025
17/11/2030

Start Date				Requested Licence Expiry Date


Please ensure you submit your application for a Marine Licence at least 4 months prior to the intended start date. Some projects, such as EIA projects, will take significantly longer to determine.
6. Project Description

6(a).	Please give a description of the proposed project.
This should include the purpose of the project, estimated timescales of construction and operation, and broken down by the phases of works, if applicable.
Details should include, but not be limited to, dimensions of project, quantity of material being deposited and removed.
Purpose of the project
The Saline Lagoons at WWT Llanelli, situated within the Burry Inlet SPA, regularly host internationally important populations of waterbirds which use the lagoons as safe feeding and roosting habitat; to continue supporting these birds urgent repairs are needed. The lagoons are only topped up a few times annually during large spring tides and they now dry up annually, affecting the SPA bird assemblages and other saline lagoon wildlife.

The WWT Llanelli Saline Lagoons Restoration Project will improve the quality and resilience of the Saline Lagoons at WWT Llanelli Wetland Centre in Carmarthenshire. The work is being carried out to restore and protect this vital habitat for the benefit of a wide range of species including European Eel, Otter, and specialised Saline Lagoon invertebrates, as well as the wintering and passage birds for which the wider area is designated. 
Description of the work
All work will be delivered by a tracked, 13 tonne excavator and a tracked dumper truck:
1.                   Repairs to the banks of the saline lagoons, which have been eroded by wind and wave to the extent that they now have limited capacity to hold water and to support the large populations of SPA citation bird species that use the lagoons as a refuge.  All repair work to the banks will take place above Mean High Water Springs. An excavator will be used to repair banks, through minor re-profiling, using substrate excavated from dried-out areas within the lagoons to a maximum depth of 0.2m. The total length of banks requiring repairs is less than 200m, and the amount of material we will need to excavate to undertake these repairs is up to 200 cubic metres.
[bookmark: _Hlk203475426][bookmark: _Hlk203474561]2.                   Re-distribution of sediment which has accumulated within the lagoons, to increase the depth of the lagoons in certain areas and to vary the depth profile. This will increase their resilience to drying out during periods of low rainfall and improve the habitat for a range of species. This work will take place within the lagoons using an excavator and tracked dumper truck, while the lagoons are naturally drained-down in summer weather. The area of sediment that will be re-profiled is 2 ha in extent. Sediment will be excavated to a maximum depth of 0.5m, and generally by only 0.0-0.2m. This will revert the lagoons to no more than their original depth. Sediment will be redistributed to the exposed south-west corner of the lagoons, to widen the bank and create additional saltmarsh habitat thereby providing additional protection for the lagoons from the prevailing wind and wave action. The total amount of material to be moved within the lagoons is estimated to be less than 2,000 cubic metres.

There will be no materials brought onto or off the site.









































Timescales of construction

Please note that we have put a project start date of 18th November in this application, as we require a completed Habitats Regulations Assessment by this date in order to meet the requirements of a funding application to deliver this work through the Nature Networks Fund.

The bulk of the project work will take place in 2026 however we have applied for a Marine Licence covering a period of 5 years to allow for potential project delays, and the high possibility that we will need to carry out minor additional repairs in subsequent years while the lagoon banks are re-stabilising and saltmarsh habitat is developing. We are a wetland conservation charity are keen to minimise our costs and time in applying for consents so would be very grateful for a 5 year licence period if possible.

Phase 1:
All work described above will be undertaken between April to August (and ideally May to July) 2026. 
The duration of this phase is estimated to be around 2 weeks’ work in total.
Phase 2:
If there are delays to the project delivery we may need to postpone works until the period April to August 2027
Phase 3:
We may need to carry out minor repairs to lagoon banks between April to August 2028 to fix any leaks or cracks in the banks following winter storms and high tides.
Phase 4:
We may need to carry out minor repairs to lagoon banks between April to August 2029 to fix any leaks or cracks in the banks following winter storms and high tides.
Phase 5:
We may need to carry out minor repairs to lagoon banks between April to August 2030 to fix any leaks or cracks in the banks following winter storms and high tides.





































Please continue on a separate sheet if necessary. Please tick if you have done this ☐

6(b).	Please detail the location of the proposed construction project.
These should be Latitude and Longitude coordinates (WGS84) in decimal degrees to 5 decimal places (e.g. Lat 52.12345 Long -4.12345), defining the extent of the project.
Saline Lagoons North central point: 51.66525 , -4.12988

Saline Lagoons South central point: 51.66260 , -4.12998

Saline Lagoons West central point: 51.66400 , -4.13173

Saline Lagoons East central point: 51.66405 , -4.12802










Please continue on a separate sheet if necessary. Please tick if you have done this ☐

6(c).	The following must be provided with the completed application form:

(i) a suitably scaled extract of an Ordnance Survey Map or Admiralty Chart with location of project, complete with North Arrow and Scale

(ii) construction plans and sectional drawings showing those proposed works below/seaward of MHWS, which should give details of the materials to be used (for beach replenishment the quantity, particle size and source of material to be deposited and deposit location is also required).

(iii) a descriptive schematic drawing and suitably scaled location plan which show the full extent of the project clearly in relation to the surrounding area and features.

Please list below all supporting documents that have been submitted with this application, including suitable documents/maps/drawing titles and reference numbers
(i) OS map of WWT Llanelli, showing location of Saline Lagoons.pdf
(ii) Google Earth plan of Saline Lagoon proposed works with scale.jpeg
(iii) Google Earth plan showing full extent of project area and access route.jpeg
(iv) Impact Assessment 1 - Saltmarsh Habitat
(v) Impact Assessment 2 – Protected Sites
(vi) Impact Assessment 3 – Fish
(vii) WFD scoping Exercise for Saline Lagoons Project
(viii) Correspondance with NRW Marine Licencing regarding the project
(ix) Correspondance with NRW Marine Area Advice and Mgmt Team
(x) Photographs showing eroded saline lagoon banks and dried up lagoon bed

Please note that ecological reports and survey data for wetland birds, saline lagoon invertebrates, and saltmarsh flora NVC mapping can be provided on request.


















Please continue on a separate sheet if necessary. Please tick if you have done this ☐

The applicant should note that these drawings/plans may be copied to others as part of the MLT's consultation procedures. If they are subject to copyright, it is the responsibility of the applicant to obtain the necessary approvals to reproduce the documents.

7. Methods Statement

7(a).	Please provide a detailed method statement for the works
This must include methods for all works including temporary structures or deposits such as jetties, cofferdams, moorings or landing stages to be constructed seaward of MHWS
Construction methods: details of materials, how waste generated will be managed, sediment management

There will be no waste generated by the project work. 

A 13 tonne excavator will be used to repair banks, through minor re-profiling, around the saline lagoons where high tides and storms have caused damage or erosion. This will require the excavation and movement of up to 200m3 of substrate from within the saline lagoons, excavated from dried-out areas to a maximum depth of 0.2m. The total length of banks requiring repairs is less than 200m. 

We used the same technique to carry out minor repair work to the banksides previously as approved by National Resources Wales under SSSI consent, and the saltmarsh vegetation has recovered quickly in repaired sections once the sediment has stabilised. 

A 13 tonne excavator and tracked dumper will also be used to re-distribute sediment which has accumulated within the lagoons, to increase the depth of the lagoons in certain areas and to vary the depth profile. Work will be limited to dried-out areas of the lagoons, while they are drained-down in summer weather. The area of sediment that will be re-profiled is 2 ha in extent. Sediment will be excavated to a maximum depth of 0.5m, and generally by only 0.0-0.2m. This will revert the lagoons to no more than their original depth. 






















Sediment will be redistributed to the exposed south-west corner of the lagoons, and built up to a level no higher than the surrounding saltmarsh habitat. This will serve to widen the bank and create additional saltmarsh habitat thereby providing additional protection for the lagoons from the prevailing wind and wave action. The total amount of material to be moved within the lagoons is estimated to be no more than 2,000 cubic metres.

There will be no materials brought onto or off the site.

Bank repairs will be undertaken by TJK Harries and Sons Ltd, using a 13 tonne tracked excavator. This company is experienced in a variety of landscaping and wetland management work.  The contractors will follow a variety of practices to minimise their environmental impact.

General Site Management: 

No oils, chemicals, or concrete mixing/washing areas will be stored on site.  All machinery refuelling will take place off the N2K site, and a minimum of 30m from any waterbody or surface drain, and spill kits will be carried.

The repair of the banks is anticipated to require no more than 10 days of work in total, which will be completed between the months of April and August 2026, and ideally between May and July, with exact dates depending on contractor availability.  The repairs will take place on weekdays between the hours of 9am to 5pm.

Biodiversity Management: invasive species management; species and habitats protection (including any time of year restrictions), avoidance and mitigation measures. 

The Wildfowl and Wetlands Trust are an internationally respected nature conservation charity and the purpose of the work is to deliver environmental benefits to the N2K site. Minimising impacts on the environment and wildlife has been considered for all stages of the work delivery.

This work takes place within the Burry Inlet Special Protection Area and Carmarthen Bay Estuaries Special Area for Conservation, The work will repair the banks of the lagoon, to enable them to function properly and hold water, and it will benefit the internationally-important wintering and passage birds for which the N2K area is designated.
All work will be undertaken by local contractors with a 360° excavator, experienced in creating wetland features and working in areas with sensitive wildlife and habitats. 

Mitigation measures are listed in section 12c below and in the three associated impact assessments.

• Invasive species management

No invasive species have been recorded on the project site and if found subsequently they will not be disturbed as part of any construction work. Once on site, vehicles and other equipment or materials will not be moved between different areas of the site, to avoid accidental transmission of INNS.  We will also ensure that foot wear, chest waders, and equipment are thoroughly washed before and after use in the lagoons. This is standard practice at WWT Llanelli under our existing INNS biosecurity protocols to avoid accidental transmission of INNS within the site.

Silt management, and a waste management plan to identify where the waste material would go. 

No silt will be moved outside the footprint of the Saline Lagoons during project delivery.

There will be no other waste resulting from the project.

Control of Nuisances: details of restrictions to be applied during construction including timing, duration and frequency of works; details of measures to minimise noise and vibration from piling activities, for example acoustic barriers; details of dust control measures; measures to control light spill and the conservation of dark skies. 

Work will take place between the hours of 8am to 5pm on weekdays, and the delivery of the project work will take place as quickly as possible, lasting an estimated 2 days in total.

In the Saline Lagoon noise will be created by a 13 tonne excavator working for an estimated 2 weeks.  Noise arising from work on the Saline Lagoon is screened by the sea wall embankment. 

Owing to the natural screening and the distance from areas accessible to the public we do not propose using acoustic barriers for the project.



























































Vibration from the work will be minimal, resulting from the movement of machinery around the site. There will be no piling activities.

Due to the nature of the habitat and materials being worked with, it is unlikely that dust will be created during the work, hence no dust control measures are proposed.

Work will not take place outside of daylight hours hence there will be no need for artificial lighting or measures to control light spill.

Resource Management: details of fuel and chemical storage and containment; details of waste generation and its management; details of water consumption, wastewater and energy use 

No oils or other chemicals will be stored on the designated site. Diesel fuel for the Saline Lagoon work will be kept off site and will be brought on site by contractors as and when required, with all refuelling taking place away from the N2K site and at least 30m from any waterbody or surface drain.

There will be no waste generated from the repair work.

No water will be required for the project delivery, nor wastewater created. 

Once machinery arrives on site to commence project delivery it will remain on site until the work is completed.
No deliveries will be required for the repair work.

Pollution Prevention: demonstrate how relevant Guidelines for Pollution Prevention and best practice will be implemented, especially whilst de-silting, including details of emergency spill procedures and incident response plan. 

The following pollution prevention method statement will be communicated to the contractors by the project manager on site.  

· Spill kits will be present at all times on site located next to the refuelling point. 
· Refueling will take place at least 30m away from any waterbody and from the N2K site boundary.
· Fuel will be transported and stored in approved, sealed containers/jerry cans that are specifically designed for fuel storage.
· In the event of a spillage contain the area using a spill kit and report to the site supervisor immediately.
Details of the persons and bodies responsible for activities associated with the project and emergency contact details 

Role
Name
Job title
Contact number
Project Manager, First Aider
Brian Briggs
WWT Llanelli Nature Reserve Manager
01554 741087/07734 456484
Site access, First Aider
Aled Evans
WWT Llanelli Living Collections Manager
01554 741087
WWT Centre Manager
Jo Jones
WWT Centre Manager
01554 741087
Saline Lagoon contractor
Iwan Harries
TJK Harries & Son


Landscape/ecological clerk of works to ensure construction compliance with approved plans and environmental regulations. 

Dr Brian Briggs, Ecologist and WWT Llanelli Reserve Manager with extensive experience of delivering habitat creation, water vole and wildlife enhancement projects.




















































Please continue on a separate sheet if necessary. Please tick if you have done this ☐

7(b). Do you intend to undertake activities that could generate underwater noise?
This include piling, use of explosives, geophysical, acoustic deterrent devices and multibean echosounders. 								Yes ☐ No ☒

7(b) (i). If Yes, what type(s) of activities will be undertaken?














7(b) (ii). If Yes, approximately how many days will the activity be undertaken for?  














If Yes, you will be required to complete an additional form that will be provided.

7(c).	Please state the measures to be taken to:
(i) Minimise risk to the marine environment 
Please see section 12c below.













(ii) Prevent undue interference to others 
The work will take place on the saline lagoons at WWT Llanelli, which are visible from two wildlife viewing hides on site, but not accessible to the public. The work is scheduled for a two week period between May to July 2026 when there are low numbers of visitors to WWT Llanelli and hence very few people will be inconvenienced by the work. 
Noise levels will be kept to a minimum and no piling work is required.















(iii) Maintain navigational safety, including marking and lighting of works
N/A














Please continue on a separate sheet if necessary. Please tick if you have done this ☐

8. Materials of Project 

8(a).	Description of materials to be deposited seaward of MHWS (Please tick all that apply)
Timber	☐	Iron/Steel	☐	Concrete	☐	Biocides/other chemicals	☐
Silt		☒	Stone/Rock	☐	Gravel		☐	Plastic/Synthetics		☐ 
Sand	☐	Other		☐	

If other, please provide a description of materials.
Bare sediment (silt) from the dried-out bed of the saline lagoons will be excavated to a maximum depth of 0.5m and re-distributed within the perimeter of the saline lagoons. No materials will be brought on to, or off, the project site.












8(b).	Delivery method of materials to site
If sea delivery, please include details of vessels to be used with a chart of proposed route and transhipment area. If vehicle delivery, please provide the proposed access route. 













Please continue on a separate sheet if necessary. Please tick if you have done this ☐

8(c).	Will the works involve removals seaward of MHWS?		Yes ☒ No ☐

8(c) (i). Description of materials to be removed seaward of MHWS (Please tick all that apply)
Timber	☐	Iron/Steel	☐	Concrete	☐	Biocides/other chemicals	☐
Silt		☒	Stone/Rock	☐	Gravel		☐	Plastic/Synthetics		☐ 
Sand	☐	Other		☐	
8(c) (ii). Description of objects/materials to be removed seaward of MHWS
Including quantities to be removed.
Bare sediment (silt) from the dried-out base of the saline lagoons will be excavated to a maximum depth of 0.5m and re-distributed within the perimeter of the saline lagoons. No materials will be brought on to, or off, the project site.















9. Beach Replenishment, Land Reclamation or Salt Marsh Feeding
For works involving any of the above, please provide the following information 

9(a). Is the material to be deposited like for like to existing material? 	Yes ☐ No ☐

9(a)(i) If No for Beach Replenishment please provide justification why?













9(b).	Description of material to be deposited
Please provide the grading specification of materials to be used, if using a range of grain sizes please state the percentage by weight passing. If unsure, please refer to the Wentworth Scale 
















Please continue on a separate sheet if necessary. Please tick if you have done this ☐

9(c).	Source of the material to be deposited
Including dredged or land based stating the origin of material
















9(d).	Has the material been chemically analysed? 			Yes ☐ No ☐
If material has been analysed, we may request this information to determine the application

9(d) (i) If Yes, is the analysis data been included with the application? Yes ☐ No ☐


10. Temporary Works

10(a).	Will there be any temporary deposits below MHWS? 		Yes ☐ No ☒
This includes construction materials, removed objects/material, jetties or cofferdams
If Yes, please continue with section 10

10(b).	Please provide the location of temporary deposits 
Please include a map/chart displaying the location of temporary deposits, if necessary.














10(c).	Description of temporary deposits

















Please continue on a separate sheet if necessary. Please tick if you have done this ☐


11. Dredge and Disposal of Dredge Material
If you are undertaking Dredge and Disposal activities please also complete the Dredge and Disposal application form and submit together.

11(a).	Do you intend to apply for a marine licence to dispose of dredged material to sea as part of the works in this application? 			Yes ☐ No ☒

12. Protected Sites

Licensing Authorities have a duty to ensure that projects will not have significant adverse environmental impact, particularly on any designated European Site of Conservation Importance - Special Areas of Conservation (SAC) and Special Protection Areas (SPA), listed under the Habitats Directive (Council Directive 92/42/EEC on the conservation of natural habitats and of wild fauna and flora). In addition, it is Government Policy that Wetlands of International Importance (Ramsar sites) are also considered as European Sites.  There is a duty to take reasonable steps to further the conservation and enhancement of nationally designated sites (Sites of Special Scientific Interest (SSSIs).

12(a).	Have you had pre-application correspondence with NRW, its legacy bodies or Natural England? 								Yes ☒ No ☐


12(a)(i). If Yes, please provide copies of correspondence with application and state which team(s) you have contacted? 
Joe Thomas, Senior Officer, Marine Licencing Team, and Adam Cooper, NRW Senior Marine Advisor, correspondence attached.
















12(b).	Are any part of the works located within or likely to affect a designated conservation site? (SAC, SPA, SSSI or Ramsar)			 Yes ☒ No ☐

12(b)(i). If Yes, which designated site(s) may be affected?
Carmarthen Bay and Estuaries SAC
Burry Inlet SPA
Burry Inlet Ramsar Site
Burry Inlet and Loughor Estuary SSSI














12(c).	Please provide a description of all mitigation measures proposed to avoid any impact on designated conservation sites.
· We will take measures to reduce saltmarsh and creek damage by vehicles by using existing access tracks, and where this is not possible we will minimise impacts by using tracked vehicles to spread the weight distribution, and by using mats in softer sections.
· We will only use vehicles on the saline lagoon banks and within the lagoons themselves, and will not need to access any creeks or other areas of Saltmarsh SAC habitat. Within the lagoons themselves vehicles will only work in areas of bare sediment that have dried out in summer weather.
· To carry out repairs of the saline lagoon banks, excavation and movement of sediment will be kept to a minimum, estimated at up to 200m3 of material. Only degraded areas of saltmarsh would be repaired and built up to their original height.  By doing this we would avoid smothering any developed areas of saltmarsh with sediment, and the repaired sections of the banks would gradually revert to saltmarsh. 
· Any minor loss of up to 0.4ha, equivalent to 10% of Saline lagoon habitat resulting from the redistribution of sediment within the lagoons will be compensated for by an increase in the quality, diversity, and resilience of the remaining lagoon habitat. 
· Furthermore, as part of a wider WWT Llanelli habitat enhancement project, two freshwater wetland areas inland of the sea wall called the Dafen Scrapes and Western Scrapes, will be enhanced for wetland wildlife and open water areas will be extended by around 1ha in 2027-8. These areas will offer additional habitat for SPA bird assemblages moving in and out of the protected site.
· An alternative approach to redistributing sediment within the footprint of the saline lagoons would be to take the excavated sediment off the protected site.  However we are following the guidance of the NRW position statement on The Sustainable Management of Marine and Coastal Sediment which favours retaining the sediment as close as possible from where it originated, within the same sediment system, and using it for habitat (saltmarsh) restoration.
· The project will result in a net increase in SAC saltmarsh habitat, which is classed as a ‘higher sensitivity habitat’ in the WFD scoping template.
· Pollution prevention measures will be taken to reduce any contamination, suspended sediments etc. from the works. We will carry a spill kit for use in the unlikely event of any fuel spillage. All refuelling will be carried out off the protected site.
· We will time the works to reduce disturbance on bird features as much as possible.  We will ensure that works are completed during the period April to August, and if possible May to July, to minimise impacts on wintering and migratory waterbirds. We will also avoid working during spring high tides to ensure that the lagoons remain available as an undisturbed roosting area for birds when much of the wider estuary is under water. The saltmarsh and lagoons will be checked carefully for signs of any ground nesting birds prior to work commencing and work will be postponed if necessary.  
· Work on the lagoons will be undertaken as quickly as possible (an anticipated duration of 2 weeks) to minimise disturbance impacts on wildlife and protected site features. One of the three saline lagoons will be left entirely undisturbed as a refuge for fish and invertebrates. 
















































· The work will not take place in areas where notable plant species were recorded by local ecologist Barry Stewart as part of his 2019 saltmarsh flora survey.
· To avoid introducing or spreading INNS, We will ensure that contractors and WWT vehicles have not been used in other waterbodies and are not moved to other waterbodies inland of the sea wall embankment. 

Further details of mitigation measures are provided in the associated Impact Assessment documents.




















Please continue on a separate sheet if necessary. Please tick if you have done this ☐

12(d).	If the works are not located within or likely to affect a designated conservation site, please indicated the approximate distance to the nearest designated conservation site.













Please note that if the proposed works are in or within 2km of a European Site of Conservation Importance you will have to provide suitable mitigation measure to avoid any impact on designated conservation sites.

13. Other Consents

Please detail all consents that you have applied for or received for these works

	Type of Consent
	Applied for
	To be applied for
	Reference Number
	Date of Issue and Expiry

	Planning Permission under Town and County Planning Act 1990 – From Local Planning Authority (LPA)

	Not required for Saline Lagoon restoration works
	Likely to be required for future freshwater habitat creation works as part of a wider project and we have enquired with the LPA about this.
	
	

	Name and Address of LPA for location of works

	Carmarthenshire County Council, County Hall, Carmarthen, SA31 1JP

	Land Owners Consent such as The Crown Estate Consent

	Requested from CCC on 16-7-25
	
	
	

	Port Authority or Local Harbour permissions

	N/A
	
	
	

	Other NRW consents such as Flood Defence or SSSI assent
	N/A
	
	
	

	Details of NRW consent

	SSSI assent and a HRA will be informed by this Marine Licence

	Other consents such as Transport and Works Act Order, Section 36 Electricity Act, grant/loan sanction
	N/A
	
	
	

	Details of other consents 


	



14. Statutory Powers

14(a).Does the applicant have statutory powers to consent any aspect of the project? 
E.g. coast protection authority, dredging powers, statutory undertakers	Yes ☐ No ☒

14(a)(i).If Yes, please give details and state the relevant legislation that gives these powers
















15. Public Register

Under The Marine Licensing (Register of Licensing Information)(Wales) Regulations 2011 and the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended) , all information contained within or provided in support of this application will be placed on the Public Register unless NRW approve of the applicant’s reasons for withholding all or part.	

15.	Is there any information contained within or provided in support of this application that you consider should NOT be included on the Public Register on the grounds that its disclosure:

15(a).	Would be contrary to the interest of National Security? 		Yes ☐ No ☒

15(b).	Would prejudice to an unreasonable degree you, or some other person’s commercial interest of those of a third party? 			Yes ☐ No ☒

If Yes to either (a) or (b), please provide full justification as to why all or part of the information you have provided should be withheld
























Please continue on a separate sheet if necessary. Please tick if you have done this ☐

16. Application Fee

16(a). What are the corresponding fee band for this application? Band 2 ☒ Band 3 ☐

16(b) Band 2 Only
Projects are charged at a fixed fee of £1920. The application will not be processed until the correct fee has been provided.

Please provide the method of payment 

	Method
	Yes (√)
	Reference Number

	Cheque
	
	

	BACS (not remittance no.)
	
YES

	

	World Pay (phone or CC1)
	

	


Please attach CC1 Form with application. Can be found on our web pages

16(c) Band 3 Application only
Band 3 applications are charged at on hourly rate of £120 and are invoiced in arrears. Please complete the details below which will be required for invoicing.


Customer Name




FAO



Purchase order number



Address for invoice





Telephone Number





Email Address




17. Declaration

I declare that to the best of my knowledge and belief that the information given in this application form and supporting documentation is true.

	WARNING: It is an offence under the Marine and Coastal Access Act 2009, under which this application is made, to fail to disclose information or to provide false or misleading information and can invalidate any licence granted.




Signature	Brian Briggs					Date	16-7-25



Name (in capitals)	BRIAN BRIGGS

Position in Company	WWT Llanelli Reserve Manager							
	


Applications cannot be processed unless signed by the Applicant (not agent), the applicant must have appropriate level of authority within the company.

Applications will not be processed unless signed
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