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Site: SA1 Phase 7
Product: Diesel fuel – DERV / GAS OIL





Assessment by: Nathan Hunt
Date: 24.08.18 22626.01.187 2m225/05/07002.03.07
REF No: 005





	Site Specific Activity and Control Measures        
                                     (This section must be completed)

	Method
	General use. Plant filled from bund protected tank

	
	Location
	Site compound and bowser

	
	Duration
	Duration of contract

	
	Control
	Toolbox talk to all plant/machine operators. Tank controlled by storeman.

	Exposure Limits

	None applicable

	Physical Properties
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	Petroleum distillates and hydrocarbons

DERV - Clear liquid, flashpoint >56°C, characteristic odour

GAS OIL - also contains red additives (HM Customs markers)

	Hazard
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	Vapour in high concentrations can lead to nausea, headaches and dizziness.
Skin contact over prolonged period can lead to skin irritation, dermatitis.  

	
	
	Warty skin growths can occur which can become cancerous if occupational and personal hygiene standards are poor.
Ingestion/vomiting can result in aspiration into lungs which can be fatal

	Work Procedures/PPE
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	Avoid contact with skin and eyes
Wear impervious gloves (impervious heavy duty knitted wrist) to
BS EN 374.
No smoking or other sources of ignition during re-fuelling
Avoid breathing vapour, ensure adequate ventilation


	First Aid/Fire
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	Inhalation: remove to fresh air and rest
Ingestion: do not induce vomiting – seek immediate medical attention
Eye Contact: irrigate with plenty of water
Skin Contact: wash with soap and water – remove contaminated clothing
Fire: treat as a petroleum fire - use foam / dry powder / CO2 


	Storage/Disposal
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	Storage: clearly labelled (UN No 1202), Flammable liquid diamond warning symbol.  A secondary containment facility must be provided for the storage unit, in accordance with the Control of Pollution (Oil Storage) Regulations 2001

Disposal: as special waste

	Environmental
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	Harmful to aquatic organisms, may cause long-term damage in aquatic environment

Spillages: remove all ignition sources, absorb with spill kit / sand and prevent entering drains or watercourses, evacuate personnel from area, transfer to suitable containers for disposal
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