
Permit Number: 	EPR/KP3135KV		Operator: 		The Royal Mint Limited

Facility: 		The Royal Mint		Form Number: 	 Air1 / 18/06/2026
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A32
	Particulate Matter
	5 mg/m3
	Averaged over the sampling period (at least half an hour)
	
	BS EN 13284-1
	
	

	A32
	Hydrogen Bromide
	No limit set
	None set
	
	To be agreed in writing with Natural Resources Wales
	
	

	A33
	Particulate Matter
	5 mg/m3
	Averaged over the sampling period (at least half an hour)
	
	BS EN 13284-1
	
	

	A33
	Acetic Acid
	No limit set
	None set
	
	
	
	

	A33
	Hydrogen Chloride
	No limit set
	None set
	
	
	
	

	A34
	Particulate Matter
	5 mg/m3
	Averaged over the sampling period (at least half an hour)
	
	BS EN 13284-1
	
	

	A34
	Brominated fire retardants
	No limit set
	None set
	
	To be agreed in writing with Natural Resources Wales
	
	

	EP1
	Hydrogen Bromide
	No limit set
	None set
	
	To be agreed in writing with Natural Resources Wales
	
	






[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

Permit Number: 	EPR/KP3135KV		Operator: 		The Royal Mint Limited

Facility:		The Royal Mint		Form Number: 	Water1 / 19/01/2023
Reporting of emissions to water (other than to sewer) and land for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	W1
	Suspended solids
	50 mg/l
	24 hour flow proportional sample
	
	BS EN 872
BS 6068-2.54:1996
	
	

	W1
	Temperature
	30 °C
	Spot sample
	
	As approved by Natural Resources Wales
	
	

	W1
	Free Chlorine
	0.1 mg/l
	Spot sample
	
	As approved by Natural Resources Wales
	
	

	W1
	Oil
	None Visable
	Instantaneous
	
	Visual Check
	
	

	W2
	Oil
	None Visable
	Instantaneous
	
	Visual Check
	
	

	W3
	Oil
	None Visable
	Instantaneous
	
	Visual Check
	
	

	W5
	Oil
	None Visable
	Instantaneous
	
	Visual Check
	
	

	W6
	Oil
	None Visable
	Instantaneous
	
	Visual Check
	
	

	W7
	Oil
	None Visable
	Instantaneous
	
	Visual Check
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.


Signed …………………………………………………………….  		Date………………………..
	(Authorised to sign as representative of Operator)

Permit Number: 	EPR/KP3135KV		Operator: 		The Royal Mint Limited

Facility:		The Royal Mint		Form Number: 	Sewer1 / 18/06/2026
Reporting of emissions to sewer for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	S1
	Free Cyanide
	30 mg/l
	Spot Sample
	
	BS EN ISO 14403-1 or BS EN ISO 14403-2
	
	

	S1
	Copper and its compounds
	0.005 mg/l
	Spot Sample
	
	BS ISO 17294-2
BS6068-2.89:2003
	
	

	S1
	pH
	Minmium 6
Maximum 11
	Houly Average
	
	BS ISO 10523
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)
[bookmark: _Hlk117597971]
Permit Number: 	EPR/KP3135KV		Operator: 		The Royal Mint Limited

Facility:		The Royal Mint		Form Number: 	WaterUsage1 / 18/06/2026

Reporting of Water Usage for the year 20XX

	Water Source
	Usage
(m3/year
	Specific Usage 
(m3/unit output)
	

	
	
	
	

	
	
	
	

	Mains water
	
	
	

	River abstraction
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	TOTAL WATER USAGE
	
	
	



	Operator’s comments :







Signed …………………………………………………………….  		Date………………………..   	
	(authorised to sign as representative of Operator)
Drafting note: if the operator is required to submit Resource Efficiency Physical Index (REPI) data to the Pollution Inventory, please ensure that no metrics are repeated in this reporting form.

Permit Number: 	EPR/KP3135KV		Operator: 		The Royal Mint Limited

Facility:		The Royal Mint		Form Number: 	Energy1 / 18/06/2026

Reporting of Energy Usage for the year 20XX

	
Energy Source
	Energy Usage
	
Specific Usage
(MWh/unit output)
	

	
	
Quantity
	Primary Energy
(MWh)
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	Electricity *
	MWh
	
	
	

	Natural Gas
	MWh
	
	
	

	Gas Oil
	tonnes
	
	
	

	Recovered Fuel Oil
	tonnes
	
	
	

	
	
	
	
	

	TOTAL
	-
	
	
	

	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments :









Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)
Drafting note: if the operator is required to submit Resource Efficiency Physical Index (REPI) data to the Pollution Inventory, please ensure that no metrics are repeated in this reporting form.


Permit Number: 	EPR/KP3135KV			Operator: 		The Royal Mint Limited

Facility:		The Royal Mint			Form Number: 	Performance1 / 18/06/2026

Reporting of other performance indicators for the period DD/MM/YYYY to DD/MM/YYYY

	Parameter
	
	Units 
	

	
	
	
	

	Total raw material used 
	tonnes
	

	Water abstraction from river
	m3/year
	

	Natural Gas usage
	MWh
	

	CO2/Final product tonnage
	Kg/Tonne
	

	Total waste/final product tonnage
	Tonne/tonnes
	

	
	
	

	
	
	

	
	
	



	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)
Drafting note: if the operator is required to submit Resource Efficiency Physical Index (REPI) data to the Pollution Inventory, please ensure that no metrics are repeated in this reporting form.
