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LPD1- landspreading of waste

Please note – this document is to assist in making a decision
and may not necessarily cover all information required
See TGN8.01 for all required information
Each application is assessed based on its own individual merit
	Details

	Deployment Reference Number:
	PAN-032644

	Permit Reference Number:
	EPR-DB3592ZM

	Permit Holder:
	Puffin Produce Ltd

	Site Address:
	Clarborough Farm,Narberth Road, Haverfordwest, SA62 4PB

	Grid Reference:
	Farm location: SM 99017 15525

Fields: 
Above Bungalow SM98820 15792 
Upper Cotts Park SM98588 15624 
Middle Cotts Park SM98763 15466 
Lower Cotts Park SM98790 15252 
Front Field SM99239 15376 
Gold Mine SM 99100 15228 
Bungalow Paddock SM 98839 15655 
Triangle Yard SM 98975 15651 
Bottom Field SM 99200 15012

Storage: No storage details




	Administrative Checks- by permit support officer

	
	Comments

	Consultation
	Waste reg team: wasteregulation.swwales@cyfoethnaturiolcymru.gov.uk 
Environment team: pembsdistrictteam@cyfoethnaturiolcymru.gov.uk 
NLO: Michael.Edwards@cyfoethnaturiolcymru.gov.uk 

	Date due:
	15/05/2026

	Are fields on Anglesey? If yes, then send application.
	No: N/A

	Permit compliance rating and multiplier
	Rating A- 100%




	Fundamental checks- by determining permitting officer

	Item
	Action completed, or document provided 
(Yes, No or n/a)
	Comments

	Is the base permit still live? 
Has there been any variations we need to be aware of?
	Y 
	Welsh- DMS/PaLS


	Correct fee?
	Y 
	See permit compliance multiplier above and deployment fee- Charging Scheme

Transaction ref: 2154176
Date: 28/04/2026
Ref: BS/280426/24 PUFFIN PRODUCE LIMFP 28/04/26 13090632826090318240HNEPDEPPUFFI0426
Amount: 1,707.00

	Agricultural Benefit Statement
	Y 
	

	Waste Analysis Report
	Y 
	13/01/2026

	Soil Analysis Report
	Y 
	13/01/2026

	Location Map
	Y 
	

	Environmental Impact Assessment- Agricultural Regulations Evidence
	Y 
	

	Risk assessment (if applicable)
	Y 
	Only if in high risk location 

	Landowner/occupier consent
	Y 
	Applicant is the owner of the land 

	If confidentiality box has been ticked, no evidence provided
	N/A
	Only if confidentiality requested

	Declaration authorisation
	Y 
	Only if not signed by a relevant person



	[bookmark: _Hlk200437951]Saving documents- by determining permitting officer
	Y N

	Save embedded application documents from application form
	 Y



	Application Form
Word versions of online forms - NRW View (sharepoint.com)
	Y N n/a
	Comments

	1. About the Permit

	Has there been any pre-application discussions?
	Y 
	Previous returns 

	Has the permit number been provided?
	Y 
	

	Has the permit holder name been provided
	Y 
	

	What permit is being deployed under?
	SR2010 No4

	

	2. Contact details

	Has contact information been provided?
	Y 
	

	Has the technically competent manager details been provided?
	Y 
	

	Has the nominated competent person details been provided?
	Y 
	

	3. About the land you want to treat

	Has the address and grid reference of the main farm address been given?
	Y 
	

	Does the farm address match the grid reference?
	Y 
	

	What type of land do they want to treat?
	Agricultural land

	

	If it is agricultural land; has the holding number been given?
	Y 
	

	Has all of parcels of land table been completed?
	Y 
	

	Is the total area of land to be treated less than 50 ha, or 100 hectares for a single continuously managed area of land?
	Y 
	

	Is the land to be treated within a 10 miles radius of the main address?
	Y 
	

	Is this deployment one of a batch (multiple deployments) for the same area of land?
	N
	

	Is the permit holder the owner or occupier of the land you want to spread on/treat?
	Y 
	

	Have details of the land owner or occupier been provided?
	N/A
	

	Has written consent of all owners(s) or occupiers(s) been given?
	Y 
	

	4. Previous land treatment

	Has all of the previous land treatment table been completed?
	N/A
	

	5. Which risk band does the activity fall within?
6. SR2010No4 List A wastes (Lower risk)
7. Location risk
8. Low risk deployment
9. Medium risk (1) deployment
10. Medium risk (2) deployment
11. High risk deployment

	Which risk band does the activity fall within?
	Medium (1)
	

	Is the risk banding correct?
	N
	Medium but have applied for high

	If Medium risk (2) or High risk deployment has a SSRA been provided?
	Y N n/a
	

	12. Additional information on sensitive receptors

	What type of risk assessment has been submitted?
	benefit statement

	SSRA submitted, not required.

	Does the land onto which the specified waste is to be spread as part of this deployment fall within scope of the Environmental Impact Assessment (Agriculture) (Wales) Regulations 2017 as semi-natural (habitat)?
	Y 
	

	If yes has the screening opinion provided by Welsh Government been provided?
	N/A
	

	If no have details of the assessment evidence to support this conclusion been provided?
	Y 
	

	13. About the waste 

	Have all parts of the waste-types table been completed?
· List of waste code (6 digit)
· Description of waste (this must be an accurate description specific to this waste that refers to the List of Waste written description)
· Physical form of waste/Is it stackable or non-stackable
· Is the waste high in readily available nitrogen?
· Producer of waste & permit number (if applicable)
· Total amount being spread/used (tonnes)
	Y 
	

	Are the wastes listed in the deployment specifically listed in the permit? 
	Y 
	

	Can you verify the waste producer (source of waste) is correct in terms of production, coding and description?
	Y 
	

	14. About the storage 

	Has all of waste storage table been completed?
	N/A
	

	Is the storage given no more than 1250 tonnes shall be non-stackable waste, and no more than 3000 tonnes of all other wastes? 
	N/A
	

	      18. Supporting documents

	Has checklist been completed?
	Y 
	

	      20. Confidentiality and national security

	Has confidentially been claimed?
	N
	

	Has national security been claimed?
	N
	

	      21. Declaration

	If signing on behalf of a relevant person, has written confirmation from a relevant person been given?
	Y 
	

	Has the operator confirmed they will comply with the conditions of the rule set?
	Y 
	

	Has the operator confirmed they will comply with the NRW pre-notification requirements.
	Y 
	

	Has a relevant person or approved person signed the declaration?
	Y 
	



	Location 
	Y N n/a
	Comments

	Has determining officer completed MyMap screening report?
	Y
	

	Do the grid references match the site plan?
	Y 
	

	If there is storage; do the grid references match the site plan?
	N/A
	

	The map must include the following details in relation to both storage and spreading 
(TGN 8.01, box 3.1)

	location of all storage sites for the waste to be spread 
	N/A
	

	surface water courses 
(permit condition: no storage or spreading within 10 meters) 
(buffer zones needed)
	Y 
	

	groundwater source protection zones 
(permit condition: no storage or spreading in SPZ1)
(high risk deployment if in SPZ2) 
	N/A
	

	any well, spring (or issue) or borehole used for the supply of water for human consumption including from a private water supply or supplies.
(permit condition: no storage or spreading within 50 meters) 
	Y 
	

	any spring (or issue), well or borehole not used to supply water for domestic or food production purposes within 50m 
(shown on map)
	N
	Spring not on maps 

	any spring (or issue), well or borehole used to supply water for domestic or food production purposes within 250m 
(shown on map)
	Y 
	

	any European designated sites- Natura 2000 (SPA, pSPA, SAC or cSAC) or Ramsar- or SSSI within 500m
(shown on map)
	N/A
	

	location of any public rights of way
(shown on map)
	N/A
	

	any buildings or houses within 250m
(shown on map)
	Y 
	

	Within Groundwater Safeguard Zone
	N/A
	

	the location of any other designated environmentally sensitive sites within 500m. Including but not limited to:
· Protected Species/Habitats
· Section 7 species 
· Scheduled Monument
· Local Nature Reserve
· National Nature Reserve
· Ancient Woodlands
· Local Wildlife Sites (SINC)
· National Park
· Hedges
· Ditches
	N
	National park not identified

	Flood risk
	Y 
	

	What is the slope of the fields?



	N/A



	Waste Storage 
	Y N n/a
	Comments

	Is waste storage occurring at the place where waste is being deployed? 
	N/A
	

	Is only waste as specified in this deployment being stored in the proposed storage locations? i.e. slurry in lagoons
Note: There may be multiple deployments using one storage location
	N/A
	

	If the waste is stackable and stored in temporary field heaps; are the storage locations in the same place one constructed within the last two years? or in different location?
	N/A
	

	If the waste is stackable and stored in temporary field heaps; are the storage locations in a field:
· liable to flooding or becoming waterlogged, or 
· within 50 metres of a borehole, spring or well or 
· within 10 metres of surface water or a land drain
· within 30 meters of a watercourse on steeply sloping land
	N/A
	

	If the waste is non-stackable is the waste stored within either a vessel, a covered building, or on an impermeable surface
	N/A
	

	If the waste is high RAN and it is being stored within 200 metres of a European Site (SAC/SPA), Ramsar Site or a Site of Special Scientific Interest (SSSI) is the waste being covered to prevent loss of ammonia? (condition 3.2.4 of the permit)
	N/A
	



	Waste Analysis
	Y N n/a
	Comments

	Is the waste analysis report less than 12 months old at time of application?
	Y 
	Waste analysis is in m3 and no density provided to convert 

	Does the analysis include the following?

	· pH
	Y 
	

	· Nitrogen (N)
	Y 
	

	· Phosphorus (P)
	Y 
	

	· Potassium (K) 
	Y 
	

	· % dry matter
	Y 
	

	Does the analysis include the following? 
If it is a required parameter for the waste (see section below) and has not been tested for; has adequate justification been provided?

	· Zinc 
	Y 
	

	· Copper 
	Y 
	

	· Nickel 
	N 
	

	· Lead 
	N 
	

	· Cadmium 
	N
	

	· Mercury 
	Y
	

	· Magnesium 
	Y
	

	· Sodium   
	N
	

	· Sulphur 
	Y 
	

	Check Appendix A of TGN 8.01 for the wastes types applied for. 

	· Are there any special testing requirements?
	N
	

	· If yes; have they been tested for?
	N/A
	

	If spreading waste soil, has the analysis been carried out at an MCERTS Lab?
	N/A
	

	If the spreading is in a groundwater safeguard zone (permit condition 2.1.8); are any wastes “high readily available nitrogen wastes”? i.e. organic wastes in which more than 30% of the total nitrogen content is available to the crop at the time of spreading.
	N/A
	

	· If yes, have they stated condition 2.1.8 of the permit will be complied with?
	N/A
	



	Soil Analysis
	Y N n/a
	Comments

	Is the soil analysis report less than 4 years old at time of application?
	Y 
	

	Does the analysis include the following?

	· pH
	Y 
	

	· Potassium (K)
	Y 
	

	· Phosphorus (P)
	Y
	

	· Magnesium (Mg) 
	Y 
	

	If the waste analysis shows high PTE’s; have these been tested for in the soil?
	N
	

	Have the soil indices for P, K and Mg on each field been given?

	N
	Can’t fully assess due to incorrect units but Mg indices of 3 with no justification 

	Does analysis show that the soils are deficient in the nutrients or properties required by the proposed cropping? 
	N
	



	Benefit Statement
	Y N n/a
	Comments

	Does the writer of the benefit statement have appropriate technical expertise? (TGN 8.01 6.1)
	Y 
	

	Does the activity meet the definition of recovery? (TGN 8.01 6.2)

	· Is there a clear benefit from the activity? 
	Y N
	Full assessment cannot be completed due to not knowing correct additions 

	· Is the material suitable for its intended use? 
	Y N
	

	· Is the minimum amount of waste being used to achieve the intended benefit? 
	Y N
	

	· Is the waste being used as a substitute for a non-waste material? 
	Y N
	

	· Will the proposal be completed to an appropriate standard? 
NOTE: For this activity, the standard is the deployment application that has been assessed and approved. Any deviation from this which has not been agreed is likely to be viewed as disposal.
	Y
	

	Benefit should be assessed against the following criteria. If the chosen benefit, has information been given on? (TGN 8.01 6.3)

	· Plant nutrient requirements
	Y 
	

	· Timing of application
	N
	No timing of spreading given

	· Amount of waste to be applied and application rate
	Y N n/a
	Application rate in wrong units 

	· Soil chemical properties (e.g. liming and pH) 
	N
	

	· Soil physical properties (e.g. organic matter and soil structure)
	Y
	

	· Soil water content 
	Y
	

	· Levelling the land
	N/A
	

	Timing of application- if any of the wastes are high RAN, are they being spread OUTSIDE of the closed periods 
	N/A
	

	Groundwater Safeguard Zone for nitrate- if any of the wastes are high RAN, are the application rates less than 50 m3/ha, with a minimum 3 week gap between applications
	N/A
	

	If an operator wants to apply more nutrients than is recommended in RB209 have they? (TGN 8.01 6.3)

	· Justified the nutrient level with appropriate technical expertise
	Y N n/a
	Unsure due to incomplete nutrient assessment 

	· Included the nutrient level in their environmental risk assessment
	Y N n/a
	

	· Stated the source of information that they used to set the nutrient level.
	Y N n/a
	

	Have any potential negative impacts of the activity been addressed? 
(TGN 8.01 6.5)
	N
	Minimal and has been focused on the activity rather than risks of the material being spread 

	Is the application rate appropriate (i.e. not be applied in excess of crop or soil need, as this may not meet the principles of waste recovery) in terms of? (TGN 8.01 6.7)

	· Waste type
	Y N
	Unsure due to incomplete nutrient assessment

	· Waste analysis
	Y N
	

	· Crop nutrient requirements
	Y N
	

	If the cropping is any of the following, check if that the available Nitrogen applied is less than the below amount:
· Field beans, Peas- 0 kg/ha
· Sugar beet- 120 kg/ha
· Asparagus, Carrots, Forage maize. Radish, Spring barley, Swedes- 150 kg/ha
· Spring-sown wheat, Winter barley- 180 kg/ha
· Autumn or early winter sown wheat- 220 kg/ha

*Regulation 10 The Water Resources (Control of Agricultural Pollution) (Wales) Regulations 2021
	N/A
	

	Nutrient assessments for P- If land is above target index (3+ for arable, grassland, and forage crops. 4+ for vegetables) has a net reduction in P levels across the crop rotation been demonstrated?
	Y N n/a
	Unsure due to incomplete nutrient assessment

	Nutrient assessments for P- if the above has been agreed for a previous deployment, is it still correct for this this application?
	N/A
	

	If multiple wastes are being mixed: (TGN 8.01 6.8)

	· Does each waste confer benefit in its own right?
	N/A
	

	· Is it only for operational purposes?
	N/A
	

	· Have individual application rates for each waste been given?
	N/A
	

	· If mixing ratios have not been given, is there a statement saying that the highest limiting parameter will be used as the maximum application rate allowed to be spread, i.e. the waste will be spread at the lowest application rate.
	N/A
	

	Application of waste (TGN 8.01 6.10)

	· Is method of application appropriate for the waste type and cropping?
	Y 
	

	· Is the timing of application appropriate? 
	N
	Not specified 

	· Have they stated when the waste will be spread?
	N
	

	· Have they stated how often the waste will be spread?
	N
	

	Have the total nutrients supplied by the waste been given? 
	Y 
	Magnesium missing 

	Does the total nutrients given by the applicant match NRW calculations?
	N
	

	Has total nutrients supplied been given in oxide format?
	N
	

	Has the SNS for each field been provided? Or enough information provided to calculate the SNS?
	N 
	

	If the operator has stated (or intelligence from local teams have told us) that other sources of nutrients have been applied in the last 12 months; have they stated:

	· What material was spread?
	N/A
	

	· How much material was spread?
	N/A
	

	· At what application rate material was spread?
	N/A
	

	· The nutrients supplied by the material?
	N/A
	



	Site specific risk assessment (TGN 8.01 2.2)
	Y N n/a
	Comments

	If the deployment is in a high-risk location as per LPD1 has a site-specific risk assessment been submitted?
	N/A
	

	If there are other designated environmentally sensitive sites within 500 meters has a site-specific risk assessment been submitted?
	N/A
	

	Does the site-specific risk assessment identify all potential?
	N/A
	

	· Sources of pollution or hazards. Potential hazards include but are not limited to dust, odours, run-off, leachate etc.
	N/A
	

	· Pathways
	N/A
	

	· Receptors that can be affected by that source of pollution. Receptors include but are not limited to environmentally sensitive sites, watercourse, local residents, public rights of way, housing, schools, workplaces and recreational facilities etc.
	N/A
	

	· Measures that will minimise or mitigate the impact will be put in place
	N/A
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	Appendix 4 assessment 
	Y N n/a
	Comments

	Is the site within 500 meters of a SSSI? 
· If yes, the complete an Appendix 4 CroW assessment.
	N
	

	Has a likely significant effect been identified?
· If yes, consult with the relevant Environment team.
· If no, save the Appendix 4 to the DMS as information only
	N/A
	



	Habitat Regulation Assessment
	Comments

	Is the site (project) within 500 meters of a European Site (SPA, pSPA, SAC or cSAC) or a Ramsar site?
	No- there is no conceivable impact pathway between the project and any European site features, due to the location of the project.



	Comments

	Consultation responses: 

No comments provided. 


	MyMap/location and slope assessments:

MyMap/location assessment

See mapping report 

Slope assessment

Limited sloping across all fields. As deployment is being returned full assessment was not competed. 


	CPH details: 

55/477/0019 – Correct to our system 


	Agricultural benefit calculations:

Analysis have been given in volumetric units and no density of waste has been provided to conduct a full assessment. Mg indices of 3 which will need to be justified for spreading regardless of additions. 



	Request for information/Return/Refusal reasons: 

	Request for information: 

N/A 


	Return/Refusal: 

The submitted waste analysis results have been provided in volumetric units. However, for assessment purposes, the results must be presented in mg/kg. As no waste density has been provided, we are unable to accurately convert the results and complete our assessment. Prior to resubmission please either:
•	Provide the density of the waste to enable conversion (via a lab analysis report); or
•	Convert the analytical results to mg/kg.


To ensure our feedback is complete, we have undertaken a preliminary assessment using an assumed density. On that basis, the following points would also need to be addressed prior to resubmission:
· Confirm whether total nitrogen or available nitrogen has been used in the assessment in regard to nitrogen applied to the soil via application
· In accordance with TGN 8.01 (Page157), if magnesium is to be applied at index 3 or above the operator should: 
· explain why the increased levels are appropriate for the receiving land 
· address the increased risks in the risk assessment within the benefit statement.
· In accordance with TGN 8.01 (page 43), the assessment of crop nutrient requirements should include nitrogen, phosphate, phosphorus and magnesium. The nutrient addition section of the Agricultural Benefit Statement does not currently include magnesium.
· The Agricultural Benefit Statement includes a table showing additions and application rates relating to manure. Please confirm whether manure forms part of the proposed deployment.
· Confirm the total application rate. This has currently been presented as three separate applications and in volumetric units. The total application rate should be provided in tonnes per hectare (t/ha).
· The proposed application rates do not align with our calculations. While this may be due to the assumed density used during our preliminary assessment, please ensure that nutrient values are expressed in oxide form, as standard practise in agronomy (refer to crop nutrient requirements,  section 1 of RB209).  

While one spring has been identified within the mapping document, there is a second spring located next to bottom field which has not been identified in the maps. See image below. As per TGN 8.01 maps must include any spring, well or borehole not used to supply water for domestic or food production purposes within 50m.
 

Cover Cotts is included in the waste analysis but is not in either the parcels of land list or maps. In addition, Lower Cotts waste analysis has not been submitted. Please ensure names of fields are consistent across all deployment documents.  





	Decision

	Can the deployment application be approved?
	No

	Issue date
	

	Effective date
	

	Permitting Officer
Date
	

	Team leader or Transfer of Powers (ToP) approval
Date 
	Huw Davies
13/07/2026




	Time recording

	Admin/consultations (Permit support time)
	60

	Determination (waste permitting team time)
	

	Total (to be added to PALS)
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