Phone log
Date 01/10/2025
Time of call approx. 13:45.
Call lasted approx. 15 minutes

Call between applicant: James Wright and 
Permitting officer: James Wakeford

The applicant confirmed the Vp value used to size the infiltration system was 30secs and was obtained by the company complying with BS trials process while replacing the system in 2021. 
The applicant agreed with the revised daily flow rate of 3.8m3/d and for it to rounded up to 4m3/d for ease after explanation of how that figure was reached using existing Flows and Loads 4 document. 
Explanation of possible outcomes of the application and the possible need for further information was provided by the permitting officer and how this could effect the time required to complete determination of the application.  



File note:  

The applicant is fully aware that being sole named operator on the permit they are liable for compliance with the permit irrespective of the fact all properties owners discharging to/being served by the treatment system not being named as operators on the permit. The applicant has informed the permitting officer, the other property owners are aware of this and still refused to be named on the permit. 

