Permit Number: 
JP3239ST



Operator: 

The County Council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…Apr19-L…
Reporting of ……LEACHATE…… monitoring for the period for … April 2019
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	L2
	AM Nitrogen
	904
	April 2019
	2,122
	678
	25 Apr 2019
	10.6

	L2
	Cadmium
	0.05
	April 2019
	0.78
	34
	25 Apr 2019
	7.83

	L2
	Nickel
	0.4
	April 2019
	201
	34
	25 Apr 2019
	8.82

	L2
	Chloride
	1306
	April 2019
	3,826
	678
	25 Apr 2019
	21.5

	L2
	MP Xylene
	0.032
	April 2019
	5.7
	54
	25 Apr 2019
	

	L2
	Mecoprop
	0.024
	April 2019
	<0.1
	1214
	25 Apr 2019
	14.6


	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	L4
	Am Nitrogen


	1370


	Apr 2019
	1,327
	678
	25 Apr 2019
	10.6



	L4
	Cadmium


	0.1


	Apr 2019
	<0.080
	34
	25 Apr 2019
	7.83



	L4
	Nickel


	0.1


	Apr 2019
	162
	34
	25 Apr 2019
	8.82



	L4
	Chloride


	13713


	Apr 2019
	1,745
	678
	25 Apr 2019
	21.5



	L4
	MP Xylene


	0.029


	Apr 2019
	3.4
	54
	25 Apr 2019
	

	L4
	Mecoprop


	0.032


	Apr 2019
	<0.1
	1214
	25 Apr 2019
	14.6




	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	L7
	Am Nitrogen


	1370


	Apr 2019
	NO SAMPLE
	678
	25 Apr 2019
	10.6



	L7
	Cadmium


	0.1


	Apr 2019
	NO SAMPLE
	34
	25 Apr 2019
	7.83



	L7
	Nickel


	0.1


	Apr 2019
	NO SAMPLE
	34
	25 Apr 2019
	8.82



	L7
	Chloride


	13713


	Apr 2019
	NO SAMPLE
	678
	25 Apr 2019
	21.5



	L7
	MP Xylene


	0.029


	Apr 2019
	NO SAMPLE
	54
	25 Apr 2019
	

	L7
	Mecoprop


	0.032


	Apr 2019
	NO SAMPLE
	1214
	25 Apr 2019
	14.6




The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date:  9/12/19

(Authorised to sign as representative of Operator)

