Permit Reference Number: BR7321






Operator: Tata Steel Colors


Installation: Tata Steel Colors Shotton Works




Form Number: E1

Reporting of Energy Usage for the year ……2019
	Energy Source
	Energy Usage
	CO2
Produced

(tonnes)
	
	Trends in Energy Usage

	
	Quantity
	Primary Energy

(MWh)
	
	
	Year
	Parameter

	
	
	
	
	
	
	Primary Energy usage
	CO2

produced
	CO2 per

MWh

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	2005
	662658 MWh
	127741 Tonnes
	0.193 T/MWh

	Electricity *
	MWh
	129397
	12620
	
	2006
	728829 MWh
	134225 Tonnes
	0.184 T/MWh

	Natural Gas
	GJ
	892963
	45519
	
	2007
	662742 MWh
	121571 Tonnes
	0.183 T/MWh

	Gas Oil
	Tonnes
	0
	
	
	2008
	583065 MWh
	113566 Tonnes
	0.194 T/MWh

	
	
	
	
	
	2009
	487,380 MWh
	93480 Tonnes
	0.191 T/MWh

	TOTAL
	MWh
	377442
	58139
	
	2010
	494,226 MWh
	94789 Tonnes
	0.191 T/MWh

	
	
	
	
	
	2011
	478,530 MWh
	91472 Tonnes
	0.191 T/MWh

	
	
	
	
	
	2012
	422,833 MWh
	76,541 Tonnes
	0.181 T/MWh

	
	
	
	
	
	2013
	478,857 MWh
	90,552 Tonnes
	0.189 T/MWh

	
	
	
	
	
	2014
	483,365 MWh
	91,422 Tonnes
	0.189 T/MWh

	
	
	
	
	
	2015
	432,427 MWh
	84,157 Tonnes
	0.195 T/MWh

	
	
	
	
	
	2016
	392,060 MWh
	76,820 Tonnes
	0.196 T/MWh

	
	
	
	
	
	2017
	391,879 MWh
	66,285 Tonnes
	0.169 T/MWh

	
	
	
	
	
	2018
	398,893 MWh
	61,662 Tonnes
	0.155 T/MWh

	
	
	
	
	
	2019
	377,442 MWh
	58,139 Tonnes
	0.154 T/MWh


* Conversion factor for delivered electricity to primary energy = 2.6

*1 MWh = 3.6 GJ

	Operator’s comments :

Gas and Electricity emission factors taken from UK government GHG conversion factors for companies reporting 2018.  Gas factor based on gross CV . Electricity factor based on delivered electricity for Scope 2 and Scope 3.
Oil emission factors taken from EU ETS Emissions factors




Signed ………………D. Harris…………………………………………….  

Date……23/01/2020………………..




(authorised to sign as representative of the Operator)

Installation: Tata Steel Colors Shotton Works




Form Number: WU1

Reporting of Water Usage for the year - 2019
	Water Source
	Usage

(m3)
	Specific Usage 

(m3/t)
	
	Trends in Water Usage

	
	
	
	
	Year
	Parameter

	
	
	
	
	
	Potable 

Water 
	Non-Potable 

Water  
	Water per unit output

	Mains water
	841427
	1.3
	
	
	
	
	

	Site borehole
	0
	0
	
	2004
	263,427
	1,642,412
	1.69

	River abstraction
	
	
	
	2005
	206,477
	1,191,544
	1.30

	
	
	
	
	2006
	333,940
	1,013,508
	1.17

	
	
	
	
	2007
	120,066
	881,258 (FWD)

12,341 (Boreholes)
	1.04

	TOTAL WATER USAGE
	841427
	
	
	2008
	155,875
	736,049 (FWD)

32,572 (Boreholes)
	0.91

	
	
	
	
	2009
	117,015
	494,822 (FWD)

122,823 (boreholes)
	1.10

	
	
	
	
	2010
	98,791
	539,728 (FWD)

42,786 (borehole)
	0.89

	
	
	
	
	2011
	159,408
	548,670 (FWD)
	0.93

	
	
	
	
	2012
	218,611
	448,102 (FWD)
	0.92

	
	
	
	
	2013
	134,807
	323,765 (FWD)
	0.53

	
	
	
	
	2014
	132,222
	352,316 (FWD)
	0.54

	
	
	
	
	2015
	151,154
	370,084(FWD)
	0.61

	
	
	
	
	2016
	119,101
	334,153 (FWD)
	0.70

	
	
	
	
	2017
	126518
	310004(FWD)
	0.68

	
	
	
	
	2018
	156928
	427501(FWD)
	0.9

	
	
	
	
	2019
	383,884
	457,543 (FWD)
	1.3

	Operator’s comments :

Note: Water figures are estimated for Nov and Dec 2019


Signed ………… D. Harris…………………………………………….  

Date……23/01/2020…………………..




(authorised to sign as representative of the Operator)

Installation: Tata Steel Colors Shotton Works




Form Number: R1

Reporting of Waste Disposal and Recovery for the year 2019
	Waste

Description
	Disposal
	Recovery
	
	Trends in Waste Disposal and Recovery

	
	Route
	Tonnes
	Tonnes
	
	Year
	Parameter

	
	
	
	
	
	
	Total Hazardous 

Waste
	Total Non-Hazardous

Waste
	Waste per unit output

	1) Hazardous Wastes
	
	
	
	
	2004
	1041.02
	6096.01
	0.006

	Chromate
	licenced contractor
	77.14
	0
	
	2005
	1356.52
	3800.49
	0.0049

	Oil
	licenced contractor
	39.19
	18.77
	
	2006
	1513.74
	4321.23
	0.0051

	Dry Oily Waste
	licenced contractor
	14.68
	0.55
	
	2007
	1247.52
	4003.59
	0.0049

	Solvent/paint
	licenced contractor
	1019.64
	676.74
	
	2008
	1367.9
	4182.34
	0.0055

	Batteries
	licenced contractor
	0
	0
	
	2009
	1250.569
	7380.59
	0.013

	WEEE
	licenced contractor
	3.81
	0
	
	2010
	1428.36
	10325
	0.015

	Other hazardous wastes
	licenced contractor
	470.7
	1.6
	
	2011
	1952.83
	11273
	0.015

	Total hazardous waste
	
	1625.16
	697.66
	
	2012
	1422.88
	10215.212
	0.016

	2) Non-Hazardous Wastes
	
	
	
	
	2013
	1176.11
	13091.69
	0.016

	Clinical waste
	licenced contractor
	0.55
	0
	
	2014
	1470.79
	12464.967
	0.016

	Filtercake
	licenced contractor
	19.84
	0
	
	2015
	1694.11
	11095.094
	0.015

	Office waste/ General Skip Waste
	licenced contractor
	101.86
	99.88
	
	2016
	1254.09
	9585.08
	0.017

	Construction / demolition waste
	Internal Landfill / licenced contractor
	79.8
	0
	
	2017
	945.16
	9177.146
	0.016

	Paper/cardboard/plastic
	licenced contractor
	115.52
	115.52
	
	2018
	1327.613
	8805.657
	0.016

	Zinc Dross
	licenced contractor
	530.05
	530.05
	
	2019
	1625.16
	8421.68
	0.016

	Waste Drums
	licenced contractor
	0
	0
	
	
	
	
	

	Metals
	licenced contractor
	7123.42
	7123.42
	
	
	
	
	

	Other non-hazardous wastes
	licenced contractor
	450.64
	254.69
	
	
	
	
	

	Total non-hazardous waste
	
	8421.68
	8123.56
	
	
	
	
	

	Total Haz & non-hazardous waste
	
	10046.84
	8821.22
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	TOTAL WASTE
	
	
	
	
	
	
	
	


Signed ……………… D. Harris…………………………………………….  

Date……23/01/2020…………………..
(authorised to sign as representative of the Operator)

Installation: Tata Steel Colors Shotton Works




Form Number: PI1

Reporting of Performance Indicators for the year  2019
	Annual Production/Treatment

	Production of galvanised steel product
	357432 tonnes

	Production of colour coated steel product 
	285243  tonnes

	Total Production of coated steel products
	642675 tonnes


Environmental Performance Indicators

	Parameter
	Annual Average
	Units
	
	Trends in Environmental Performance

	
	
	
	
	Year
	Parameter

	
	
	
	
	
	Total VOC / tonne 
	% VOC Fugitives
	Primary Energy / tonne

	Primary Energy Use 
	0.59
	MW-hr /  tonne
	
	
	
	
	

	Total VOC Emission to Air (as Carbon)
	0.15
	Kg /  tonne
	
	2004
	0.13
	2.75
	0.66

	VOC Fugitive Emission Value
	3.19
	%
	
	2005
	0.145
	2.83
	0.615

	Potable Water Use
	0.59
	m3 / tonne
	
	2006
	0.137
	2.87
	0.635

	Non-Potable Water Use
	0.71
	m3 / tonne
	
	2007
	0.15
	2.92
	0.620

	Quantity of Hazardous Waste
	2.53
	Kg / tonne
	
	2008
	0.05
	2.43
	0.65

	Quantity of Non-Hazardous Waste
	13.1
	Kg / tonne
	
	2009
	0.157
	9.11
	0.73

	
	
	
	
	2010
	0.159
	10.2
	0.65

	
	
	
	
	2011
	0.07
	4.86
	0.61

	
	
	
	
	2012
	0.05
	3.13
	0.59

	
	
	
	
	2013
	0.05
	3.57
	0.561

	
	
	
	
	2014
	0.07
	4.87
	0.54

	
	
	
	
	2015
	0.07
	4.57
	0.50

	
	
	
	
	2016
	0.07
	3.88
	0.60

	
	
	
	
	2017
	0.06
	3.1
	0.62

	
	
	
	
	2018
	0.1
	5.44
	0.62

	
	
	
	
	2019
	0.15
	3.19
	0.59

	Operator’s comments :


Signed …………… D. Harris…………………………………………….  

Date……23/01/2020…………………..
(authorised to sign as representative of the Operator)

