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	Consent no
	NRWWIA179

	
	


WATER INDUSTRY ACT 1991

SECTION 165 / 166
CONSENT TO DISCHARGE

TO:
Dŵr Cymru Cyfyngedig


Pentwyn Road


Nelson


Treharris


Mid Glamorgan


CF46 6LY
	The NATURAL RESOURCES BODY FOR WALES ("Natural Resources Wales") in pursuance of its powers under the Water Industry Act 1991 HEREBY CONSENTS to the making of a discharge as follows:
Raw Water 


	FROM: Marchlyn Bach Reservoir, near Llanberis, LL55 4UN

	

	AT: NATIONAL GRID REFERENCE SH 60774 62577

	

	TO: Afon Marchlyn Bach

	

	SUBJECT TO: the conditions set out in the following schedule:

Raw Water                     Schedule No. NRWWIA179

	

	This consent is issued on the 4th day of February 2020
This consent takes effect on the 4th day of February 2020
This consent shall cease to have effect on the 14th day of August 2020
Signed:
Amy Nethercott

	


CONDITIONS OF CONSENT TO DISCHARGE

RAW WATER (“the Discharge”)

NATURE OF THE DISCHARGE

1.
The Discharge shall consist solely of raw water. 

SOURCE OF THE DISCHARGE

2. The Discharge shall be derived from Marchlyn Bach Reservoir.
LOCATION OF DISCHARGE

3.
The location of the Discharge shall be at NGR SH 60659 62698, marked ‘LOCATION WHERE FLOWS ENTER WATERCOURSE’ on the site plan in Annex 1.

SAMPLE POINT

4.
A sample point shall be provided and maintained so that a representative sample of the Discharge may be obtained. 

VOLUME

5. The total volume of the Discharge shall not exceed 161,000 cubic metres.

6. The total daily volume of the Discharge shall not exceed 864 cubic metres.
7. The rate of the Discharge shall not exceed 10 litres per second.
COMPOSITION

8.
The consent holder shall take all necessary steps to secure that any water discharged by it under this consent is as free as may be reasonably practicable from — 

(a) 
mud and silt;

(b) 
solid, polluting, offensive or injurious substances; 
and

(c)
any substances prejudicial to fish or spawn, or to spawning beds or food of fish.
SCOURING
9.
The rate of discharge shall be controlled to prevent any significant scouring of the bed or bankside of the receiving water as in line with Environmental Risk Assessment and Management System dated 06/10/2015 and submitted as part of the application of consent and approved by NRW.
FLOODING

10.
The discharge shall not cause or significantly contribute to flooding in the downstream catchment.
PERIOD OF DISCHARGE

11.
The Discharge shall only be made between 4th day of February 2020 and the 14th day of August 2020.
ANNEX 1- PLAN No. NRWWIA179
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