Permit Number: 
EPR/BL1096IB




Operator: 
Castle Cement Limited
Installation:

Padeswood Cement Works


Form Number: Process Waste 1 

Date : 30/01/20
6-Monthly reporting of Cement Kiln 4 by-pass dust composition for the period from:          
01/07/2019 to 31/12/2019
	Cement kiln 4 by-pass dust composition (Metals, Dioxins, etc.)

	
	Sb mg/kg
	Cd mg/kg
	TI

mg/kg
	Hg

mg/kg
	Pb

mg/kg
	Cr

mg/kg
	Cu

mg/kg
	Mn

mg/kg
	Ni

mg/kg
	As

mg/kg
	Co

mg/kg
	V

mg/kg 
	Zn

mg/kg
	DIOXIN /FURAN         I-TEQ

ng/kg
	DIOXIN / FURAN
	DIOXIN-LIKE PCBs
	HALIDES

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	WHO-TEQ ng/kg
	WHO-TEQ ng/kg
	%

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	Humans / mammals
	Birds
	Fish
	Humans / mammals
	Birds
	Fish
	Chloride
	Bromide
	Fluoride

	Cement Kiln 4 by-pass dust
	144
	105
	12
	33
	467
	140
	2980
	303
	109
	142
	107
	18
	3500
	4.98
	4.64
	14.5
	5.2
	0.17
	0.571
	0.0092
	0.64
	<0.0001
	<0.0001


The following reporting is required before use of a new disposal route for Cement Kiln 4 by-pass dust

Reporting of Total Soluble Fraction for the period from:          

01/0 to DD/MM/YYYY
	Total Soluble Fraction (Free Lime & Metals)

	
	Free Lime

%
	Sb mg/kg
	Cd mg/kg
	TI

mg/kg
	Hg

mg/kg
	Pb

mg/kg
	Cr

mg/kg
	Cu

mg/kg
	Mn

mg/kg
	Ni

mg/kg
	As

mg/kg
	Co

mg/kg
	V

mg/kg
	Zn

mg/kg

	Cement Kiln 4 by-pass dust
	
	
	
	
	
	
	
	
	
	
	
	
	
	


Signed ………………Stewart Mitchell……………….  

Date………30/01/2020……..   


(Authorised to sign as representative of Castle Cement Limited) 

