AB CONNECTORS
PC 4.1.4
Review of Fugitive Emissions

January to December 2019
Permit Number BV7443IP

Annual Review of Fugitive Emissions

Previous 12 months January to December 2018
No fugitive emissions reported

January to December 2019
No fugitive releases reported

2019 Environmental Incident Reports
15/02/2019 - Smoke coming from flat screen monitor in Assembly area. Power disconnected and      equipment checked for fire damage. All other monitors checked. Manufacturer informed of fault
15/02/2019 – Leak from discharge valve of Nitric Acid IBC. Leak absorbed using chemical absorbent matting. Slight staining to paint on walkway in Machine Shop

29/04/2019 – Air recirculation fan on oven in Assembly Area overheated and caught fire. Fire put out with extinguisher 

27/08/2019 – Water based coolant spilled onto the floor of the Machine Shop whilst being topped up. Spillage contained within the Machine Shop area and cleaned up using wet/dry vac and absorbent material.

04/11/2019 – Oil mist fire (flash) in Bumotec 4 whilst turning Aluminium Bronze material. Fire extinguished itself
Trade effluent and Stack Emission Results 2019
Emissions to sewer and stack emissions within permitted limits

Reviews and Improvements to Further Minimise the Risk of Fugitive Emissions

· New storage facility for flammable chemicals installed 

· New caged area for storage of gas bottles.

· Entry to all external doors now controlled by a card key entry system
· New  bund purchased for storage of oil and coolant in the Machine shop
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New Bund for storage of oil in Machine Shop                    
















