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Notice of variation and consolidation with introductory note
The Environmental Permitting (England & Wales) Regulations 2016

Dŵr Cymru Cyfyngedig

Stormy Down Sewage Treatment Works
Stormy Down
Pyle
Bridgend 
CF32 0NP


Variation application number
PAN-010505
Permit number
BB4018701






Stormy Down Sewage Treatment Works
Permit number BB4018701
Introductory note
This introductory note does not form a part of the notice.

The following notice gives notice of the variation and consolidation of an environmental permit.

Following an NRW groundwater review of the existing permit this variation notice changes the conditions to ensure compliance with the Environmental Permitting (England and Wales) Regulations 2016 (‘the Regulations’). The operator has confirmed sewage effluent discharge volumes of 28m3 per day, serving a population equivalent of 33. 

The schedules specify the changes made to the permit.

The status log of a permit sets out the permitting history, including any changes to the permit reference number.  It is not backdated before 6 April 2010. 

	Status log of the permit

	Description
	Date
	Comments

	NRW initiated variation PAN-010505
(variation and consolidation)
	Duly made
22/05/2020
	Groundwater review to vary and update the permit to modern conditions.

	Variation determined BB4018701
	14/07/2020
	Varied and consolidated permit issued in modern condition format.




End of introductory note
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Notice of variation and consolidation 


The Environmental Permitting (England and Wales) Regulations 2016

[bookmark: _Hlt13295849][bookmark: OperatorName2]The Natural Resources Body for Wales (“Natural Resources Wales”) in exercise of its powers under regulation 20 of the Environmental Permitting (England and Wales) Regulations 2016 varies and consolidates

permit number
BB4018701

issued to:
Dŵr Cymru Cyfyngedig (“the operator”)

whose principal office is

Pentwyn Road
Nelson
Treharris
Caerphilly
CF46 6LY

[bookmark: _Hlk43099194]company registration number 02366777 

[bookmark: _Hlk42509082]to operate a regulated facility at

Stormy Down Sewage Treatment Works
Stormy Down
Pyle
Bridgend 
CF32 0NP 


to the extent set out in the schedules.


The notice shall take effect from 14/07/2020

	Name
	Date

	Melissa Broad
	14/07/2020



Authorised on behalf of Natural Resources Wales

Schedule 1 
All conditions have been varied by the consolidated permit as a result of a Natural Resources Wales initiated variation.


Schedule 2 – consolidated permit
Consolidated permit issued as a separate document. 






	
Permit


The Environmental Permitting (England and Wales) Regulations 2016

Permit number 
BB4018701
This is the consolidated permit referred to in the variation and consolidation notice for application PAN-010505 authorising, 

Dŵr Cymru Cyfyngedig (“the operator”),
whose principal office is

Pentwyn Road
Nelson
Treharris
Caerphilly
CF46 6LY
 

company registration number 02366777 
to operate a groundwater activity

Stormy Down Sewage Treatment Works
Stormy Down
Pyle
Bridgend 
CF32 0NP 

to the extent authorised by and subject to the conditions of this permit.

Authorised on behalf of Natural Resources Wales


	Name
	Date

	Melissa Broad
	14/07/2020



Authorised on behalf of Natural Resources Wales




[bookmark: _Toc392252823]	


Conditions
Management
0. [bookmark: _Ref373938749]General management
[bookmark: _Ref373938830]The operator shall manage and operate the activity:
in accordance with a written management system that identifies and minimises risks of pollution so far as is reasonably practicable, including those risks arising from operations, maintenance, accidents, incidents, non-conformances and those drawn to the attention of the operator as a result of complaints; and
using sufficient competent persons and resources.
Records demonstrating compliance with condition 1.1.1 shall be maintained. 
Any person having duties that are or may be affected by the matters set out in this permit shall have convenient access to a copy of the permit.
Operations
Permitted activities
The only activity authorised by the permit is the activity specified in schedule 1 table S1.1.
The site 
The groundwater activity shall take place at the discharge point marked on the site plan at schedule 7 to this permit, and as listed in table S3.2. 
Emissions and monitoring
Emissions to water or land
The limits given in schedule 3 table S3.1 shall not be exceeded.
 
For the emission limits in schedule 3 table S3.1 to which this condition applies, no inspection of the discharge made at a time when unusual weather conditions are adversely affecting the operation of the waste water treatment works, shall be taken into account in deciding whether or not the emission limit has been complied with.
On any occasion where unusual weather conditions adversely affect the operation of the waste water treatment works, the operator shall use its best endeavours to mitigate that adverse effect.
For any inspection of the discharge to be considered for the purposes of (a) above, the operator shall notify Natural Resources Wales in writing within 14 days of becoming aware that an emission limit has been exceeded. That notification shall include a full description of the unusual weather conditions and their impact on the operation of the works.

Emissions of substances not controlled by emission limits
For the activity referenced in schedule 1, table S1.1 the operator shall take appropriate measures as far as is reasonably practicable:
to prevent the input of hazardous substances to groundwater; and
where a non-hazardous pollutant is not controlled by an emission limit, to limit the input of such non-hazardous pollutants to groundwater so as to ensure that inputs do not cause pollution of groundwater. 
Monitoring 
An Accessible monitoring point(s) shall be provided and maintained to enable the emissions monitoring programme [and the environmental or other monitoring] to be carried out at the monitoring point specified in table S3.2 and S3.3 of schedule 3 and shown marked on the site plan(s) in schedule 7
Information
Records
All records required to be made by schedule 3, 4 and 5 to this permit shall:
be legible;
be made as soon as reasonably practicable;
if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and
be retained, unless otherwise agreed in writing by Natural Resources Wales, for at least 6 years from the date when the records were made. 
The operator shall maintain convenient access, in either electronic or hard copy, to the records, plan and management system required to be maintained by this permit. 
Reporting
The operator shall send all reports and notifications required by the permit to Natural Resources Wales using the contact details supplied in writing by Natural Resources Wales.
Notifications
Natural Resources Wales shall be notified as soon as reasonably practicable following detection, within the site of the regulated facility of:
any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution; and
any breach of a limit specified in schedule 3 table S3.1.
Any other significant adverse environmental effects, which may have been caused by the activity, shall also be notified to Natural Resources Wales as soon as reasonably practicable following detection.
The information provided under condition 4.3.1 shall be supported by sending the information listed in schedule 5 to this permit within the time period specified in that schedule.
Natural Resources Wales shall be notified within 14 days of the occurrence of the following matters, except where such disclosure is prohibited by Stock Exchange rules:
Where the operator is a registered company:
any change in the operator’s trading name, registered name or registered office address; and
any steps taken with a view to the operator going into administration, entering into a company voluntary arrangement or being wound up.
Where the operator is a corporate body other than a registered company:
(a) any change in the operator’s name or address; and
any steps taken with a view to the dissolution of the operator.
Where the operator proposes to make a change in the nature of the activity by increasing the concentration of, or the addition of, or allowing the introduction of, a substance to the activity to an extent that the operator considers could have a significant adverse environmental effect on the receiving waters, and the change is not the subject of an application for approval under the EP Regulations or under the terms of this permit:
Natural Resources Wales shall be notified in writing at least 14 days before the increase or addition or allowing the introduction; and
the notification shall contain a description of the proposed change.
Interpretation
In this permit the expressions listed in schedule 6 shall have the meaning given in that schedule.
In this permit references to reports and notifications mean written reports and notifications, except where reference is made to notification being made “as soon as reasonably practicable”, in which case it may be provided by telephone.


Schedule 1 – Operations 

	Table S1.1 Activities

	Activity reference
	Description of activity
	Limits of specified activity

	A1
	Groundwater activity: discharge of secondary treated sewage effluent into underground strata
	Via an infiltration system (Reed Bed) into underground strata located at NGR: SS 84646 79851









































Schedule 2 – Waste types, raw materials and fuels

Schedule 2 not in use.




Permit number
BB4018701
	9
Schedule 3 – Emissions and monitoring

	Table S3.1 Point Source emissions to water (other than sewer) and land – emission limits and monitoring requirements

	Effluent(s) and discharge point(s)
	Parameter  
	Limit (including unit)
	Reference Period
	Monitoring method
	Limit of effective range
	Monitoring frequency
	Compliance Statistic

	A1 Secondary treated sewage effluent via Outlet 1
	Maximum daily flow
	28 m3/day
	Total daily volume
	N/A
	N/A
	N/A
	Maximum

	A1 Reed bed via Outlet 1
	
Visible oil or grease

	No significant trace present so far as is reasonably practicable
	Instantaneous (visual examination)
	Visual examination
	N/A
	N/A
	No significant trace
(Condition 3.1.2 applies)



	Table S3.2 Discharge points

	Effluent Name
	Discharge Point
	 Discharge point NGR
	Receiving water/Environment

	Sewage Effluent
	Outlet 1
	NGR: SS 84646 79851
	Groundwater via reed bed system



	Table S3.3 Monitoring points

	Effluent(s) and discharge point(s)
	Monitoring type
	Monitoring point NGR
	Monitoring point reference

	Sewage effluent via Outlet 1
	Effluent sampling
	NGR: SS 84646 79851
	 Sample Point















Schedule 4 – Reporting
Schedule 4 not in use.




Schedule 5 – Notification 1
These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.
Part A
	Permit Number
	BB4018701

	Name of operator
	

	Location of Facility
	Stormy Down Sewage Treatment Works, Stormy Down, Pyle, Bridgend, CF32 0NP 

	Time and date of the detection 
	



	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 7 days of detection  

	Date and time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released/type or nature of sewage released
	

	Best estimate of the quantity or rate of release of substances and/or duration of discharge
	

	Best estimate of the environmental impact of the discharge
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	



	(b) Notification requirements for the breach of a limit specified in schedule 3 table S3.1

	To be notified within 7 days of detection unless otherwise agreed in writing by Natural Resources Wales

	Description of where the effect on the environment was detected
	

	Description of and best estimate of the scale of environmental impact of the discharge
	



Part B – to be submitted as soon as reasonably practicable unless otherwise agreed in writing by Natural Resources Wales
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident/breach/exceedance
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	



	Name*
	

	Post
	

	Signature
	

	Date
	


* authorised to sign on behalf of the operator

Schedule 6 – Interpretation 
 “accident” means an accident that may result in pollution.

"annually" means once every year.

“application” means the application for this permit, together with any additional information supplied by the operator as part of the application and any response to a notice served under Schedule 5 to the EP Regulations.

“Dry weather flow” (DWF), measured as m3/d, is defined as follows: DWF = PG + IDWF + E, where P = population in the catchment, G = per capita domestic sewage flow, IDWF = dry weather infiltration, and E = trade effluent flow.

“appropriate measures” for the purposes of the emission of substances not controlled by emission limits condition (condition 3.2.1) do not require the operator to undertake treatment to a level beyond that specified in schedule 1 table S1.1, or to carry out routine monitoring for substances not controlled by emission limits.

“emissions of substances not controlled by emission limits” means emissions of substances to air, water or land from the permitted activities, which are not controlled by an emission limit.

“emissions to land” includes emissions to groundwater.

“EP Regulations” means The Environmental Permitting (England and Wales) Regulations SI 2016 No.1154 and words and expressions used in this permit which are also used in the Regulations have the same meanings as in those Regulations.

“groundwater” means all water, which is below the surface of the ground in the saturation zone and in direct contact with the ground or subsoil.

“Natural Resources Wales” means the Natural Resources Body for Wales established by article 3 of the Natural Resources Body for Wales (Establishment) Order 2012. The Natural Resources Body for Wales (Functions) Order 2013 transferred the relevant functions of the Countryside Council for Wales, and functions of the Environment Agency and the Forestry Commission in Wales to the Natural Resources Body for Wales.

"quarter" means a calendar year quarter commencing on 1 January, 1 April, 1 July or 1 October.

“significant pollution” means a high level impact incident as indicated by NRW incident classification system.

“unusual weather conditions” includes, but is not limited to:
low ambient temperatures, or the freezing of mechanical equipment in the works;
significant snow deposits;
tidal or fluvial flooding;
weather conditions causing unforeseen loss of power supply to the sewage treatment that could not be ameliorated by the reasonable provision and operation of standby generation facilities.
 “year” means calendar year ending 31 December.


Schedule 7 – Site plan

[image: ]



© Crown Copyright and database right 2020. Ordnance Survey licence number 100019741.



END OF PERMIT
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