[bookmark: _GoBack]Schedule 5 - Notification
These pages outline the information that the operator must provide.

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part A
	Permit Number
	 EPR/BL1096IB/V014

	Name of operator
	 Castle Cement Limited

	Location of Facility
	 Padeswood Works, Padeswood, Mold.

	Time and date of the detection
	20:15 10/07/2020



	(a) Notification requirements for any activity that gives rise to an incident or accident which significantly affects or may significantly affect the environment

	                                                  To be notified within 24 hours

	Date and time of the event
	20:15 10/07/2020

	Reference or description of the location of the event
	Packing Bay silo1

	Description of where any release into the environment took place
	Penthouse above silo 1, emission to air

	Substances(s) potentially
released
	Cement  

	Best estimate of the quantity or rate of release of substances
	10kg

	Measures taken, or intended to
be taken, to stop any emission
	Blow line stopped. Seal identified. Route to silo forced out to stop use. Repairs planned 

	Description of the failure or
accident.
	Gasket failure on blow line



	(b) Notification requirements for the breach of a permit condition

	                                                  To be notified within 24 hours

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	



	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	



Permit Number: EPR/BL1096IB
Page 2
19/07/16

	
	

	
	



	(c) In the event of a breach of permit condition which poses an immediate danger to human health
or threatens to cause an immediate significant adverse effect on the environment:

	To be notified immediately

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	




Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	On further inspection it was identified that the valve at the point of the leak had worn and this resulted in the emission to air. The value was installed as part of the VRM project and has been operational for approximately 18 months. The line and valve is used when making packed products.


	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	The valve has been replaced and a preventive maintenance schedule has been created to inspect on a quarterly frequency. As the valve was installed in September 2020 the first inspection will be completed during December 2020. Similar valve are also included within the preventative maintenance.


	Measures taken, or intended to be taken, to rectify,
limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	27/07/2018
04/08/2018
16/08/2018
21/08/2018
18/09/2018
17/12/2018
05/01/2019
22/03/2019
29/03/2019
15/08/2019
29/08/2019
21/09/2019
23/10/2019
28/10/2019
15/12/2019
23/12/2019
09/02/2020
07/03/2020
23/04/2020
26/04/2020



	Name*
	Stewart Mitchell

	Post
	Quality and Environment Manager

	Signature
	S. Mitchell

	Date
	17/12/2020


* authorised to sign on behalf of the operator
