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OWNER/OCCUPIER – NOTICE OF INTENTION TO CARRY OUT OR PERMIT AN OPERATION LIKELY TO DAMAGE SPECIAL INTEREST ON A SITE OF SPECIAL SCIENTIFIC INTEREST (SSSI)

This form should be used by owners and occupiers of SSSI intending to carry out, or give permission for someone else to carry out, one or more activities listed on the list of Operations Likely to Damage the Special Interest (OLDSI list) for the site. On older sites this will be called the PDO list.
	Name of SSSI 
	Dyfi SSSI


I/We hereby give notice under Section 28E (1) of the Wildlife and Countryside Act 1981 that I/we intend to carry out, cause or permit to be carried out the operation(s) specified below:-

	1.
	Details of proposed operation. Attach method statements, photographs or diagrams if these will help to explain your proposals. (Operations may be changes in management practices)

	YGC were commissioned to produce a Habitats Regulations Assessment (HRA) for the works of replacement defective timbers and associated metal works at Leri Viaduct Ynys Las, Borth, Ceredigion (Grid Reference SN61667 – 92957) as described below: 

The viaduct is 89m long and is constructed of timber heart wood. Recent investigation works have found some timbers have become rotten and need replacing. The contractors plan will consider the safety and wellbeing of all working on the structure, and the people who live and work in the area.

As always rail passengers come first and because of this we will be carrying out as much preparatory work as possible while passenger trains are still running as not to cause disruption. The main blockade, consisting of a 53 hour possession of the line in week 24, this is where the main structural elements of the works will be completed.

Leri viaduct is a grade II* listed structure on the SBA2 line between Dyfi junction station and Aberystwyth, which runs over the tidal river AFON LERI. It is an 8-trestle bridge which has a newer GRP public footpath attached to the upside of the structure, this is attached along the extended crossheads and bolted to the top.

A significant amount of wailer removals, pile replacements and steel repairs are required along with new corbels at certain locations.

The contractor will successfully deliver this project using their own internal plant including Road Rail Vehicles (RRVs) and a highly skilled workforce who have already proved themselves on other similar wooden structures in the area on the same line.

A dive team will be required for most of these works due to the area being in a tidal estuary.

All of the above combined will reduce any risk of an overrun to the possession and the project program timescale.

Key dates: 

Site set up
1st to 12th March, including access across field 

Prep/doubler works including scaffold 15th March to 26th March
Wailing Doubler removal possessions 8th March to 26th March Midweek and sat nights

Main Possession
Sat morn 27th to Mon morn 29th March 2021(24/7)

Removal of scaffold/snagging
29th March to 16th April

Snagging/removal of material poss
Sat nights; 3rd 10th and 17th April
Site demob
19th to 26th April
Please extend the end date for 6 months incase of isses on site.


	2.
	I/We intend to carry out this operation on the area of land detailed on the enclosed

	
	YGC have been commissioned to complete the Environmental Appraisal, HRA and Marine Licence and Section 28 consent for works within SSSI for Alun Griffiths Contractors on behalf of Network Rail.  

Leri Viaduct Ynys Las, Borth, Ceredigion (Grid Reference SN61667 – 92957). The six number co-ordinates for each corner of the bridge is: 268771-296629, 268772-296626, 268794-296633, 268795-296628
Please see Initial Environmental Appraisal Document Appendix for map of location.



	
	Please see Initial Environmental Appraisal Document Appendix for site photographs and method statement for whote details of the works.


* Tick as appropriate

You must supply enough information to allow us to locate the land where you wish to carry out the work. If your notice does not specify where the operation will take place we will be unable to accept it. An annotated map is most helpful. Please also include details of any relevant secondary works, such as access routes, material storage or disposal locations.
	3
	I/We propose to start the operation (or implement the changes) on/after
	1st March (site setup on hard standing NR Compound)


	
	Work will continue until (if there is no end date strike out this section)
	End April 2021 but extend until October 2021. 



	Note: Only owners and occupiers of the site can apply for consent. If you are not the owner or occupier, you will need to ask them for permission. The owner or occupier will then need to notify us and get consent before they give you permission.



	Name:
	Mr Andrew Mc Monagle

	Address :
	Alun Griffiths (Contractor) Ltd

Waterways House

Merthyr Road

Llanfoist

Abergavenny

Monmouthshire

NP7 9PE
Gareth Yates
Floor 2

St Patrick’s House 
Penarth Road 
Cardiff. CF10 5ZA gareth.yates@networkrail.co.uk


D +44 1492 542 223

 M +44 7919 307 779

	
	


	 Andrew.mcmonagle@alungriffiths.co.uk 

	

	Date:
	18/12/2020


Natural Resources Wales must process your application within 4 months of receipt of a duly made notice. We will usually be able to respond much more quickly than this if sufficient information is included.
Please return to SSSI.notices@cyfoethnaturiolcymru.gov.uk  or your local Natural Resources Wales office. 
