Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…Sep 20 - L…
Reporting of ……LEACHATE…… monitoring for the period for … September 2020
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	
	
	
	
	
	
	
	

	L2
	Am Nitrogen
	904
	Sep-20
	1,230
	INORG-L12
	30th Sep 20
	12.69



	
	
	
	
	
	
	
	

	L2
	Cadmium
	0.05
	Sep-20
	<0.080
	1450
	30th Sep 20
	3.93

	
	
	
	
	
	
	
	

	L2
	Nickel
	0.4
	Sep-20
	211
	METALS-L
	30th Sep 20
	5.23


	
	
	
	
	
	
	
	

	L2
	Chloride
	1306
	Sep-20
	1,533
	INORG-L13
	30th Sep 20
	6.71



	
	
	
	
	
	
	
	

	L2
	MP Xylene
	0.032
	Sep-20
	2.9
	ORG-LO5
	30th Sep 20
	7.66



	
	
	
	
	
	
	
	

	L2
	Mecoprop
	0.024
	Sep-20
	9.6
	ORG-L17
	30th Sep 20
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	 
	Am Nitrogen
	1370
	Sep-20
	1,200
	INORG-L12
	30th Sep 20
	12.69



	L4
	
	
	
	
	
	
	

	 
	Cadmium
	0.1
	Sep-20
	<0.080
	1450
	30th Sep 20
	3.93

	L4
	
	
	
	
	
	
	

	 
	Nickel
	0.1
	Sep-20
	179
	METALS-L
	30th Sep 20
	5.23


	L4
	
	
	
	
	
	
	

	 
	Chloride
	13713
	Sep-20
	1,540
	INORG-L13
	30th Sep 20
	6.71



	L4
	
	
	
	
	
	
	

	 
	MP Xylene
	0.029
	Sep-20
	9.4
	ORG-LO5
	30th Sep 20
	7.66



	L4
	
	
	
	
	
	
	

	 
	Mecoprop
	0.032
	Sep-20
	43.1
	ORG-L17
	30th Sep 20
	8.27



	L4
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	 
	Am Nitrogen
	1370
	Sep-20
	190
	INORG-L12
	30th Sep 20
	12.69



	L7
	
	
	
	
	
	
	

	 
	Cadmium
	0.1
	Sep-20
	-
	1450
	30th Sep 20
	3.93

	L7
	
	
	
	
	
	
	

	 
	Nickel
	0.1
	Sep-20
	34.6
	METALS-L
	30th Sep 20
	5.23


	L7
	
	
	
	
	
	
	

	 
	Chloride
	13713
	Sep-20
	444
	INORG-L13
	30th Sep 20
	6.71



	L7
	
	
	
	
	
	
	

	 
	MP Xylene
	0.029
	Sep-20
	-
	ORG-LO5
	30th Sep 20
	7.66



	L7
	
	
	
	
	
	
	

	 
	Mecoprop
	0.032
	Sep-20
	-
	ORG-L17
	30th Sep 20
	8.27



	L7
	
	
	
	
	
	
	


The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date……13/11/20……     



(Authorised to sign as representative of Operator)

