Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
…Aug 20 - L…
Reporting of ……LEACHATE…… monitoring for the period for … August 2020
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	
	
	
	
	
	
	
	

	L2
	Am Nitrogen
	904
	Aug-20
	1,246
	INORG-L12
	28th Aug 20
	12.69



	
	
	
	
	
	
	
	

	L2
	Cadmium
	0.05
	Aug-20
	0.38
	1450
	28th Aug 20
	3.93

	
	
	
	
	
	
	
	

	L2
	Nickel
	0.4
	Aug-20
	201
	METALS-L
	28th Aug 20
	5.23


	
	
	
	
	
	
	
	

	L2
	Chloride
	1306
	Aug-20
	1660
	INORG-L13
	28th Aug 20
	6.71



	
	
	
	
	
	
	
	

	L2
	MP Xylene
	0.032
	Aug-20
	<1.0
	ORG-LO5
	28th Aug 20
	7.66



	
	
	
	
	
	
	
	

	L2
	Mecoprop
	0.024
	Aug-20
	17.7
	ORG-L17
	28th Aug 
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	 
	Am Nitrogen
	1370
	Aug-20
	1,244
	INORG-L12
	28th Aug 20
	12.69



	L4
	
	
	
	
	
	
	

	 
	Cadmium
	0.1
	Aug-20
	<0.08
	1450
	28th Aug 20
	3.93

	L4
	
	
	
	
	
	
	

	 
	Nickel
	0.1
	Aug-20
	180
	METALS-L
	28th Aug 20
	5.23


	L4
	
	
	
	
	
	
	

	 
	Chloride
	13713
	Aug-20
	1,560
	INORG-L13
	28th Aug 20
	6.71



	L4
	
	
	
	
	
	
	

	 
	MP Xylene
	0.029
	Aug-20
	13
	ORG-LO5
	28th Aug 20
	7.66



	L4
	
	
	
	
	
	
	

	 
	Mecoprop
	0.032
	Aug-20
	36.3
	ORG-L17
	28th Aug 
	8.27



	L4
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	 
	Am Nitrogen
	1370
	Aug-20
	180
	INORG-L12
	28th Aug 20
	12.69



	L7
	
	
	
	
	
	
	

	 
	Cadmium
	0.1
	Aug-20
	-
	1450
	28th Aug 20
	3.93

	L7
	
	
	
	
	
	
	

	 
	Nickel
	0.1
	Aug-20
	43.6
	METALS-L
	28th Aug 20
	5.23


	L7
	
	
	
	
	
	
	

	 
	Chloride
	13713
	Aug-20
	455
	INORG-L13
	28th Aug 20
	6.71



	L7
	
	
	
	
	
	
	

	 
	MP Xylene
	0.029
	Aug-20
	<1.0
	ORG-LO5
	28th Aug 20
	7.66



	L7
	
	
	
	
	
	
	

	 
	Mecoprop
	0.032
	Aug-20
	-
	ORG-L17
	28th Aug 
	8.27



	L7
	
	
	
	
	
	
	


The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date……13/11/20……     



(Authorised to sign as representative of Operator)

