Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
……
Reporting of ……LEACHATE…… monitoring for the period for … October 2020
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	
	
	
	
	
	
	
	

	L2
	Am Nitrogen
	904
	Oct-20
	1200
	INORG-L12
	23rd Oct 20
	12.69



	
	
	
	
	
	
	
	

	L2
	Cadmium
	0.05
	Oct-20
	<0.08
	1450
	23rd Oct 20
	3.93

	
	
	
	
	
	
	
	

	L2
	Nickel
	0.4
	Oct-20
	224
	METALS-L
	23rd Oct 20
	5.23


	
	
	
	
	
	
	
	

	L2
	Chloride
	1306
	Oct-20
	1469
	INORG-L13
	23rd Oct 20
	6.71



	
	
	
	
	
	
	
	

	L2
	MP Xylene
	0.032
	Oct-20
	9.9
	ORG-LO5
	23rd Oct 20
	7.66



	
	
	
	
	
	
	
	

	L2
	Mecoprop
	0.024
	Oct-20
	15.3
	ORG-L17
	23rd Oct 20
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	 
	Am Nitrogen
	1370
	Oct-20
	1200
	INORG-L12
	23rd Oct 20
	12.69



	L4
	
	
	
	
	
	
	

	 
	Cadmium
	0.1
	Oct-20
	<0.08
	1450
	23rd Oct 20
	3.93

	L4
	
	
	
	
	
	
	

	 
	Nickel
	0.1
	Oct-20
	207
	METALS-L
	23rd Oct 20
	5.23


	L4
	
	
	
	
	
	
	

	 
	Chloride
	13713
	Oct-20
	1437
	INORG-L13
	23rd Oct 20
	6.71



	L4
	
	
	
	
	
	
	

	 
	MP Xylene
	0.029
	Oct-20
	27
	ORG-LO5
	23rd Oct 20
	7.66



	L4
	
	
	
	
	
	
	

	 
	Mecoprop
	0.032
	Oct-20
	26.6
	ORG-L17
	23rd Oct 20
	8.27



	L4
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	 
	Am Nitrogen
	1370
	Oct-20
	190
	INORG-L12
	23rd Oct 20
	12.69



	LTP1
	
	
	
	
	
	
	

	 
	Cadmium
	0.1
	Oct-20
	-
	1450
	23rd Oct 20
	3.93

	LTP1
	
	
	
	
	
	
	

	
	Nickel
	0.1
	Oct-20
	45.6
	METALS-L
	23rd Oct 20
	5.23


	LTP1
	
	
	
	
	
	
	

	
	Chloride
	13713
	Oct-20
	400
	INORG-L13
	23rd Oct 20
	6.71



	LTP1
	
	
	
	
	
	
	

	
	MP Xylene
	0.029
	Oct-20
	-
	ORG-LO5
	23rd Oct 20
	7.66



	LTP1
	
	
	
	
	
	
	

	LTP1
	Mecoprop
	0.032
	Oct-20
	-
	ORG-L17
	23rd Oct 20
	8.27



	
	
	
	
	
	
	
	


The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………………………Gareth Ffoulkes………………………………….  

Date…………27/01/21



(Authorised to sign as representative of Operator)

