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Notice of variation with introductory note
Environmental Permitting (England & Wales) Regulations 2016

Morganite Electrical Carbon Limited

Electrical Carbon, Swansea
Upper Fforest Way 
Morriston
Swansea 
SA6 8PP

Variation number
[bookmark: _Hlk72922700]EPR/VP3339PD/V012
Permit number
EPR/VP3339PD




Electrical Carbon, Swansea
Permit number EPR/VP3339PD
Introductory note
This introductory note does not form a part of the notice

The following notice gives notice of the variation of an environmental permit.

The variation is to change the abatement for the emission point A15. The new abatement is a horizontal deep bed filter which is to replace the wet scrubber that had previously used as abatement for this emission point. The new abatement plant also replaces the stack reducing the stack height from 12 meters to 4 meters. As a result the variation has reduced the emission limit value of particulate matter and Benzo-a-pyrene for A15 from 5 mg/Nm3 and 0.01mg/Nm3 (respectfully) to 4 mg/Nm3 and 0.005 mg/Nm3.

[bookmark: _Hlk73606450]Conditions 3.1.1, 3.5.1 and 3.5.4 have also been updated to removed the reference to table S3.3 which was removed as part of a previous variation (V010).

The schedules specify the changes made to the original permit.

The status log of a permit sets out the permitting history, including any changes to the permit reference number.  


	[bookmark: _Hlk69745572]Status log of the permit

	Description
	Date
	Comments

	Application VP3339PD (EPR/VP3339PD/A001)
	Duly made 11/03/2004
	

	Additional Information Received
	Requested 04/08/2004
	Received 27/08/2004, 20/09/2004

	Permit determined VP3339PD (EPR/VP3339PD/A001)
	06/05/2005
	

	Regulation 16 Notice* Application
	14/06/2005
	

	Regulation 16 Notice Determined
	05/07/2005
	

	Variation application EP3533LE (EPR/VP3339PD/V002)
	Duly made 30/10/2005
	

	Variation determined EP3533LE (EPR/VP3339PD/V002
	05/01/2006
	

	Variation application EP3536LY (EPR/VP3339PD/V003)
	Duly made 05/06/2006
	

	Variation determined EP3536LY (EPR/VP3339PD/V003)
	04/09/2006
	

	Variation application CP3331MX (EPR/VP3339PD/V004)
	Duly made
21/12/2006
	

	Variation determined CP3331MX (EPR/VP3339PD/V004)
	04/05/2007
	

	Variation application EPR/VP3339PD/V005
	Duly Made
04/03/2011
	

	Variation determined EPR/VP3339PD/V005
	17/06/2011
	

	Agency variation determined EPR/VP3339PD/V006
	04/03/2013
	Agency variation to implement the changes introduced by IED

	Part Surrender application EPR/VP3339PD/S007
	Duly Made
	Part surrender of non-process areas of the site

	Additional information received
	31/05/2016
	Plan showing new installation boundary

	Part Surrender determined EPR/VP3339PD/S007
	18/07/2016
	Part surrender issued

	Regulation 60 Notice dated 25/07/16 (Notice requiring information for statutory review of permit)
	Response received 14/12/2016
	Technical standards detailed in response to the information notice. Information to demonstrate that relevant BAT conclusions are met for non-ferrous metal production

	Variation application EPR/VP3339PD/V008
	Duly Made
24/01/2017
	

	Application EPR/ EPR/VP3339PD/V008 (Variation and Consolidation)
	03/04/2017
	Variation and consolidation following the implementation of IED. In addition, a normal variation to add a new LMC and extruder process has been completed.

	Variation application EPR/VP3339PD/V009
	Duly Made 12/02/2018
	

	Application EPR/ EPR/VP3339PD/V009 (Variation and Consolidation)
	23/03/2018
	Normal variation to make several changes within the LMC process.

	Variation application EPR/VP3339PD/V010
	Duly Made 29/10/2018
	Application to move site waste handling and review sites discharge to sewer.

	Variation determined EPR/VP3339PD/V010
	30/11/2018
	Variation determined

	Part Surrender application EPR/VP3339PD/S011
	Duly Made 06/08/2019
	Application to surrender the permit in part – to surrender areas of nonprocess.

	Part Surrender determined EPR/VP3339PD/S011
	23/10/2019
	Part surrender issued

	Application EPR/VP3339/V012
	Duly Made 
08/02/2021
	Application to change abatement and stack at emission point A15

	Application EPR/VP3339/V012
	Duly Made 
18/06/2021
	Variation issued to Morganite Electrical Carbon Limited




End of introductory note
[image: ]

	Variation application number
EPR/VP3339PD/V012
	Page i	-  -	- i -	- i -i
	





	Variation application number  EPR/VP3339PD/V012
	Page ii	

	



	[bookmark: _Toc77056945]
Notice of variation 


Environmental Permitting (England and Wales) Regulations 2016
[bookmark: _Hlt13295849][bookmark: OperatorName2]
The Natural Resources Body for Wales (“Natural Resources Wales”) in exercise of its powers under regulation 20 of the Environmental Permitting (England and Wales) Regulations 2016 varies 

Permit number
EPR/VP3339PD

issued to:
Morganite Electrical Carbon Limited (“the operator”)

[bookmark: InstallationAddress21]whose registered office is

Upper Fforest Way 
Morriston 
Swansea
West Glamorgan 
SA6 8PP 

company registration number 01034653

to operate a regulated facility at

Electrical Carbon, Swansea 
Upper Fforest Way 
Morriston
Swansea 
SA6 8PP

to the extent set out in the schedules.

The notice shall take effect from 18/06/2021

	Signed
	Date

	Holly Noble
	18/06/2021



Authorised on behalf of Natural Resources Wales

Schedule 1 – conditions to be deleted
None  

Schedule 2 – conditions to be amended 
The following conditions are amended as a result of the application made by the operator: 3.1.1, 3.5.1 (a), 3.5.4 and Table S1.2 and Table S3.1b

Conditions 3.1.1 is amended as follow:
3.1.1	There shall be no point source emissions to water, air or land except from the sources and emission points listed in schedule 3 tables S3.1 and S3.2
Conditions 3.5.1 and 3.5.4 are amended as follow:
3.5.1   The operator shall, unless otherwise agreed in writing by Natural Resources Wales, undertake the monitoring specified in the following tables in schedule 3 to this permit:
(a)	point source emissions specified in tables S3.1, and S3.2.

3.5.4   Permanent means of access shall be provided to enable sampling/monitoring to be carried out in relation to the emission points specified in schedule 3 tables S3.1, S3.2 unless otherwise agreed in writing by Natural Resources Wales
Table S1.2 is amended as follow:

	Table S1.2 Operating techniques

	Description
	Parts
	Date Received

	Application
	The response to questions 2.1 and 2.2 and given in section 2.3 of the application
	11/03/2004

	Variation
	Variation Application CP3331MX and response to Sch7 Notice
	21/12/2006

	Variation
	Variation Application VP33339PD/V005 Non-technical summary
	23/02/2011

	Response to Regulation 60 notice
	The response and supporting information requested by NRW and submitted by email
	14/12/2016

	Variation
	Variation Application VP33339PD/V008 Non-technical summary
	24/01/2017

	Variation
	Variation Application VP33339PD/V008 Air Quality Assessment
	24/01/2017

	Variation
	Variation Application VP33339PD/V008 Application Document P2703/R003
	24/01/2017

	Variation
	Non-Technical Summary v4
	02/02/2018

	Variation
	IPPC Morgan Carbon Site Emissions Point to Air, Drawing No – SITEMISS01/I
	02/02/2018

	Variation
	[bookmark: _GoBack]Variation Application VP3339PD/V010 Application Document Minor Technical Variation 2010-10

	16/10/2018

	Variation
	Variation Application VP3339PD/V012
· Document Reference: VP3339PD/V012/A15
· Appendix 3 HDB Vessal Information


	08/02/2021





Table S3.1b is amended as follow:
	Table S3.1b Point source emissions to air – emission limits and monitoring requirements – from 30th June 2020

	Emission point ref. & location
	Source
	Parameter
	Limit (including unit)
	Reference period
	Monitoring frequency
	Monitoring standard or method

	A2
	Production Line 1
	-
	-
	-
	-
	-

	A3
	LMC decompression exhaust
	-
	-
	-
	-
	-

	A8
	Production Line 4, G building
	-
	-
	-
	-
	-

	A9
	Metal Spraying
	-
	-
	-
	-
	-

	A10
	Dust plant
	Lead
	2 mg/Nm3
	
	
	

	
	
	Copper
	2 mg/Nm3
	Spot Sample
	Quarterly
	BS EN 14385:2004

	
	
	Antimony
	2 mg/Nm3
	
	
	

	
	
	Total Particulate
	5 mg/Nm3
	Hourly Average
	Annual
	BS ISO 13284-1:2002

	A11

	LMC pre-heat furnaces
	-
	-
	-
	-
	-

	A15
	Production Line 1
	Total Particulates
	4 mg/Nm3
	Hourly Average

	Annual
	BS ISO 13284-1:2002

	
	
	BaP
	0.005 mg/Nm3

	
	
	

	A19
	Production Line 4, G building
	Total Particulate
	5 mg/Nm3
	Hourly Average
	Annual
	BS ISO 13284-1:2002

	A27

	Production Line 1
	Sulphur Dioxide
	2900 mg/Nm3
	24 Hourly Average
	
Annual
	BS ISO 7935:1992

	
	
	Oxides of Nitrogen (expressed as NO2)
	150 mg/Nm3
	
	
	BS ISO 10849:1996

	
	
	Total Particulate
	10 mg/Nm3
	Hourly Average
	
	BS ISO 13284-1:2002

	
	
	BaP
	0.01 mg/Nm3
	
	
	

	
	
	
	
	
	
	

	A28
	Production Line 1
	Sulphur Dioxide
	2900 mg/Nm3
	24 Hourly Average
	
	BS ISO 10849:1996

	
	
	Oxides of Nitrogen (expressed as NO2)
	150 mg/Nm3
	
	Annual
	BS ISO 10849:1996

	
	
	Total Particulate
	10 mg/Nm3
	Hourly Average
	
	BS ISO 13284-1:2002

	



	
	BaP

	0.01 mg/Nm3

	
	
	

	Emission point ref. & location
	Source
	Parameter
	Limit (including unit)
	Reference period
	Monitoring frequency
	Monitoring standard or method

	A39
	EHT, G building
	-
	-
	-



	-
	-

	A61
	Production Line 1
	Sulphur Dioxide
	2900 mg/Nm3
	24 hourly average
	Annual
	BS ISO 7935:1992

	
	
	Oxides of Nitrogen 
(expressed as NO2
	150 mg/Nm3
	
	
	BS ISO 13284-1:2002

	
	
	Total Particulate
	10 mg/Nm3
	Hourly average
	
	BS ISO 13284-1:2002

	
	
	BaP
	0.01 mg/Nm3 

	
	
	

	A62
	LMC
	-
	-
	-
	-
	-

	A63
	Small batch plating (tin, 
copper, silver plant)
	-
	-
	-
	-
	-

	A64
	Ceramic and zinc spray booth
	-
	-
	-
	-
	-

	A65-A69
	LMC pressure and 
depressurisation. Emergency 
pressure release valves
	-
	-
	-
	-
	-

	





Schedule 3 – conditions to be added
None
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