


[bookmark: _GoBack]Permit Number: 	SP3531SK						Operator: 		Tradebe Gwent Limited

Facility:		Gwent Waste Management Centre		Form Number: 	 Air1 / 17/08/22
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Hydrogen Chloride (HCI)
	5 mg/Nm3
	None set
	
	EN 1911
	
	

	A1
	Total Volatile Organic Compounds (TVOC)
	20 mg/Nm3
	None set
	
	EN 12619
	
	






[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	

Permit Number: 	SP3531SK						Operator: 		Tradebe Gwent Limited

Facility:		Gwent Waste Management Centre		Form Number: 	Sewer1 / 17/08/22
Reporting of emissions to sewer for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	S1
	Flow Rate
	None set
	None set
	
	As agreed with Natural Resources Wales
	
	

	S1
	Adsorbable Organically Bound Halogens (AOX)
	1 mg/l
	None set
	
	EN ISO 9562
	
	

	S1
	Benzene, Toluene, Ethylbenzene, Xylene (BTEX)
	None set
	None set
	
	EN ISO 15680
	
	

	S1
	Free Cyanide (CN)
	0.1 mg/l
	None set
	
	Various EN standards available (e.g. EN ISO 14403-1 and -2)
	
	

	S1
	Hydrocarbon Oil Index (HOI)
	10 mg/l
	None set
	
	EN ISO 9377-2
	
	

	S1
	Arsenic (As)
	0.1 mg/l
	None set
	
	Various EN standards available (e.g. EN ISO 11885, EN ISO 17294-2, EN ISO 15586)
	
	

	S1
	Cadmium (Cd)
	0.1 mg/l
	None set
	
	
	
	

	S1
	Chromium (Cr)
	0.3 mg/l
	None set
	
	
	
	

	S1
	Copper (Cu)
	0.5 mg/l
	None set
	
	
	
	

	S1
	Nickel (Ni)
	1 mg/l
	None set
	
	
	
	

	S1
	Lead (Pb)
	0.3 mg/l
	None set
	
	
	
	

	S1
	Zinc (Zn)
	2 mg/l
	None set
	
	
	
	

	S1
	Manganese (Mn)
	No limit set
	None set
	
	
	
	

	S1
	Hexavalent Chromium (Cr(VI))
	0.1 mg/l
	None set
	
	Various EN standards available (e.g. EN ISO 10304-3, EN ISO 23913)
	
	

	S1
	Mercury (Hg)
	10 µg/l
	None set
	
	Various EN standards available (e.g. EN ISO 17852, EN ISO 12846)
	
	

	S1
	PFOA
	No limit set
	None set
	
	No EN standard available
	
	

	S1
	PFOS
	No limit set
	None set
	
	No EN standard available
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	

Permit Number: 	SP3531SK						Operator: 		Tradebe Gwent Limited

Facility:		Gwent Waste Management Centre		Form Number: 	WaterUsage1 / 01/06/06

Reporting of Water Usage for the year YYYY

	Water Source
	Usage
(m3/year
	Specific Usage 
(m3/unit output)
	

	
	
	
	

	
	
	
	

	Mains water
	
	
	

	Site borehole
	
	
	

	River abstraction
	
	
	

	
	
	
	

	
	
	
	

	TOTAL WATER USAGE
	
	
	



	Operator’s comments :







Signed …………………………………………………………….  		Date………………………..   	
	

Permit Number: 	SP3531SK						Operator: 		Tradebe Gwent Limited

Facility:		Gwent Waste Management Centre		Form Number: 	Energy1 / 01/06/06

Reporting of Energy Usage for the year YYYY

	
Energy Source
	Energy Usage
	
Specific Usage
(MWh/unit output)
	

	
	
Quantity
	Primary Energy
(MWh)
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	Electricity *
	MWh
	
	
	

	Natural Gas
	MWh
	
	
	

	Gas Oil
	tonnes
	
	
	

	Recovered Fuel Oil
	tonnes
	
	
	

	
	
	
	
	

	TOTAL
	-
	
	
	

	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments :









Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number: 	SP3531SK						Operator: 		Tradebe Gwent Limited

Facility:		Gwent Waste Management Centre		Form Number: 	Performance1 / 01/06/06

Reporting of other performance indicators for the period DD/MM/YYYY to DD/MM/YYYY

	Parameter
	
	Units 
	

	
	
	
	

	Total raw material used 
	tonnes
	

	Total amounts of waste treated
	tonnes
	

	Generation of waste water
	m3
	

	Treatment residues where disposal is to a non-hazardous waste landfill site.
	tonnes
	

	Treatment residues where disposal is to a hazardous waste landfill site.
	tonnes
	

	
	
	



	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)
.

 

