Permit Number: 	EP3698FL								Operator: 		CWM Environmental Limited

Facility:		Nantycaws HCI Waste Transfer & Treatment Facility		Form Number: 	 Air1 / 08/07/21
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Hydrogen Sulphide
	-
	-
	
	No Standard
	
	

	A1
	Ammonia
	2.0 mg/Nm3
	-
	
	No Standard
	
	

	A1
	Odour
	1000 OUE/Nm3
	-
	
	BS EN 13725

	
	






[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

Permit Number: 	EP3698FL								Operator: 		CWM Environmental Limited

Facility:		Nantycaws HCI Waste Transfer & Treatment Facility		Form Number: 	Water1 / 08/07/21
Reporting of emissions to water (other than to sewer) and land for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	The watercourse adjacent to the site which flows south before joining the Afon-y-Bantwen
	Oil and grease
	None visible
	Weekly or as agreed in writing with Natural Resources Wales
	
	
	
	-



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.


Signed …………………………………………………………….  		Date………………………..
	(Authorised to sign as representative of Operator)

 
Permit Number: 	EP3698FL								Operator: 		CWM Environmental Limited

Facility:		Nantycaws HCI Waste Transfer & Treatment Facility		Form Number: 	WaterUsage1 / 08/07/21

Reporting of Water Usage for the year YYYY

	Water Source
	Usage
(m3/year
	Specific Usage 
(m3/unit output)
	

	
	
	
	

	
	
	
	

	Mains water
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	TOTAL WATER USAGE
	
	
	



	Operator’s comments :







Signed …………………………………………………………….  		Date………………………..   	
	(authorised to sign as representative of Operator)

Permit Number: 	EP3698FL								Operator: 		CWM Environmental Limited

Facility:		Nantycaws HCI Waste Transfer & Treatment Facility		Energy1 / 08/07/21

Reporting of Energy Usage for the year YYYY

	
Energy Source
	Energy Usage
	
Specific Usage
(MWh/unit output)
	

	
	
Quantity
	Primary Energy
(MWh)
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	Electricity *
	MWh
	
	
	

	Natural Gas
	MWh
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	TOTAL
	-
	
	
	

	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments :









Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number: 	EP3698FL								Operator: 		CWM Environmental Limited

[bookmark: _GoBack]Facility:		Nantycaws HCI Waste Transfer & Treatment Facility		Form Number: 	Performance1 / 08/07/21

Reporting of other performance indicators for the period DD/MM/YYYY to DD/MM/YYYY

	Parameter
	
	Units 
	

	
	
	
	

	Total raw material used 
	tonnes
	

	Generation of residues (solid waste generated by the waste treatment activity)
	tonnes
	

	Generation of waste water
	m3
	

	Total amount of waste treated 
	tonnes
	

	Total amount of compost produced
	tonnes 
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


