


Permit Number: 	YP3937SH			Operator: 		Mekatek Limited

Facility:		Amex Park			Form Number: 	Water1 / DD/MM/YY
Reporting of emissions to water (other than to sewer) and land for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date and Times [3]
	Uncertainty [4]

	W1
	Suspended solids
	75mg/l (winter period) [5]
	Monthly analysis of bulk daily sample.
	
	As per Technical Guidance Note (Monitoring) M18: Monitoring of discharges to water and sewer or other method as agreed in writing with the Regulator.
	
	

	
	
	60mg/l (summer period) [6]
	
	
	
	
	

	
	Total ammonium as N 
	20mg/l (winter period) [5]
	Spot sample
	
	
	
	

	
	
	15mg/l (summer period) [6
	
	
	
	
	

	
	Biochemical oxygen demand (5 day)
	75mg/l (winter period) [5]
	Spot sample
	
	
	
	

	
	
	40 mg/l (summer period) [6
	
	
	
	
	

	
	Oils and grease
	No visible release
	Visual inspection
	
	
	
	

	
	Temperature
	≤24ºC
	Spot readings
	
	
	
	

	
	pH
	6 to 8.5 
	Continuous
	
	
	
	

	
	Flow
	39l/second
	Continuous
	
	
	
	

	
	
	2500m³/day
	
	
	
	
	


[bookmark: _GoBack]
[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
[5] Winter period is defined as 01 October to 31 March.
[6] summer period is defined as 01 April to 30 September


Signed …………………………………………………………….  		Date………………………..
	(Authorised to sign as representative of Operator)


Permit Number: 	YP3937SH			Operator: 		Mekatek Limited

Facility:		Amex Park			Form Number: 	WaterUsage1 / DD/MM/YY

Reporting of Water Usage for the year YYYY

	Water Source
	Usage
(m3/year)
	Specific Usage 
(m3/unit output)
	

	
	
	
	

	
	
	
	

	Mains water
	
	
	

	Site borehole
	
	
	

	River abstraction
	
	
	

	
	
	
	

	
	
	
	

	TOTAL WATER USAGE
	
	
	



	Operator’s comments :







Signed …………………………………………………………….  		Date………………………..   	
	(authorised to sign as representative of Operator)

Permit Number: 	YP3937SH			Operator: 		Mekatek Limited

Facility:		Amex Park			Form Number: 	Energy1 / DD/MM/YY

Reporting of Energy Usage for the year YYYY

	Energy Source
	Energy Usage Quantity
	Primary Energy (MWh)
	Specific Usage (MWh/unit output)
	

	Electricity *
	MWh
	
	
	

	Natural Gas
	MWh
	
	
	

	Gas Oil
	tonnes
	
	
	

	Recovered Fuel Oil
	tonnes
	
	
	

	
	
	
	
	

	TOTAL
	-
	
	
	

	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments :









Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

