Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
……
Reporting of ……LEACHATE…… monitoring for the period for … June 2021
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	
	
	
	
	
	
	
	

	L2
	Am Nitrogen
	904
	Jun-21
	837
	INORG-L12
	28th Jun 21
	12.69



	
	
	
	
	
	
	
	

	L2
	Cadmium
	0.05
	Jun-21
	0.21
	1450
	28th Jun 21
	3.93

	
	
	
	
	
	
	
	

	L2
	Nickel
	0.4
	Jun-21
	225
	METALS-L
	28th Jun 21
	5.23


	
	
	
	
	
	
	
	

	L2
	Chloride
	1306
	Jun-21
	1,561
	INORG-L13
	28th Jun 21
	6.71



	
	
	
	
	
	
	
	

	L2
	MP Xylene
	0.032
	Jun-21
	<1.0
	ORG-LO5
	28th Jun 21
	7.66



	
	
	
	
	
	
	
	

	L2
	Mecoprop
	0.024
	Jun-21
	<0.1
	ORG-L17
	28th Jun 21
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	 
	Am Nitrogen
	1370
	Jun-21
	1,413
	INORG-L12
	28th Jun 21
	12.69



	L4
	
	
	
	
	
	
	

	 
	Cadmium
	0.1
	Jun-21
	<0.11
	1450
	28th Jun 21
	3.93

	L4
	
	
	
	
	
	
	

	 
	Nickel
	0.1
	Jun-21
	177
	METALS-L
	28th Jun 21
	5.23


	L4
	
	
	
	
	
	
	

	 
	Chloride
	13713
	Jun-21
	1,351
	INORG-L13
	28th Jun 21
	6.71



	L4
	
	
	
	
	
	
	

	 
	MP Xylene
	0.029
	Jun-21
	<1.0
	ORG-LO5
	28th Jun 21
	7.66



	L4
	
	
	
	
	
	
	

	 
	Mecoprop
	0.032
	Jun-21
	2.1
	ORG-L17
	28th Jun 21
	8.27



	L4
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	LTP1 
	Am Nitrogen
	1370
	Jun-21
	80.3
	INORG-L12
	28th Jun 21
	12.69



	
	
	
	
	
	
	
	

	LTP1
	Cadmium
	0.1
	Jun-21
	-
	1450
	28th Jun 21
	3.93

	
	
	
	
	
	
	
	

	LTP1
	Nickel
	0.1
	Jun-21
	21.4
	METALS-L
	28th Jun 21
	5.23


	
	
	
	
	
	
	
	

	LTP1
	Chloride
	13713
	Jun-21
	284
	INORG-L13
	28th Jun 21
	6.71



	
	
	
	
	
	
	
	

	LTP1
	MP Xylene
	0.029
	Jun-21
	-
	ORG-LO5
	28th Jun 21
	7.66



	
	
	
	
	
	
	
	

	
	Mecoprop
	0.032
	Jun-21
	-
	ORG-L17
	28th Jun 21
	8.27



	LTP1
	
	
	
	
	
	
	


The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed ……………………[image: image1.png]


……………….  

Date 30th July 2021     



(Authorised to sign as representative of Operator)

