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	Consent no
	NRWWIA279

	
	


WATER INDUSTRY ACT 1991

SECTION 165 / 166
CONSENT TO DISCHARGE

TO:
Dŵr Cymru Cyfyngedig

Linea


Fotran Road

St Mellons


CARDIFF

CF3 0LT
	The NATURAL RESOURCES BODY FOR WALES ("Natural Resources Wales") in pursuance of its powers under the Water Industry Act 1991 HEREBY CONSENTS to the making of a discharge as follows:
Raw Water


	FROM: nant hir reservoir, llwydcoed, aberdare, rhondda cynon taff, cf44 0dj

	

	AT: NATIONAL GRID REFERENCE SN 98918 06700

	

	TO: nant hir

	

	SUBJECT TO: the conditions set out in the following schedule:

Raw Water                     Schedule No. NRWWIA279

	

	This consent is issued on the 27th day of October 2021
This consent takes effect on the 1st day of November 2021
This consent shall cease to have effect on the 14th day of March 2022
Signed: Melissa Broad


	


CONDITIONS OF CONSENT TO DISCHARGE

RAW WATER (“the Discharge”)
NATURE OF THE DISCHARGE

1.
The Discharge shall consist solely of raw water. 

SOURCE OF THE DISCHARGE

2. The Discharge shall be derived from Nant Hir Reservoir.
LOCATION OF DISCHARGE

3.
The location of the Discharge shall be at NGR SN 98915 06695, marked ‘Location where flow enters the watercourse’ on the site plan in Annex 1.

SAMPLE POINT

4.
A sample point shall be provided and maintained so that a representative sample of the Discharge may be obtained. 

VOLUME

5. The total daily volume of the Discharge shall not exceed 34,560 cubic metres.

6. The rate of the Discharge shall not exceed 400 litres per second.
COMPOSITION

8.
The consent holder shall take all necessary steps to secure that any water discharged by it under this consent is as free as may be reasonably practicable from — 

(a) 
mud and silt;

(b) 
solid, polluting, offensive or injurious substances; 
and

(c)
any substances prejudicial to fish or spawn, or to spawning beds or food of fish.
SCOURING
9.
The rate of discharge shall be controlled to prevent any significant scouring of the bed or bankside of the receiving water. 
FLOODING

10.
The discharge shall not cause or significantly contribute to flooding in the downstream catchment.
PERIOD OF DISCHARGE

11.
The Discharge shall only be made between 1st day of November 2021 and the 14th day of March 2022.
ANNEX 1- PLAN No. NRWWIA279
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