Permit Number: 
JP3239ST



Operator: 

The County council of the City and County of Cardiff

Installation:

Lamby Way Landfill Site

Form Number: 
……
Reporting of ……LEACHATE…… monitoring for the period for … September 2021
	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	
	
	
	
	
	
	
	

	L2
	Am Nitrogen
	904
	Sep-21
	899
	INORG-L12
	08th Sep 21
	12.69



	
	
	
	
	
	
	
	

	L2
	Cadmium
	0.05
	Sep-21
	0.18
	1450
	08th Sep 21
	3.93

	
	
	
	
	
	
	
	

	L2
	Nickel
	0.4
	Sep-21
	349
	METALS-L
	08th Sep 21
	5.23


	
	
	
	
	
	
	
	

	L2
	Chloride
	1306
	Sep-21
	1800
	INORG-L13
	08th Sep 21
	6.71



	
	
	
	
	
	
	
	

	L2
	MP Xylene
	0.032
	Sep-21
	<1.0
	ORG-LO5
	08th Sep 21
	7.66



	
	
	
	
	
	
	
	

	L2
	Mecoprop
	0.024
	Sep-21
	28.4
	ORG-L17
	08th Sep 21
	8.27



	
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	 
	Am Nitrogen
	1160
	Sep-21
	969
	INORG-L12
	08th Sep 21
	12.69



	L4
	
	
	
	
	
	
	

	 
	Cadmium
	<0.11
	Sep-21
	<0.08
	1450
	08th Sep 21
	3.93

	L4
	
	
	
	
	
	
	

	 
	Nickel
	212
	Sep-21
	114
	METALS-L
	08th Sep 21
	5.23


	L4
	
	
	
	
	
	
	

	 
	Chloride
	1600
	Sep-21
	1468
	INORG-L13
	08th Sep 21
	6.71



	L4
	
	
	
	
	
	
	

	 
	MP Xylene
	2.7
	Sep-21
	11.9
	ORG-LO5
	08th Sep 21
	7.66



	L4
	
	
	
	
	
	
	

	 
	Mecoprop
	46.0
	Sep-21
	2.9
	ORG-L17
	08th Sep 21
	8.27



	L4
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	

	Monitoring Point
	Substance/ Parameter
	Trigger Level
	Reference Period
	Result [1]
	Test Method [2]
	Sample Date & Times [3]
	Uncertainty [4]

	LTP1 
	Am Nitrogen
	1370
	Sep-21
	127
	INORG-L12
	08th Sep 21
	12.69



	
	
	
	
	
	
	
	

	LTP1
	Cadmium
	0.1
	Sep-21
	-
	1450
	08th Sep 21
	3.93

	
	
	
	
	
	
	
	

	LTP1
	Nickel
	0.1
	Sep-21
	172
	METALS-L
	08th Sep 21
	5.23


	
	
	
	
	
	
	
	

	LTP1
	Chloride
	13713
	Sep-21
	304
	INORG-L13
	08th Sep 21
	6.71



	
	
	
	
	
	
	
	

	LTP1
	MP Xylene
	0.029
	Sep-21
	-
	ORG-LO5
	08th Sep 21
	7.66



	
	
	
	
	
	
	
	

	
	Mecoprop
	0.032
	Sep-21
	-
	ORG-L17
	08th Sep 21
	8.27



	L7
	
	
	
	
	
	
	


The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

[image: image1.png]



Signed ………………………… ………………………………….  

Date 03/11/2021  



(Authorised to sign as representative of Operator)

