Permit Number: 	EPR/BX7282IS	                                                                        Operator: AB InBev UK Limited

Facility:		Magor Brewery	Form Number: 	 Air1 / 23/08/2021
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	220 mg/Nm3
	Periodic
	
	BS EN 14792
	
	

	
	Carbon monoxide
	No limit set
	Periodic
	
	ISO 12039
	
	

	A2
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	220 mg/Nm3
	Periodic
	
	BS EN 14792
	
	

	
	Carbon monoxide
	No limit set
	Periodic
	
	ISO 12039
	
	

	A3
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	140 mg/Nm3
	Periodic
	
	BS EN 14792
	
	

	
	Carbon monoxide
	No limit set
	Periodic
	
	ISO 12039
	
	

	A4
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	140 mg/Nm3
	Periodic
	
	BS EN 14792
	
	

	
	Carbon monoxide
	No limit set
	Periodic
	
	ISO 12039
	
	

	A8
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	500 mg/Nm3
	Periodic
	
	BS EN 14792
	
	

	
	Carbon monoxide
	650 mg/Nm3
	Periodic
	
	BS EN 15058
	
	

	
	Sulphur dioxide
	80 mg/Nm3
	Periodic
	
	BS EN 14791
	
	

	A9
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	220 mg/Nm3
	Periodic
	
	BS EN 14792
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.


Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

Permit Number: 	EPR/BX7282IS			Operator: 		AB InBev UK Limited

Facility:		Magor Brewery         Form Number: 	Water1 / 23/08/2021
Reporting of emissions to water for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	Final Effluent Sample Point
ST 4369 8494
	Flow
	10,000 m3/day
	Continuous
	
	
	
	

	
	Flow
	126 l/s
	Continuous
	
	
	
	

	
	pH
	>5 <9
	Continuous
	
	
	
	

	
	Temperature
	30 °C
	Continuous
	
	
	
	

	
	BOD
	200 mg/l
	Weekly composite
	
	
	
	

	
	COD
	450 mg/l
	Weekly composite
	
	
	
	

	
	Suspended Solids
	150 mg/l
	Weekly
	
	
	
	

	
	Total copper & its compounds
	0.01 mg/l as annual average
	Monthly composite
	
	
	
	

	
	Total cadmium & its compounds
	0.005 mg/l as annual average
	Monthly composite
	
	
	
	

	
	Total chromium & its compounds
	0.015 mg/l as annual average
	Monthly composite
	
	
	
	

	
	Total mercury & its compounds
	0.0005 mg/l as annual average
	Monthly composite
	
	
	
	

	
	Total nickel & its
compounds
	0.03 mg/l as annual average
	Monthly composite
	
	
	
	

	
	Total zinc & its compounds
	0.07 mg/l as annual average
	Monthly composite
	
	
	
	

	
	Total arsenic & its compounds
	0.025 mg/l as annual average
	Monthly composite
	
	
	
	

	
	Total mercury and its compounds
	915 g in a year
	
	
	
	
	

	
	Total cadmium and its compounds
	9150 g in a year
	
	
	
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number: 	EPR/BX7282IS			Operator: 		AB InBev UK Limited

Facility:		Magor Brewery	Form Number: 	WaterUsage1 / 23/08/2021

Reporting of Water Usage for the year YYYY

	Water Source
	Usage
(m3/year)
	Specific Usage 
(m3/unit output)
	

	
	
	
	

	Spring water
	
	
	

	Mains water
	
	
	

	TOTAL WATER USAGE
	
	
	

	
	
	
	



	Operator’s comments:







Signed …………………………………………………………….  		Date………………………..   	
	(authorised to sign as representative of Operator)

Permit Number: 	EPR/BX7282IS			Operator: 		AB InBev UK Limited

Facility:		Magor Brewery		Form Number: 	Energy1 / 23/08/2021

Reporting of Energy Usage for the year YYYY

	
Energy Source
	Energy Usage
	
Specific Usage
(MWh/unit output)
	

	
	
Quantity
	Primary Energy
(MWh)
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	Electricity *
	MWh
	
	
	

	Natural Gas
	MWh
	
	
	

	Fuel oil
	tonnes
	
	
	

	
	
	
	
	

	TOTAL
	
	
	
	

	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments:









Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number: 	EPR/BX7282IS			Operator: 		AB InBev UK Limited

[bookmark: _GoBack]Facility:		Magor Brewery		Form Number: 	Performance1 / 23/08/2021

Reporting of other performance indicators for the period DD/MM/YYYY to DD/MM/YYYY

	Parameter
	
	Result
	

	
	
	
	

	Production of beers and lagers (tonnes)
	
	

	BOD (BOD/t)
	
	

	COD (COD/t)
	
	

	Carbon dioxide (tonne/tonne)
	
	

	Ammonia (kg/year)
	
	

	Gas engine energy generated, electricity and heat (MWth)
	
	

	Hydrogen sulphide concentration (ppm)
	
	

	Hydrogen sulphide mass emission (g/s)
	
	

	Waste disposal and/or recovery(tonnes/year)
	
	



	Operator’s comments:








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


