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[bookmark: _Toc112747535]1.	Introduction
This procedure is in place to ensure that SPTS has adequate emergency response and corrective action procedures in place to cover environmental issues. 


[bookmark: _Toc112747536]2.	Scope
Environmental considerations arising from emergency situations on the Newport site.



[bookmark: _Toc112747537]3.	General
1.	In the event of any risk to the environment from fire, gas or chemical leakage/spillage/damage the appropriate authorities shall be informed.
2.	There shall be adequate containment measures in place to allow minor spillages to be contained before entering water/soil/atmosphere.
3.	The EHS Manager (or Facilities Manager as deputy) is responsible for ensuring that Natural Resources Wales (and The Fire Service) are contacted once an environmental risk is evident.
	    Emergency contacts for Environmental issues only: 
· Natural Resources Wales (was Environment Agency)  Tel : 0300 065 3000
· Fire Services 5555 (or 9999)


[bookmark: _Toc112747538]4.	Reporting & Corrective Action
1.	All incidents and near misses must be reported and recorded.
2.	Any Investigations carried out must be recorded using the Accident/Incident/Near Miss Form (No: 861-1035496). 

[bookmark: _Toc112747539]5.	Fire
This is covered by Fire Evacuation procedure No.1035557.


[bookmark: _Toc112747540]6.	Gas Escapes
This is covered by Gas Evacuation procedure 1035569.  This procedure ensures that the site is evacuated safely, that a full roll call is carried out using the Tensor reporting system and that the ERT/BA team are employed safely, where required (BA procedure 103555).




7. 	Spill Containment	
The accidental release of chemicals and other substances can quickly and dramatically affect the environment.  In the event of a spillage it’s important to control the spill to minimize its effects. Doing so will help minimize potential harm; avoid fines and clean-up costs; and avoid negative publicity for the company.

7.1	Minor Spills	
· If an accidental release of a substance occurs, prompt action must be taken to contain the spillage and prevent its entering the site drainage system. Equipment for this purpose will be found in site spillage kits which are located throughout the service chase areas, cleanroom and plant room. Where possible, stop the escape of the substance at source.

· Advice from COSHH assessments and Safety Data Sheets (SDS) must be observed at all times and should be referred to BEFORE attempting any clean-up operation.  SDS are held in the following areas;
· Manufacturing (paper copy)
· First Aid Room & Gatehouse (paper copy)
· SharePoint document library, folders 800 and 810

· Once contained, spills should be thoroughly cleaned up using absorbent granules/pads. Do not hose spillages into the drainage system! Larger spills may need to be cleaned and removed by specialized contractors.

· Dispose of all contaminated materials (e.g. absorbent pads) correctly by triple bagging and sealing them in contaminated waste bags and removing the bags to the chemical waste store. The bags must be clearly marked so as to properly identify their content.

· All spillages of hazardous substances must be promptly reported so that a thorough clean-up and investigation can be instigated. Spillages should be reported to the line manager/supervisor with immediate responsibility for the work area in which the event has occurred or for the persons involved. Should a spillage involve contractors or visitors, the matter should be reported to the relevant SPTS site host. 

· Where a spillage presents a risk to the environment, the EHS Manager must ALWAYS be informed immediately so that appropriate action may be taken to minimise any resultant harm. 

7.2	Major Spills	
For larger spillages which cannot be contained adequately or which pose an imminent risk to site personnel or the environment, an emergency alarm should be raised immediately. This may be achieved by ringing the site emergency telephone number 5555.


Once notified of a major spillage of a hazardous substance, the following actions must be taken by the Incident Controller:
· If appropriate, contact the fire service and request their attendance at site

· Identify the material spilled and obtain appropriate PPE before intervening

· If possible stop the escape of the substance at source by, for example, switching off pumps, closing valves, blocking openings etc.

· Ensure the spill is contained and prevent it reaching surface drains. For this purpose consider the use of drain covers, absorbent socks etc. (see Section 7.1)

· Restrict access to the area using hazard tape and signs

· If the emergency services are required to attend site, ensure the substance SDS is passed to fire service personnel. SDS's are located in the following areas:
· Manufacturing (paper copy)
· First Aid Room & Gatehouse (paper copy)
· SharePoint document library, folders 800 and 810

· Ensure the EHS Manager or Facilities Manager informs Natural Resources Wales of the incident as soon as practically possible.

· Should an evacuation of the site prove necessary, this should follow standard Fire Evacuation procedure 1035557

Note: 
· If a spillage occurs we must do everything in our power to prevent substances entering the drainage system. Snakes & pads etc. are found in spill trolleys and grab bags. It is however imperative that you do not put yourself or others at risk by carrying out this operation.

· Due to the small quantities of materials kept/used on site, large spills are unlikely other than for nitrogen which is stored in an external 52 ton capacity tank.
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