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Brynrorin Farm
Policy on Emergencies

It is our aim to 

· minimise the likelihood of an emergency situation occurring, and 

· minimise the detrimental effects of an emergency on 

· Flocks, 

· Personnel, 

· The environment and 

· The site itself.

We will achieve the above by ensuring detailed emergency action plan is readily available to all members of staff and that the staff understand these and have been appropriately trained in operating emergency procedures.

All incidents are investigated and if appropriate remedial measures taken to reduce the risk of a recurrence.

FARM SITE PROCEDURES

Section 1 Aims, Responsibilities, and Reviews.

To minimise the likelihood of an emergency situation occurring and minimise the detrimental effects of an emergency on flocks, personnel, the environment and the site through the use of detailed documented instructions, management review and preventative measures.

This procedure is the responsibility of Brynrorin Farm, and it covers the whole of the poultry operation at Brynrorin Farm. It will be reviewed in the event of an emergency to ensure that it has proved to be effective, and it will be reviewed annually in any event to ensure its currency.

Section 2 General Description

The Farm Site Plan 
is a key document in the emergency procedures. It is maintained in an accurate condition, and it will be current, legible and accessible to all members of staff. It contains detailed information that may be required in an emergency situation.

An Emergency Action Plan is maintained in a prominent position near a telephone, and shows procedures to be followed in the event of an emergency, specific directions to the site, and the grid reference. The Emergency Action Plan is reviewed regularly and amended whenever there is a change to the information in it.

A telephone is available and operational on site, both in the Poultry site office and in the Operators Farm House.

Brynrorin Farm ensures that all members of staff are aware of the Emergency Action Plan, Farm Site Plan and water sources 
available for fire fighting. (mains water supply and borehole water)
Provision has been made for an emergency supply of drinking water to cover a period of 24hrs at full demand. Provision has been made for an emergency supply of food. The site has a generator to be used as an emergency power supply for all essential electrical systems and this is regularly tested with the results being recorded and any failure of the generator is immediately rectified. Alarms are installed for any temperature or power problems. Staff are made aware of the documented fire precautions and all houses have a notice indicating the nearest telephone. It is policy to ensure that every building greater than 30 metres in length has two doors. Adequately equipped first aid kits are available.

Section 3 – Relevant Documentation

Site Plan

Emergency Action Plan:

· Fire & Fire Precautions

· Pollution Prevention Control

· Power Failure

· Flood

· Equipment failure

· Food failure

· Water failure

· Disease / High Mortality Plan

· Containment Failure Fuel/Chemical/Foul Water

· Contacts List

· Raw Materials Sheet

· Inventory

SITE PLAN

A site plan is available in the farm office and at the poultry site showing:

The position and size of all poultry house and access points 

All auxiliary poultry buildings and their purpose 

Location of fire extinguishers and first aid kits

Water sources for fire fighting

Drainage routes Dirty and Clean

Feed Storage

Fuel Storage

Fuel Isolation Valves

Change over Valves

Catchment Tanks

In the event of FIRE

· Ensure that all farm personnel, contractors and visitors evacuate the farm buildings and proceed to the agreed assembly point which is at the front of the farm, away from danger Contact the Fire Brigade immediately on 999

· Do not attempt to tackle the fire unless it is safe to do so without putting yourself or others at risk.

· Inform neighbours in case of toxic fume emission.

· Turn off electricity supply to buildings (to avoid fans fanning the fire)

· If possible / accessible
, open the manhole covers in the sheds to allow water to flow to the dirty water tanks – arrange pumping out as necessary

· Any fire water run off will collect in natural ground depression by site entrance and will allow pumping to take place preventing contamination of water course.  
· The nearest water source for fire fighting is the bore hole supply and mains water supply.

· Fire extinguishers are as on the Farm Site Plan.

· As soon as site is safe, attend to bird welfare – ventilation, drinking water, heat, feed (also see disease / high mortality plan below)

Fire Precautions

     Operator and staff will receive training and record will be held          for inspection. 
· Ensure you are familiar with the fire fighting equipment on site and their specific uses i.e. powder and liquid - do not use liquid extinguishers on electrical fires.

· Ensure you are familiar with the position of the equipment.

· Report any equipment defects promptly.

· Ensure all safety notices are obeyed.
· Ensure all exits are clear and fire fighting equipment readily accessible

· Pay particular attention to overheating machinery noticed during inspections or testing (e.g. Generator) and ensure remedial actions are undertaken promptly

· Maintain restricted access to the site

· Ensure buildings are secure

· No smoking, except in designated areas only (outside at site entrance)

· Ensure all flammable / combustible materials are utilised and stored safely and according to manufacture's instructions if appropriate.

· Materials and equipment must not be stored in escape routes and passages

· Ensure you know the location of house doors, the nearest telephone, Site Plan and Emergency Action Plan.

Pollution Prevention/Control

(   Wash water change over valves to be checked 3 days prior to use
 and just before commencement of washing procedures.
(    Prior to wash down ensure catchment tanks are empty.   DO NOT ENTER TANKS 

(  Ensure all staff and cleaning contractors are aware of the        location and operation of change over valves

(  Monitor levels of catchment tanks during washdown to prevent overfill
, if 300mm freeboard is reached cease washing operations and arrange tanks to be emptied.
(   Washdown water to be emptied as per manure management plan as soon as possible after washing

(   Chemical spills
. Diverter valves to be set to containment. Correct PPE must be worn. Minor spills can be cleared up with the use of the chemical spill kit. In the event of a major spillage/leak contact the emergency services/Natural Resources Wales/integrator.

( Fuel oil leakage. Close valves if safe to do so. Change diverter valves/bungs to containment to prevent contamination of clean water drainage. Minor leaks can be contained by the use of proprietary spill kit. In the event of a major spill/leak inform emergency services/ Natural Resources Wales /integrator.  

POWER FAILURE

Site has a back up generator with 24 hour emergency breakdown call out. 
In the event of a power failure ensure that the generator is running and that the correct loads are operating for fans, lights, feeders etc.

· Call the electricity supplier if the problem is a disruption in supply.

· Call the site Electrician if the problem is localised on site.

Total
 Failure (including backups
)

· In the event of total power failure, including the generator, immediate action must be taken to ventilate the houses ie.

· Open house doors and ensure all fan louvers are lowered and vents are fully open

· Contact the site Electrician

· Call for additional help to ventilate houses

· Ensure vents and pop holes are open

· The extent to which the above actions to ventilate are taken is dependent upon stage of growth and ambient temperature.
 (Training undertaken and recorded)
· Return of Supply

· When power is on again, close the house doors and maximise ventilation to facilitate rapid cooling.

· If necessary use catching fans to facilitate cooling.

· Monitor bird behavior

· Ensure an adequate water supply and only run feeders when the houses have been cooled to normal temperature

Precautions

· Check alarms and generator a minimum of weekly and rectify any faults as a priority.

· Ensure the generator battery
, oil and water are adequately replenished. 

· Ensure gas oil tank is replenished after use.

· Ensure the generator is well maintained and the airways clear and radiator clean.

FLOOD

Fire water covered in fire precautions.
To reduce the risks of flooding ensure all ditches and drains are kept clear and regularly maintained.

If flooding is the result of a burst water pipe ensure that leak is repaired as a matter of urgency.

If the inside of a layer house is affected every effort should be made to remove as much water as possible and fresh dry shavings spread over the affected area.

EQUIPMENT FAILURE

In the event of equipment failure (ie. Feeder malfunction, ventilation fan breakdown) 
contact the appropriate service Engineer.

Bird welfare is a priority and every effort must be made to ensure welfare is not compromised by equipment failure.

FOOD FAILURE

To prevent running out of feed bin stocks to be checked daily to ensure sufficient stock in line with next planned delivery, if stock is low 
contact area manager or the feed mill for an extra I emergency delivery.

WATER FAILURE

· In the event of a disruption to the water supply immediately ascertain the cause of the failure – ensure repairs are put in hand as a matter of emergency. 

· In the event that remedy is not possible within twenty hours of failure, arrange emergency tankered supply of potable water.  

· Turn off house lights to alleviate unnecessary stress.

If the emergency water supply is not available contact the local Fire Brigade.

DISEASE / HIGH MORTALITY PLAN

     (   Contact Company Area Manager

· Is it a potentially notifiable disease? – contact Vet for advice, and follow advice / instructions

· Implement Major Loss Procedures.

Containment Failure
Fuel

In the event of a fuel leak or spillage isolate taps if safe to do so.

Switch diverter valves/ bungs to containment to prevent fuel from entering clean water drainage.

Small amounts can be soaked up using propriety spill kit, contact integrator for disposal advice.

Contact emergency services/Natural Resources Wales/integrator in event of serious leakage.

Chemical

Only small amounts of chemicals kept on site (2 x 5 litres footdip disinfectant)
Correct PPE must be worn. (Refer to Product Data Sheet)

Small spills 
can be dealt with by use of chemical spill kit, located in chemical store.

Larger spills to be contained by switching diverter valves to containment.

Contact emergency services/environment agency/integrator in event of serious leakage.

Foul Water

Stop washing procedure to minimise leakage/overfill.

Contact integrator for emergency wastewater removal.

Use Farm equipment for wastewater removal
 to be spread on operator controlled land.

Contact emergency services/ Natural Resources Wales /integrator in event of serious leakage.

Feed

Minor spills can be cleared up with equipment provided (i.e. broom, shovel, bags)

Major containment failure, contact company area manager/feed mill for pneumatic recovery vehicle

Signed

Date
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	Site name
	 Brynrorin Farm

	Grid Reference
	314259,295607 


	
	Telephone Numbers

	Site
	 

	Fire Brigade
	 999

	Police
	 999

	Hospital
	 999

	Area Manager/Integrator
	 

	Electricity.
	 08457331331

	Gas
	 N/A

	Natural Resources Wales             0800807060

	Service Engineer Electricity          

	Service Engineer Plumbing          

	Service Engineer Pest Control     

	Service Engineer Equipment        

	Emergency water supply              01568615942/07831529535

	Key Staff Home & Mobile            

	Key Staff Home & Mobile             

	Veterinary Surgeon
	

	Feed Supplier
	 

	Emergency Litter Disposal
	 Temporary Field Storage

	
	

	
	

	
	

	Directions to the Site:  



�There are references further along in the document to ‘Emergency Action Plan’ – is this the same plan, or a different one?  If they are the same please amend the wording so that it is consistent.


�Is this the same plan as submitted in the permit application?  Please can you clarify.


�Please can you list the sources of water available for fire fighting.


�What happens to the fire water if the manholes are not accessible?


�Will staff receive training on this procedure?  Will a record of the training be made, and if so, where?


�Can you please specify the designated smoking areas that will be available.


�And immediately prior to use?


�What is the procedure for containing wash water if the tanks are full?  Please include details.


�How will chemical spills be dealt with?  Will chemicals be diverted to the dirty water containment system?  Please include details.


�What are the contingency measures for electrical equipment in the event of a power failure to ensure that emissions are controlled?  Please include the details.


�Is there a different procedure for partial failure?  If yes, please include this procedure.  If do, please amend this title to make it clearer.


�Does ‘backups’ mean generator backups?  If yes, please state.


�Will staff be given training on this?


�Please provide details of what this battery is for.


�How will flooding from fire water be dealt with?


�Please include some examples of equipment failure that might be expected.


�Please outline procedures that are in place to prevent this happening.


�Please list which chemicals are likely to be stored on site and could potentially be spilled.


�How will large spills be dealt with?  Please include details.


�Where would it be removed too?





