
Schedule 6 - Notification 

This page outlines the information that the Operator must provide.

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part A 
	Permit Number
	GP3337KD

	Name of Operator
	EnviroWales Ltd.

	Location of Facility
	Unit 5 Tafarnaubach Industrial Estate, Tredegar, NP22 5AA

	Time and date of the detection
	12/03/2015


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant  pollution

	To be notified within 24 hours of detection

	Date and time of the event
	12/3/2015 (date of site visit by D Griffiths)

	Reference or description of the location of the event
	Unit 5, Tafarnaubach Industrial Estate Tredegar.

	Description of where any release in the environment took place
	Potential fugitive release to air from roof vents of Unit 5

	Substance(s) potentially released
	Particulate matter

	Best estimate of the quantity or rate of release of the substances
	Not known

	Measures taken, or intended to be taken to stop the emission
	Cessation of tipping and crushing activities on site with immediate effect pending the following actions.

(1) Roof vents to be repaired – inspection 13/3/2015; schedule of works to be completed by 21/3/2015
(2) Dust suppression technique to be reinstated
(3) Checks on status of environmental protection measures to prevent fugitive release are to be reported daily to management team – as from 13/3/2015.

	Description of the failure or accident
	Wind damage to roof vents not repaired in a timely manner.

	

	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection

	Emission point reference / source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and Time of Monitoring
	

	Measures taken, or intended to be taken to stop the emission
	

	

	Time periods for notification following detection of breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	

	

	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where effect on the environment was detected
	

	Substance(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring / sampling
	


Part B
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment or harm which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	None
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Authorised to sign on behalf of Envirowales.
	Mr. Steven Brian Kelly

	Post
	EHS Director

	Signature
	

	Date
	12/3/2015


