Permit Reference Number: KP3734SH 





Operator: Vopak Terminal Windmill Limited

Installation: Barry Silicon Based Manufacturing Installation

Form Number: R1

Reporting of Waste Disposal and Recovery for the year 2015
	Waste

Description
	Disposal
	Recovery
	
	Trends in Waste Disposal and Recovery

	
	Route
	Tonnes (t)
	Tonnes (t)
	
	Year
	Parameter

	
	
	
	
	
	
	Total Hazardous Wastes (t)
	Total Non-Hazardous Wastes (t)
	Total Materials for Recovery by Dow Corning

	1) Hazardous Waste: (WEEE)
	
	0
	0.050
	
	2006
	185
	15.6
	5

	
	
	
	
	
	2007
	203
	10.3
	6.5

	
	
	
	
	
	2008
	202
	14.4
	9.7

	1) Non-Hazardous Wastes: General
	Landfill
	7.92
	4.72
	
	2009
	167
	15.6
	12.8

	2) Non-Hazardous Waste: Site Cess Pit
	Treatment
	134.92
	
	
	2010
	170
	15.0
	9.6

	
	
	
	
	
	2011
	33.72
	217.25
	43.42

	1) Materials for Recovery by Dow Corning
	
	
	
	
	2012
	0
	219.88
	46.94

	    Tank wash water
	
	---------
	0
	
	2013
	0
	180.76
	28.82

	    Product samples
	
	
	3.899
	
	2014
	0.5
	170.32
	27.76

	   Tank water from base of Linears tanks
	
	
	15.663
	
	2015
	0.05
	142.84
	19.562

	                                     
	
	
	
	
	
	
	
	

	
	
	142.84
	24.332
	
	
	
	
	


	Operator’s comments: 


Signed …D Pratt………………









Date……05/01/16……..




(Authorised to sign as representative of the Operator)
Permit Reference Number: KP3734SH




Operator: Vopak Terminal Windmill Limited

Installation: Barry Silicon Based Manufacturing Installation

Form Number: E1

Reporting of Energy Usage for the year 2015
	Energy Source
	Energy Usage
	CO2 Produced (t)
	
	Trends in Energy Usage

	
	Quantity
	Primary Energy

(MWh)
	
	
	Year
	Parameter

	
	
	
	
	
	
	Primary Energy Usage (MWh)
	CO2  Produced (t)

	Electricity * (MWh)
	1181741
	1182**
	196
	
	2006
	1655
	279.69

	Natural Gas (MWh)
	123.742
	124
	23.56
	
	2007
	1557
	262.232

	Diesel / Distillate Fuel Oil (t)
	0.578
	4
	1.04
	
	2008
	1521
	256

	
	
	
	
	
	2009
	1532
	261

	
	
	
	
	
	2010
	1466
	249

	
	
	
	
	
	2011
	1392
	237

	TOTAL
	
	1310
	220.6
	
	2012
	1476
	249

	
	
	
	
	
	2013
	1389
	234

	
	
	
	
	
	2014
	1280
	216

	
	
	
	
	
	2015
	1310
	220.6

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	


	Operator’s comments :

**Electric  supplied from the adjacent CHP plant,  losses are assumed to be negligible



Signed …D Pratt………………









Date……05/01/16……..




(Authorised to sign as representative of the Operator)
Permit Reference Number: KP3734SH




Operator: Vopak Terminal Windmill Limited

Installation: Barry Silicon Based Manufacturing Installation

Form Number: MR1

Reporting of Mass Release for the year 2015
	Mass Release 
	
	Trends in Mass Release (kg)

	Parameter
	Medium
	kg
	
	Year
	Parameter

	
	
	
	
	
	Methanol
	Octamethylcyclotetrasiloxane
(D4 Cyclics)
	Decamethylcyclotetrasiloxane 
(D5 Cyclics)

	Methanol1

	Fugitive to air
	85
	
	2006
	202
	1491
	9.69

	Octamethylcyclotetrasiloxane
(D4 Cyclics)1
	Fugitive to air
	3298
	
	2007
	153
	1510
	8.69

	Decamethylcyclotetrasiloxane 
(D5 Cyclics)1
	Fugitive to air
	12.96
	
	2008
	43
	1699
	10.76

	

	
	
	
	2009
	100
	1431
	11.4

	
	
	
	
	2010
	55
	1678
	11

	
	
	
	
	2011
	98
	1812
	10

	
	
	
	
	2012
	70
	2170
	10

	
	
	
	
	2013
	125
	2445
	11

	
	
	
	
	2014
	121
	2530
	13.7

	
	
	
	
	2015
	85
	3298
	12.96

	
	
	
	
	2016
	
	
	

	
	
	
	
	2017
	
	
	


	Operator’s comments :

 The data for The Methanol mass (air emission) release was calculated by averaging the results obtained from the fugitive emission surveys carried out by LDAR Envolve Ltd.  
D4 and D5 Cyclic products mass emissions are calculated from ideal gas laws in conjunction with Raoult’s law using the pollutant vapour pressure, the final calculated figure is directly related to the tank throughputs.



Signed …D Pratt    (Authorised to sign as representative of the Operator)                                        Date……05/01/16


KP3734SH
 


